# Static Call Graph for image Thermal_Imaging\Thermal_Imaging.axf

#<CALLGRAPH># ARM Linker, 5050106: Last Updated: Fri May 01 11:17:00 2026

### Maximum Stack Usage = 14568 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ SaveScreenBMP ⇒ f_open ⇒ follow_path ⇒ dir_find ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write

### Mutually Recursive functions

- ADC_IRQHandler ⇒ ADC_IRQHandler

  ### Function Pointers

  - ADC_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - BusFault_Handler from stm32f4xx_it.o(i.BusFault_Handler) referenced from startup_stm32f407xx.o(RESET)
  - CAN1_RX0_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - CAN1_TX_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - CAN2_RX0_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - CAN2_RX1_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - CAN2_SCE_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - CAN2_TX_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - DCMI_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - DMA1_Stream0_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - DMA1_Stream1_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - DMA1_Stream2_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - DMA1_Stream3_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - DMA1_Stream4_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - DMA1_Stream5_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - DMA1_Stream6_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - DMA1_Stream7_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - DMA2_Stream0_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - DMA2_Stream1_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - DMA2_Stream2_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - DMA2_Stream3_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - DMA2_Stream4_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - DMA2_Stream5_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - DMA2_Stream6_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - DMA2_Stream7_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - DebugMon_Handler from stm32f4xx_it.o(i.DebugMon_Handler) referenced from startup_stm32f407xx.o(RESET)
  - ETH_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - ETH_WKUP_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - EXTI2_IRQHandler from stm32f4xx_it.o(i.EXTI2_IRQHandler) referenced from startup_stm32f407xx.o(RESET)
  - EXTI3_IRQHandler from stm32f4xx_it.o(i.EXTI3_IRQHandler) referenced from startup_stm32f407xx.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - FLASH_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - FMC_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - FPU_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - HASH_RNG_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - HardFault_Handler from stm32f4xx_it.o(i.HardFault_Handler) referenced from startup_stm32f407xx.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - I2C3_ER_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - I2C3_EV_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - MemManage_Handler from stm32f4xx_it.o(i.MemManage_Handler) referenced from startup_stm32f407xx.o(RESET)
  - NMI_Handler from stm32f4xx_it.o(i.NMI_Handler) referenced from startup_stm32f407xx.o(RESET)
  - OTG_FS_IRQHandler from stm32f4xx_it.o(i.OTG_FS_IRQHandler) referenced from startup_stm32f407xx.o(RESET)
  - OTG_FS_WKUP_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - OTG_HS_EP1_IN_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - OTG_HS_EP1_OUT_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - OTG_HS_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - OTG_HS_WKUP_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - PVD_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - PendSV_Handler from stm32f4xx_it.o(i.PendSV_Handler) referenced from startup_stm32f407xx.o(RESET)
  - RCC_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - RTC_WKUP_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - Reset_Handler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - SDIO_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - SPI1_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - SPI2_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - SPI3_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - STORAGE_GetCapacity_FS from usbd_storage_if.o(i.STORAGE_GetCapacity_FS) referenced 2 times from usbd_storage_if.o(.data)
  - STORAGE_GetMaxLun_FS from usbd_storage_if.o(i.STORAGE_GetMaxLun_FS) referenced 2 times from usbd_storage_if.o(.data)
  - STORAGE_Init_FS from usbd_storage_if.o(i.STORAGE_Init_FS) referenced 2 times from usbd_storage_if.o(.data)
  - STORAGE_IsReady_FS from usbd_storage_if.o(i.STORAGE_IsReady_FS) referenced 2 times from usbd_storage_if.o(.data)
  - STORAGE_IsWriteProtected_FS from usbd_storage_if.o(i.STORAGE_IsWriteProtected_FS) referenced 2 times from usbd_storage_if.o(.data)
  - STORAGE_Read_FS from usbd_storage_if.o(i.STORAGE_Read_FS) referenced 2 times from usbd_storage_if.o(.data)
  - STORAGE_Write_FS from usbd_storage_if.o(i.STORAGE_Write_FS) referenced 2 times from usbd_storage_if.o(.data)
  - SVC_Handler from stm32f4xx_it.o(i.SVC_Handler) referenced from startup_stm32f407xx.o(RESET)
  - SysTick_Handler from stm32f4xx_it.o(i.SysTick_Handler) referenced from startup_stm32f407xx.o(RESET)
  - SystemInit from system_stm32f4xx.o(i.SystemInit) referenced from startup_stm32f407xx.o(.text)
  - TAMP_STAMP_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - TIM1_BRK_TIM9_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - TIM1_TRG_COM_TIM11_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - TIM1_UP_TIM10_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - TIM2_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - TIM3_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - TIM4_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - TIM5_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - TIM6_DAC_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - TIM7_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - TIM8_BRK_TIM12_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - TIM8_TRG_COM_TIM14_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - TIM8_UP_TIM13_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - UART4_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - UART5_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - USART1_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - USART2_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - USART3_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - USART6_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - USBD_FS_ConfigStrDescriptor from usbd_desc.o(i.USBD_FS_ConfigStrDescriptor) referenced 2 times from usbd_desc.o(.data)
  - USBD_FS_DeviceDescriptor from usbd_desc.o(i.USBD_FS_DeviceDescriptor) referenced 2 times from usbd_desc.o(.data)
  - USBD_FS_InterfaceStrDescriptor from usbd_desc.o(i.USBD_FS_InterfaceStrDescriptor) referenced 2 times from usbd_desc.o(.data)
  - USBD_FS_LangIDStrDescriptor from usbd_desc.o(i.USBD_FS_LangIDStrDescriptor) referenced 2 times from usbd_desc.o(.data)
  - USBD_FS_ManufacturerStrDescriptor from usbd_desc.o(i.USBD_FS_ManufacturerStrDescriptor) referenced 2 times from usbd_desc.o(.data)
  - USBD_FS_ProductStrDescriptor from usbd_desc.o(i.USBD_FS_ProductStrDescriptor) referenced 2 times from usbd_desc.o(.data)
  - USBD_FS_SerialStrDescriptor from usbd_desc.o(i.USBD_FS_SerialStrDescriptor) referenced 2 times from usbd_desc.o(.data)
  - USBD_MSC_DataIn from usbd_msc.o(i.USBD_MSC_DataIn) referenced 2 times from usbd_msc.o(.data)
  - USBD_MSC_DataOut from usbd_msc.o(i.USBD_MSC_DataOut) referenced 2 times from usbd_msc.o(.data)
  - USBD_MSC_DeInit from usbd_msc.o(i.USBD_MSC_DeInit) referenced 2 times from usbd_msc.o(.data)
  - USBD_MSC_GetDeviceQualifierDescriptor from usbd_msc.o(i.USBD_MSC_GetDeviceQualifierDescriptor) referenced 2 times from usbd_msc.o(.data)
  - USBD_MSC_GetFSCfgDesc from usbd_msc.o(i.USBD_MSC_GetFSCfgDesc) referenced 2 times from usbd_msc.o(.data)
  - USBD_MSC_GetHSCfgDesc from usbd_msc.o(i.USBD_MSC_GetHSCfgDesc) referenced 2 times from usbd_msc.o(.data)
  - USBD_MSC_GetOtherSpeedCfgDesc from usbd_msc.o(i.USBD_MSC_GetOtherSpeedCfgDesc) referenced 2 times from usbd_msc.o(.data)
  - USBD_MSC_Init from usbd_msc.o(i.USBD_MSC_Init) referenced 2 times from usbd_msc.o(.data)
  - USBD_MSC_Setup from usbd_msc.o(i.USBD_MSC_Setup) referenced 2 times from usbd_msc.o(.data)
  - USER_initialize from user_diskio_1.o(i.USER_initialize) referenced 2 times from user_diskio_1.o(.data)
  - USER_ioctl from user_diskio_1.o(i.USER_ioctl) referenced 2 times from user_diskio_1.o(.data)
  - USER_read from user_diskio_1.o(i.USER_read) referenced 2 times from user_diskio_1.o(.data)
  - USER_status from user_diskio_1.o(i.USER_status) referenced 2 times from user_diskio_1.o(.data)
  - USER_write from user_diskio_1.o(i.USER_write) referenced 2 times from user_diskio_1.o(.data)
  - UsageFault_Handler from stm32f4xx_it.o(i.UsageFault_Handler) referenced from startup_stm32f407xx.o(RESET)
  - WWDG_IRQHandler from startup_stm32f407xx.o(.text) referenced from startup_stm32f407xx.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f407xx.o(.text)
  - _sputc from printfa.o(i._sputc) referenced from printfa.o(i.__0sprintf)
  - fputc from usart.o(i.fputc) referenced from printfa.o(i.__0printf)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f407xx.o(RESET)

  CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  CAN2_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  CAN2_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  CAN2_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  CAN2_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  DCMI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  DMA1_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  DMA1_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  DMA1_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  DMA1_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  DMA1_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  DMA1_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  DMA1_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  DMA1_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  DMA2_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  DMA2_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  DMA2_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  DMA2_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  DMA2_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  DMA2_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  DMA2_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  DMA2_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  ETH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  ETH_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  FMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  HASH_RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  OTG_FS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  OTG_HS_EP1_IN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  OTG_HS_EP1_OUT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  OTG_HS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  OTG_HS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  TAMP_STAMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  TIM1_BRK_TIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  TIM1_TRG_COM_TIM11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  TIM1_UP_TIM10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  TIM6_DAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  TIM8_BRK_TIM12_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  TIM8_TRG_COM_TIM14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  TIM8_UP_TIM13_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  USART6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = __aeabi_uldivmod
  [Calls]
  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> HAL_RCC_GetSysClockFreq
  - >> UART_SetConfig
  - >> _printf_core
  - >> _fp_digits

  __aeabi_memcpy (Thumb, 36 bytes, Stack size 0 bytes, memcpya.o(.text))
  [Called By]

  - >> SaveScreenBMP

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text))
  [Called By]

  - >> main
  - >> SaveScreenBMP
  - >> HAL_PCD_Init

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> HAL_UART_MspInit
  - >> HAL_SPI_MspInit
  - >> HAL_I2C_MspInit
  - >> HAL_FSMC_MspInit
  - >> HAL_ADC_MspInit
  - >> MX_GPIO_Init
  - >> MX_FSMC_Init
  - >> main
  - >> SystemClock_Config
  - >> HAL_PCD_MspInit

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  strlen (Thumb, 14 bytes, Stack size 0 bytes, strlen.o(.text))
  [Called By]

  - >> main

  __aeabi_fadd (Thumb, 164 bytes, Stack size 16 bytes, fadd.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = __aeabi_fadd ⇒ _float_epilogue
  [Calls]
  - >> _float_round
  - >> _float_epilogue
  [Called By]
  - >> MLX90640_GetVdd
  - >> MLX90640_GetTa
  - >> MLX90640_CalculateTo
  - >> MLX90640_BadPixelsCorrection
  - >> Disp_TempPic
  - >> GetThermalColor
  - >> __aeabi_fsub
  - >> __aeabi_frsub
  - >> GetMedian(float*, int)
  - >> ExtractKtaPixelParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractKvPixelParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractAlphaParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractCPParameters(unsigned short*, paramsMLX90640*)

  __aeabi_fsub (Thumb, 6 bytes, Stack size 0 bytes, fadd.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = __aeabi_fsub ⇒ __aeabi_fadd ⇒ _float_epilogue
  [Calls]
  - >> __aeabi_fadd
  [Called By]
  - >> MLX90640_GetVdd
  - >> MLX90640_GetTa
  - >> MLX90640_CalculateTo
  - >> MLX90640_BadPixelsCorrection
  - >> Disp_TempPic
  - >> GetThermalColor
  - >> ExtractKtaPixelParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractKvPixelParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractAlphaParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractPTATParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractKsToParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractKsTaParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractCILCParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractTgcParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractCPParameters(unsigned short*, paramsMLX90640*)

  __aeabi_frsub (Thumb, 6 bytes, Stack size 0 bytes, fadd.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = __aeabi_frsub ⇒ __aeabi_fadd ⇒ _float_epilogue
  [Calls]
  - >> __aeabi_fadd
  [Called By]
  - >> MLX90640_CalculateTo
  - >> ExtractAlphaParameters(unsigned short*, paramsMLX90640*)

  __aeabi_fmul (Thumb, 100 bytes, Stack size 8 bytes, fmul.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_fmul
  [Called By]
  - >> MLX90640_GetVdd
  - >> MLX90640_GetTa
  - >> MLX90640_CalculateTo
  - >> GetThermalColor
  - >> ExtractKtaPixelParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractKvPixelParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractAlphaParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractCPParameters(unsigned short*, paramsMLX90640*)

  __aeabi_fdiv (Thumb, 124 bytes, Stack size 8 bytes, fdiv.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_fdiv
  [Calls]
  - >> _float_round
  [Called By]
  - >> MLX90640_GetVdd
  - >> MLX90640_GetTa
  - >> MLX90640_CalculateTo
  - >> MLX90640_BadPixelsCorrection
  - >> Disp_TempPic
  - >> GetThermalColor
  - >> GetMedian(float*, int)
  - >> ExtractAlphaParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractPTATParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractKsToParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractKsTaParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractCILCParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractTgcParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractCPParameters(unsigned short*, paramsMLX90640*)

  __aeabi_dadd (Thumb, 322 bytes, Stack size 48 bytes, dadd.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_lasr
  - >> __aeabi_llsl
  - >> _double_round
  - >> _double_epilogue
  [Called By]
  - >> __aeabi_dsub
  - >> ExtractPTATParameters(unsigned short*, paramsMLX90640*)
  - >> __aeabi_drsub
  - >> pow
  - >> __kernel_poly
  - >> __mathlib_dbl_infnan2
  - >> _fp_digits

  __aeabi_dsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = __aeabi_dsub ⇒ __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_dadd
  [Called By]
  - >> main
  - >> pow

  __aeabi_drsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = __aeabi_drsub ⇒ __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_dadd
  [Called By]
  - >> pow

  __aeabi_dmul (Thumb, 228 bytes, Stack size 48 bytes, dmul.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> MLX90640_GetTa
  - >> lcd_ssd_backlight_set
  - >> ExtractKtaPixelParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractKvPixelParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractAlphaParameters(unsigned short*, paramsMLX90640*)
  - >> pow
  - >> __kernel_poly
  - >> _fp_digits

  __aeabi_ddiv (Thumb, 222 bytes, Stack size 32 bytes, ddiv.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = __aeabi_ddiv ⇒ _double_round
  [Calls]
  - >> _double_round
  [Called By]
  - >> MLX90640_GetVdd
  - >> ExtractKtaPixelParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractKvPixelParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractAlphaParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractPTATParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractCPParameters(unsigned short*, paramsMLX90640*)
  - >> pow
  - >> __mathlib_dbl_invalid
  - >> __mathlib_dbl_divzero
  - >> _fp_digits

  __aeabi_i2f (Thumb, 18 bytes, Stack size 0 bytes, fflti.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = __aeabi_i2f ⇒ _float_epilogue
  [Calls]
  - >> _float_epilogue
  [Called By]
  - >> MLX90640_GetVdd
  - >> MLX90640_CalculateTo
  - >> ExtractKtaPixelParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractKvPixelParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractAlphaParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractPTATParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractKsToParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractKsTaParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractCILCParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractTgcParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractCPParameters(unsigned short*, paramsMLX90640*)

  __aeabi_ui2f (Thumb, 10 bytes, Stack size 0 bytes, ffltui.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = __aeabi_ui2f ⇒ _float_epilogue
  [Calls]
  - >> _float_epilogue
  [Called By]
  - >> MLX90640_GetVdd
  - >> MLX90640_GetTa
  - >> MLX90640_CalculateTo
  - >> GetThermalColor

  __aeabi_i2d (Thumb, 34 bytes, Stack size 16 bytes, dflti.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = __aeabi_i2d ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> MLX90640_GetVdd
  - >> ExtractPTATParameters(unsigned short*, paramsMLX90640*)
  - >> pow

  __aeabi_ui2d (Thumb, 26 bytes, Stack size 16 bytes, dfltui.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = __aeabi_ui2d ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> MLX90640_GetVdd
  - >> MLX90640_CalculateTo
  - >> lcd_ssd_backlight_set
  - >> ExtractKtaPixelParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractKvPixelParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractAlphaParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractCPParameters(unsigned short*, paramsMLX90640*)

  __aeabi_f2iz (Thumb, 50 bytes, Stack size 0 bytes, ffixi.o(.text))
  [Called By]

  - >> GetThermalColor
  - >> ExtractKtaPixelParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractKvPixelParameters(unsigned short*, paramsMLX90640*)

  __aeabi_f2uiz (Thumb, 40 bytes, Stack size 0 bytes, ffixui.o(.text))
  [Called By]

  - >> Disp_TempPic
  - >> ExtractAlphaParameters(unsigned short*, paramsMLX90640*)

  __aeabi_d2uiz (Thumb, 50 bytes, Stack size 8 bytes, dfixui.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_d2uiz
  [Calls]
  - >> __aeabi_llsr
  [Called By]
  - >> lcd_ssd_backlight_set

  __aeabi_f2d (Thumb, 38 bytes, Stack size 0 bytes, f2d.o(.text))
  [Called By]

  - >> MLX90640_GetTa
  - >> Disp_TempPic
  - >> main
  - >> ExtractKtaPixelParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractKvPixelParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractAlphaParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractCPParameters(unsigned short*, paramsMLX90640*)

  __aeabi_d2f (Thumb, 56 bytes, Stack size 8 bytes, d2f.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_d2f
  [Calls]
  - >> _float_round
  [Called By]
  - >> MLX90640_GetVdd
  - >> MLX90640_GetTa
  - >> MLX90640_CalculateTo
  - >> main
  - >> ExtractKtaPixelParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractKvPixelParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractAlphaParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractPTATParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractCPParameters(unsigned short*, paramsMLX90640*)

  __aeabi_cfcmpeq (Thumb, 0 bytes, Stack size 0 bytes, cfcmple.o(.text))
  [Called By]

  - >> Disp_TempPic

  __aeabi_cfcmple (Thumb, 20 bytes, Stack size 0 bytes, cfcmple.o(.text))
  [Called By]

  - >> Disp_TempPic
  - >> GetMedian(float*, int)
  - >> ExtractKtaPixelParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractKvPixelParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractAlphaParameters(unsigned short*, paramsMLX90640*)

  __aeabi_cfrcmple (Thumb, 20 bytes, Stack size 0 bytes, cfrcmple.o(.text))
  [Called By]

  - >> MLX90640_GetVdd
  - >> MLX90640_GetTa
  - >> MLX90640_CalculateTo
  - >> MLX90640_BadPixelsCorrection
  - >> Disp_TempPic
  - >> ExtractKtaPixelParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractKvPixelParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractAlphaParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractPTATParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractKsToParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractKsTaParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractCILCParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractTgcParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractCPParameters(unsigned short*, paramsMLX90640*)

  __aeabi_uidiv (Thumb, 0 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)

  __aeabi_uidivmod (Thumb, 44 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)
  [Called By]

  - >> _printf_core

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text))
  [Called By]

  - >> __aeabi_dadd
  - >> __aeabi_uldivmod
  - >> _double_epilogue
  - >> __aeabi_d2ulz

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text))
  [Called By]

  - >> __aeabi_d2uiz
  - >> __aeabi_uldivmod
  - >> _dsqrt
  - >> _double_epilogue
  - >> __aeabi_d2ulz

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  __aeabi_lasr (Thumb, 36 bytes, Stack size 0 bytes, llsshr.o(.text))
  [Called By]

  - >> __aeabi_dadd

  _ll_sshift_r (Thumb, 0 bytes, Stack size 0 bytes, llsshr.o(.text), UNUSED)

  __I$use$fp (Thumb, 0 bytes, Stack size 0 bytes, iusefp.o(.text), UNUSED)

  _float_round (Thumb, 18 bytes, Stack size 0 bytes, fepilogue.o(.text))
  [Called By]

  - >> __aeabi_d2f
  - >> __aeabi_fdiv
  - >> __aeabi_fadd
  - >> _fsqrt

  _float_epilogue (Thumb, 92 bytes, Stack size 4 bytes, fepilogue.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = _float_epilogue
  [Called By]
  - >> __aeabi_ui2f
  - >> __aeabi_i2f
  - >> __aeabi_fadd

  _fsqrt (Thumb, 94 bytes, Stack size 16 bytes, fsqrt.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = _fsqrt
  [Calls]
  - >> _float_round
  [Called By]
  - >> sqrtf

  _double_round (Thumb, 30 bytes, Stack size 8 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = _double_round
  [Called By]
  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> _dsqrt
  - >> _double_epilogue

  _double_epilogue (Thumb, 156 bytes, Stack size 32 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_llsr
  - >> __aeabi_llsl
  - >> _double_round
  [Called By]
  - >> __aeabi_ui2d
  - >> __aeabi_dmul
  - >> __aeabi_i2d
  - >> __aeabi_dadd

  __ARM_scalbn (Thumb, 46 bytes, Stack size 16 bytes, dscalb.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = __ARM_scalbn
  [Called By]
  - >> pow
  - >> __mathlib_dbl_underflow
  - >> __mathlib_dbl_overflow

  scalbn (Thumb, 0 bytes, Stack size 16 bytes, dscalb.o(.text), UNUSED)

  __aeabi_d2ulz (Thumb, 48 bytes, Stack size 0 bytes, dfixul.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _fp_digits

  __aeabi_cdrcmple (Thumb, 48 bytes, Stack size 0 bytes, cdrcmple.o(.text))
  [Called By]

  - >> pow
  - >> _fp_digits

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  _dsqrt (Thumb, 162 bytes, Stack size 32 bytes, dsqrt.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _dsqrt ⇒ _double_round
  [Calls]
  - >> __aeabi_llsr
  - >> _double_round
  [Called By]
  - >> sqrt

  __decompress (Thumb, 0 bytes, Stack size unknown bytes, __dczerorl2.o(.text), UNUSED)

  __decompress1 (Thumb, 86 bytes, Stack size unknown bytes, __dczerorl2.o(.text), UNUSED)

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.BusFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  Disp_TempPic (Thumb, 512 bytes, Stack size 88 bytes, mlx90640.o(i.Disp_TempPic))
  [Stack]

  - Max Depth = 276
  - Call Chain = Disp_TempPic ⇒ DrawTopRows ⇒ GetThermalColor ⇒ __aeabi_fsub ⇒ __aeabi_fadd ⇒ _float_epilogue
  [Calls]
  - >> lcd_set_window
  - >> __aeabi_f2d
  - >> __aeabi_cfcmpeq
  - >> lcd_show_string_transparent
  - >> DrawValueMarker
  - >> DrawTopRows
  - >> DrawFullThermalRegion
  - >> DrawCrosshair
  - >> __aeabi_fsub
  - >> __aeabi_fdiv
  - >> __aeabi_fadd
  - >> __aeabi_f2uiz
  - >> __aeabi_cfrcmple
  - >> __aeabi_cfcmple
  - >> __2sprintf
  [Called By]
  - >> main

  EXTI2_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, stm32f4xx_it.o(i.EXTI2_IRQHandler))
  [Stack]

  - Max Depth = 48
  - Call Chain = EXTI2_IRQHandler ⇒ HAL_GPIO_EXTI_IRQHandler ⇒ HAL_GPIO_EXTI_Callback ⇒ __2printf
  [Calls]
  - >> HAL_GPIO_EXTI_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f407xx.o(RESET)

  EXTI3_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, stm32f4xx_it.o(i.EXTI3_IRQHandler))
  [Stack]

  - Max Depth = 48
  - Call Chain = EXTI3_IRQHandler ⇒ HAL_GPIO_EXTI_IRQHandler ⇒ HAL_GPIO_EXTI_Callback ⇒ __2printf
  [Calls]
  - >> HAL_GPIO_EXTI_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f407xx.o(RESET)

  Error_Handler (Thumb, 6 bytes, Stack size 0 bytes, main.o(i.Error_Handler))
  [Called By]

  - >> MX_USB_DEVICE_Init
  - >> MX_USART6_UART_Init
  - >> MX_SPI3_Init
  - >> MX_I2C2_Init
  - >> MX_FSMC_Init
  - >> MX_ADC1_Init
  - >> SystemClock_Config
  - >> USBD_LL_Init
  - >> HAL_PCD_ResetCallback

  FATFS_LinkDriver (Thumb, 18 bytes, Stack size 12 bytes, ff_gen_drv.o(i.FATFS_LinkDriver))
  [Stack]

  - Max Depth = 32
  - Call Chain = FATFS_LinkDriver ⇒ FATFS_LinkDriverEx
  [Calls]
  - >> FATFS_LinkDriverEx
  [Called By]
  - >> MX_FATFS_Init

  FATFS_LinkDriverEx (Thumb, 78 bytes, Stack size 20 bytes, ff_gen_drv.o(i.FATFS_LinkDriverEx))
  [Stack]

  - Max Depth = 20
  - Call Chain = FATFS_LinkDriverEx
  [Called By]
  - >> FATFS_LinkDriver

  FSMC_NORSRAM_Extended_Timing_Init (Thumb, 66 bytes, Stack size 16 bytes, stm32f4xx_ll_fsmc.o(i.FSMC_NORSRAM_Extended_Timing_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = FSMC_NORSRAM_Extended_Timing_Init
  [Called By]
  - >> HAL_SRAM_Init
  - >> lcd_init

  FSMC_NORSRAM_Init (Thumb, 88 bytes, Stack size 8 bytes, stm32f4xx_ll_fsmc.o(i.FSMC_NORSRAM_Init))
  [Stack]

  - Max Depth = 8
  - Call Chain = FSMC_NORSRAM_Init
  [Called By]
  - >> HAL_SRAM_Init

  FSMC_NORSRAM_Timing_Init (Thumb, 68 bytes, Stack size 12 bytes, stm32f4xx_ll_fsmc.o(i.FSMC_NORSRAM_Timing_Init))
  [Stack]

  - Max Depth = 12
  - Call Chain = FSMC_NORSRAM_Timing_Init
  [Called By]
  - >> HAL_SRAM_Init

  HAL_ADC_ConfigChannel (Thumb, 380 bytes, Stack size 16 bytes, stm32f4xx_hal_adc.o(i.HAL_ADC_ConfigChannel))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_ADC_ConfigChannel
  [Called By]
  - >> MX_ADC1_Init

  HAL_ADC_Init (Thumb, 100 bytes, Stack size 16 bytes, stm32f4xx_hal_adc.o(i.HAL_ADC_Init))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_ADC_Init ⇒ HAL_ADC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_ADC_MspInit
  - >> ADC_Init
  [Called By]
  - >> MX_ADC1_Init

  HAL_ADC_MspInit (Thumb, 114 bytes, Stack size 32 bytes, adc.o(i.HAL_ADC_MspInit))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_ADC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  - >> __aeabi_memclr4
  [Called By]
  - >> HAL_ADC_Init

  HAL_Delay (Thumb, 36 bytes, Stack size 16 bytes, stm32f4xx_hal.o(i.HAL_Delay))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_Delay
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> lcd_init
  - >> main
  - >> lcd_ex_st7796_reginit
  - >> lcd_ex_st7789_reginit
  - >> lcd_ex_ssd1963_reginit
  - >> lcd_ex_nt35510_reginit
  - >> lcd_ex_nt35310_reginit
  - >> lcd_ex_ili9806_reginit
  - >> lcd_ex_ili9341_reginit
  - >> USB_SetCurrentMode

  HAL_GPIO_EXTI_Callback (Thumb, 22 bytes, Stack size 8 bytes, main.o(i.HAL_GPIO_EXTI_Callback))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_GPIO_EXTI_Callback ⇒ __2printf
  [Calls]
  - >> __2printf
  [Called By]
  - >> HAL_GPIO_EXTI_IRQHandler

  HAL_GPIO_EXTI_IRQHandler (Thumb, 24 bytes, Stack size 8 bytes, stm32f4xx_hal_gpio.o(i.HAL_GPIO_EXTI_IRQHandler))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_GPIO_EXTI_IRQHandler ⇒ HAL_GPIO_EXTI_Callback ⇒ __2printf
  [Calls]
  - >> HAL_GPIO_EXTI_Callback
  [Called By]
  - >> EXTI3_IRQHandler
  - >> EXTI2_IRQHandler

  HAL_GPIO_Init (Thumb, 452 bytes, Stack size 24 bytes, stm32f4xx_hal_gpio.o(i.HAL_GPIO_Init))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_GPIO_Init
  [Called By]
  - >> HAL_UART_MspInit
  - >> HAL_SPI_MspInit
  - >> HAL_I2C_MspInit
  - >> HAL_FSMC_MspInit
  - >> HAL_ADC_MspInit
  - >> led_init
  - >> lcd_init
  - >> MX_GPIO_Init
  - >> HAL_PCD_MspInit

  HAL_GPIO_TogglePin (Thumb, 20 bytes, Stack size 8 bytes, stm32f4xx_hal_gpio.o(i.HAL_GPIO_TogglePin))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_GPIO_TogglePin
  [Called By]
  - >> main

  HAL_GPIO_WritePin (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_hal_gpio.o(i.HAL_GPIO_WritePin))
  [Called By]

  - >> led_init
  - >> lcd_init
  - >> MX_GPIO_Init
  - >> MySPI_Stop
  - >> MySPI_Start
  - >> MySPI_Init

  HAL_GetTick (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_hal.o(i.HAL_GetTick))
  [Called By]

  - >> HAL_UART_Transmit
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  - >> HAL_Delay
  - >> SPI_WaitFlagStateUntilTimeout
  - >> HAL_I2C_Mem_Write
  - >> HAL_I2C_Mem_Read
  - >> I2C_WaitOnTXEFlagUntilTimeout
  - >> I2C_WaitOnRXNEFlagUntilTimeout
  - >> I2C_WaitOnMasterAddressFlagUntilTimeout
  - >> I2C_WaitOnFlagUntilTimeout
  - >> I2C_WaitOnBTFFlagUntilTimeout
  - >> UART_WaitOnFlagUntilTimeout
  - >> HAL_SPI_TransmitReceive

  HAL_I2C_Init (Thumb, 446 bytes, Stack size 16 bytes, stm32f4xx_hal_i2c.o(i.HAL_I2C_Init))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_I2C_Init ⇒ HAL_I2C_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_I2C_MspInit
  - >> HAL_RCC_GetPCLK1Freq
  [Called By]
  - >> MX_I2C2_Init

  HAL_I2C_Mem_Read (Thumb, 744 bytes, Stack size 48 bytes, stm32f4xx_hal_i2c.o(i.HAL_I2C_Mem_Read))
  [Stack]

  - Max Depth = 104
  - Call Chain = HAL_I2C_Mem_Read ⇒ I2C_RequestMemoryRead ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  - >> I2C_WaitOnRXNEFlagUntilTimeout
  - >> I2C_WaitOnFlagUntilTimeout
  - >> I2C_RequestMemoryRead
  [Called By]
  - >> MLX90640_I2CRead

  HAL_I2C_Mem_Write (Thumb, 348 bytes, Stack size 48 bytes, stm32f4xx_hal_i2c.o(i.HAL_I2C_Mem_Write))
  [Stack]

  - Max Depth = 104
  - Call Chain = HAL_I2C_Mem_Write ⇒ I2C_RequestMemoryWrite ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  - >> I2C_WaitOnTXEFlagUntilTimeout
  - >> I2C_WaitOnFlagUntilTimeout
  - >> I2C_WaitOnBTFFlagUntilTimeout
  - >> I2C_RequestMemoryWrite
  [Called By]
  - >> MLX90640_I2CWrite

  HAL_I2C_MspInit (Thumb, 124 bytes, Stack size 32 bytes, i2c.o(i.HAL_I2C_MspInit))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_I2C_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  - >> __aeabi_memclr4
  [Called By]
  - >> HAL_I2C_Init

  HAL_IncTick (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_hal.o(i.HAL_IncTick))
  [Called By]

  - >> SysTick_Handler

  HAL_Init (Thumb, 54 bytes, Stack size 8 bytes, stm32f4xx_hal.o(i.HAL_Init))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_Init ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_MspInit
  - >> HAL_InitTick
  - >> HAL_NVIC_SetPriorityGrouping
  [Called By]
  - >> main

  HAL_InitTick (Thumb, 64 bytes, Stack size 16 bytes, stm32f4xx_hal.o(i.HAL_InitTick))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_InitTick ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_SYSTICK_Config
  [Called By]
  - >> HAL_RCC_ClockConfig
  - >> HAL_Init

  HAL_MspInit (Thumb, 68 bytes, Stack size 8 bytes, stm32f4xx_hal_msp.o(i.HAL_MspInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_MspInit
  [Called By]
  - >> HAL_Init

  HAL_NVIC_EnableIRQ (Thumb, 32 bytes, Stack size 0 bytes, stm32f4xx_hal_cortex.o(i.HAL_NVIC_EnableIRQ))
  [Called By]

  - >> MX_GPIO_Init
  - >> HAL_PCD_MspInit

  HAL_NVIC_SetPriority (Thumb, 124 bytes, Stack size 40 bytes, stm32f4xx_hal_cortex.o(i.HAL_NVIC_SetPriority))
  [Stack]

  - Max Depth = 48
  - Call Chain = HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> __NVIC_SetPriority
  - >> __NVIC_GetPriorityGrouping
  [Called By]
  - >> MX_GPIO_Init
  - >> HAL_PCD_MspInit
  - >> HAL_InitTick

  HAL_NVIC_SetPriorityGrouping (Thumb, 32 bytes, Stack size 0 bytes, stm32f4xx_hal_cortex.o(i.HAL_NVIC_SetPriorityGrouping))
  [Called By]

  - >> HAL_Init

  HAL_PCDEx_LPM_Callback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_pcd_ex.o(i.HAL_PCDEx_LPM_Callback))
  [Called By]

  - >> HAL_PCD_IRQHandler

  HAL_PCDEx_SetRxFiFo (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_hal_pcd_ex.o(i.HAL_PCDEx_SetRxFiFo))
  [Called By]

  - >> USBD_LL_Init

  HAL_PCDEx_SetTxFiFo (Thumb, 78 bytes, Stack size 20 bytes, stm32f4xx_hal_pcd_ex.o(i.HAL_PCDEx_SetTxFiFo))
  [Stack]

  - Max Depth = 20
  - Call Chain = HAL_PCDEx_SetTxFiFo
  [Called By]
  - >> USBD_LL_Init

  HAL_PCD_ConnectCallback (Thumb, 14 bytes, Stack size 8 bytes, usbd_conf.o(i.HAL_PCD_ConnectCallback))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_PCD_ConnectCallback
  [Calls]
  - >> USBD_LL_DevConnected
  [Called By]
  - >> HAL_PCD_IRQHandler

  HAL_PCD_DataInStageCallback (Thumb, 32 bytes, Stack size 16 bytes, usbd_conf.o(i.HAL_PCD_DataInStageCallback))
  [Stack]

  - Max Depth = 172
  - Call Chain = HAL_PCD_DataInStageCallback ⇒ USBD_LL_DataInStage ⇒ USBD_CtlContinueSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_DataInStage
  [Called By]
  - >> HAL_PCD_IRQHandler

  HAL_PCD_DataOutStageCallback (Thumb, 32 bytes, Stack size 16 bytes, usbd_conf.o(i.HAL_PCD_DataOutStageCallback))
  [Stack]

  - Max Depth = 172
  - Call Chain = HAL_PCD_DataOutStageCallback ⇒ USBD_LL_DataOutStage ⇒ USBD_CtlContinueRx ⇒ USBD_LL_PrepareReceive ⇒ HAL_PCD_EP_Receive ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_DataOutStage
  [Called By]
  - >> PCD_EP_OutXfrComplete_int

  HAL_PCD_DisconnectCallback (Thumb, 14 bytes, Stack size 8 bytes, usbd_conf.o(i.HAL_PCD_DisconnectCallback))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_PCD_DisconnectCallback ⇒ USBD_LL_DevDisconnected
  [Calls]
  - >> USBD_LL_DevDisconnected
  [Called By]
  - >> HAL_PCD_IRQHandler

  HAL_PCD_EP_Close (Thumb, 106 bytes, Stack size 16 bytes, stm32f4xx_hal_pcd.o(i.HAL_PCD_EP_Close))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_PCD_EP_Close ⇒ USB_DeactivateEndpoint
  [Calls]
  - >> USB_DeactivateEndpoint
  [Called By]
  - >> USBD_LL_CloseEP

  HAL_PCD_EP_ClrStall (Thumb, 124 bytes, Stack size 16 bytes, stm32f4xx_hal_pcd.o(i.HAL_PCD_EP_ClrStall))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_PCD_EP_ClrStall ⇒ USB_EPClearStall
  [Calls]
  - >> USB_EPClearStall
  [Called By]
  - >> USBD_LL_ClearStallEP

  HAL_PCD_EP_Flush (Thumb, 68 bytes, Stack size 16 bytes, stm32f4xx_hal_pcd.o(i.HAL_PCD_EP_Flush))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_PCD_EP_Flush ⇒ USB_FlushTxFifo
  [Calls]
  - >> USB_FlushTxFifo
  - >> USB_FlushRxFifo
  [Called By]
  - >> USBD_LL_FlushEP

  HAL_PCD_EP_GetRxCount (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_hal_pcd.o(i.HAL_PCD_EP_GetRxCount))
  [Called By]

  - >> USBD_LL_GetRxDataSize

  HAL_PCD_EP_Open (Thumb, 140 bytes, Stack size 32 bytes, stm32f4xx_hal_pcd.o(i.HAL_PCD_EP_Open))
  [Stack]

  - Max Depth = 48
  - Call Chain = HAL_PCD_EP_Open ⇒ USB_ActivateEndpoint
  [Calls]
  - >> USB_ActivateEndpoint
  [Called By]
  - >> USBD_LL_OpenEP

  HAL_PCD_EP_Receive (Thumb, 88 bytes, Stack size 24 bytes, stm32f4xx_hal_pcd.o(i.HAL_PCD_EP_Receive))
  [Stack]

  - Max Depth = 84
  - Call Chain = HAL_PCD_EP_Receive ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USB_EPStartXfer
  - >> USB_EP0StartXfer
  [Called By]
  - >> USBD_LL_PrepareReceive

  HAL_PCD_EP_SetStall (Thumb, 138 bytes, Stack size 16 bytes, stm32f4xx_hal_pcd.o(i.HAL_PCD_EP_SetStall))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_PCD_EP_SetStall ⇒ USB_EP0_OutStart
  [Calls]
  - >> USB_EPSetStall
  - >> USB_EP0_OutStart
  [Called By]
  - >> USBD_LL_StallEP

  HAL_PCD_EP_Transmit (Thumb, 90 bytes, Stack size 24 bytes, stm32f4xx_hal_pcd.o(i.HAL_PCD_EP_Transmit))
  [Stack]

  - Max Depth = 84
  - Call Chain = HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USB_EPStartXfer
  - >> USB_EP0StartXfer
  [Called By]
  - >> USBD_LL_Transmit

  HAL_PCD_IRQHandler (Thumb, 1372 bytes, Stack size 48 bytes, stm32f4xx_hal_pcd.o(i.HAL_PCD_IRQHandler))
  [Stack]

  - Max Depth = 276
  - Call Chain = HAL_PCD_IRQHandler ⇒ PCD_EP_OutSetupPacket_int ⇒ HAL_PCD_SetupStageCallback ⇒ USBD_LL_SetupStage ⇒ USBD_StdDevReq ⇒ USBD_GetDescriptor ⇒ USBD_CtlSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USB_SetTurnaroundTime
  - >> USB_ReadPacket
  - >> USB_ReadInterrupts
  - >> USB_ReadDevOutEPInterrupt
  - >> USB_ReadDevInEPInterrupt
  - >> USB_ReadDevAllOutEpInterrupt
  - >> USB_ReadDevAllInEpInterrupt
  - >> USB_GetMode
  - >> USB_GetDevSpeed
  - >> USB_FlushTxFifo
  - >> USB_EP0_OutStart
  - >> USB_ActivateSetup
  - >> HAL_RCC_GetHCLKFreq
  - >> HAL_PCDEx_LPM_Callback
  - >> PCD_WriteEmptyTxFifo
  - >> PCD_EP_OutXfrComplete_int
  - >> PCD_EP_OutSetupPacket_int
  - >> HAL_PCD_SuspendCallback
  - >> HAL_PCD_SOFCallback
  - >> HAL_PCD_ResumeCallback
  - >> HAL_PCD_ResetCallback
  - >> HAL_PCD_ISOOUTIncompleteCallback
  - >> HAL_PCD_ISOINIncompleteCallback
  - >> HAL_PCD_DisconnectCallback
  - >> HAL_PCD_DataInStageCallback
  - >> HAL_PCD_ConnectCallback
  [Called By]
  - >> OTG_FS_IRQHandler

  HAL_PCD_ISOINIncompleteCallback (Thumb, 18 bytes, Stack size 16 bytes, usbd_conf.o(i.HAL_PCD_ISOINIncompleteCallback))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_PCD_ISOINIncompleteCallback ⇒ USBD_LL_IsoINIncomplete
  [Calls]
  - >> USBD_LL_IsoINIncomplete
  [Called By]
  - >> HAL_PCD_IRQHandler

  HAL_PCD_ISOOUTIncompleteCallback (Thumb, 18 bytes, Stack size 16 bytes, usbd_conf.o(i.HAL_PCD_ISOOUTIncompleteCallback))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_PCD_ISOOUTIncompleteCallback ⇒ USBD_LL_IsoOUTIncomplete
  [Calls]
  - >> USBD_LL_IsoOUTIncomplete
  [Called By]
  - >> HAL_PCD_IRQHandler

  HAL_PCD_Init (Thumb, 358 bytes, Stack size 56 bytes, stm32f4xx_hal_pcd.o(i.HAL_PCD_Init))
  [Stack]

  - Max Depth = 136
  - Call Chain = HAL_PCD_Init ⇒ HAL_PCD_MspInit ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> USB_SetCurrentMode
  - >> USB_DisableGlobalInt
  - >> USB_DevInit
  - >> USB_DevDisconnect
  - >> USB_CoreInit
  - >> HAL_PCD_MspInit
  - >> __aeabi_memcpy4
  [Called By]
  - >> USBD_LL_Init

  HAL_PCD_MspInit (Thumb, 160 bytes, Stack size 32 bytes, usbd_conf.o(i.HAL_PCD_MspInit))
  [Stack]

  - Max Depth = 80
  - Call Chain = HAL_PCD_MspInit ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  - >> HAL_GPIO_Init
  - >> __aeabi_memclr4
  [Called By]
  - >> HAL_PCD_Init

  HAL_PCD_ResetCallback (Thumb, 48 bytes, Stack size 16 bytes, usbd_conf.o(i.HAL_PCD_ResetCallback))
  [Stack]

  - Max Depth = 104
  - Call Chain = HAL_PCD_ResetCallback ⇒ USBD_LL_Reset ⇒ USBD_LL_OpenEP ⇒ HAL_PCD_EP_Open ⇒ USB_ActivateEndpoint
  [Calls]
  - >> Error_Handler
  - >> USBD_LL_SetSpeed
  - >> USBD_LL_Reset
  [Called By]
  - >> HAL_PCD_IRQHandler

  HAL_PCD_ResumeCallback (Thumb, 14 bytes, Stack size 8 bytes, usbd_conf.o(i.HAL_PCD_ResumeCallback))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_PCD_ResumeCallback
  [Calls]
  - >> USBD_LL_Resume
  [Called By]
  - >> HAL_PCD_IRQHandler

  HAL_PCD_SOFCallback (Thumb, 14 bytes, Stack size 8 bytes, usbd_conf.o(i.HAL_PCD_SOFCallback))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_PCD_SOFCallback ⇒ USBD_LL_SOF
  [Calls]
  - >> USBD_LL_SOF
  [Called By]
  - >> HAL_PCD_IRQHandler

  HAL_PCD_SetAddress (Thumb, 54 bytes, Stack size 16 bytes, stm32f4xx_hal_pcd.o(i.HAL_PCD_SetAddress))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_PCD_SetAddress ⇒ USB_SetDevAddress
  [Calls]
  - >> USB_SetDevAddress
  [Called By]
  - >> USBD_LL_SetUSBAddress

  HAL_PCD_SetupStageCallback (Thumb, 18 bytes, Stack size 8 bytes, usbd_conf.o(i.HAL_PCD_SetupStageCallback))
  [Stack]

  - Max Depth = 196
  - Call Chain = HAL_PCD_SetupStageCallback ⇒ USBD_LL_SetupStage ⇒ USBD_StdDevReq ⇒ USBD_GetDescriptor ⇒ USBD_CtlSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_SetupStage
  [Called By]
  - >> PCD_EP_OutSetupPacket_int

  HAL_PCD_Start (Thumb, 74 bytes, Stack size 16 bytes, stm32f4xx_hal_pcd.o(i.HAL_PCD_Start))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_PCD_Start
  [Calls]
  - >> USB_EnableGlobalInt
  - >> USB_DevConnect
  [Called By]
  - >> USBD_LL_Start

  HAL_PCD_SuspendCallback (Thumb, 46 bytes, Stack size 8 bytes, usbd_conf.o(i.HAL_PCD_SuspendCallback))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_PCD_SuspendCallback
  [Calls]
  - >> USBD_LL_Suspend
  [Called By]
  - >> HAL_PCD_IRQHandler

  HAL_RCC_ClockConfig (Thumb, 368 bytes, Stack size 16 bytes, stm32f4xx_hal_rcc.o(i.HAL_RCC_ClockConfig))
  [Stack]

  - Max Depth = 88
  - Call Chain = HAL_RCC_ClockConfig ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uldivmod
  [Calls]
  - >> HAL_RCC_GetSysClockFreq
  - >> HAL_InitTick
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_RCC_GetHCLKFreq (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq))
  [Called By]

  - >> HAL_PCD_IRQHandler
  - >> HAL_RCC_GetPCLK2Freq
  - >> HAL_RCC_GetPCLK1Freq

  HAL_RCC_GetPCLK1Freq (Thumb, 22 bytes, Stack size 4 bytes, stm32f4xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq))
  [Stack]

  - Max Depth = 4
  - Call Chain = HAL_RCC_GetPCLK1Freq
  [Calls]
  - >> HAL_RCC_GetHCLKFreq
  [Called By]
  - >> HAL_I2C_Init
  - >> UART_SetConfig

  HAL_RCC_GetPCLK2Freq (Thumb, 22 bytes, Stack size 4 bytes, stm32f4xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq))
  [Stack]

  - Max Depth = 4
  - Call Chain = HAL_RCC_GetPCLK2Freq
  [Calls]
  - >> HAL_RCC_GetHCLKFreq
  [Called By]
  - >> UART_SetConfig

  HAL_RCC_GetSysClockFreq (Thumb, 162 bytes, Stack size 32 bytes, stm32f4xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_RCC_GetSysClockFreq ⇒ __aeabi_uldivmod
  [Calls]
  - >> __aeabi_uldivmod
  [Called By]
  - >> HAL_RCC_ClockConfig

  HAL_RCC_OscConfig (Thumb, 1172 bytes, Stack size 24 bytes, stm32f4xx_hal_rcc.o(i.HAL_RCC_OscConfig))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_RCC_OscConfig
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_SPI_Init (Thumb, 200 bytes, Stack size 8 bytes, stm32f4xx_hal_spi.o(i.HAL_SPI_Init))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_SPI_Init ⇒ HAL_SPI_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_SPI_MspInit
  [Called By]
  - >> MX_SPI3_Init

  HAL_SPI_MspInit (Thumb, 124 bytes, Stack size 32 bytes, spi.o(i.HAL_SPI_MspInit))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_SPI_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  - >> __aeabi_memclr4
  [Called By]
  - >> HAL_SPI_Init

  HAL_SPI_TransmitReceive (Thumb, 554 bytes, Stack size 56 bytes, stm32f4xx_hal_spi.o(i.HAL_SPI_TransmitReceive))
  [Stack]

  - Max Depth = 120
  - Call Chain = HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_GetTick
  - >> SPI_EndRxTxTransaction
  [Called By]
  - >> MySPI_SwapByte

  HAL_SRAM_Init (Thumb, 88 bytes, Stack size 16 bytes, stm32f4xx_hal_sram.o(i.HAL_SRAM_Init))
  [Stack]

  - Max Depth = 80
  - Call Chain = HAL_SRAM_Init ⇒ HAL_SRAM_MspInit ⇒ HAL_FSMC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_SRAM_MspInit
  - >> FSMC_NORSRAM_Timing_Init
  - >> FSMC_NORSRAM_Init
  - >> FSMC_NORSRAM_Extended_Timing_Init
  [Called By]
  - >> lcd_init
  - >> MX_FSMC_Init

  HAL_SRAM_MspInit (Thumb, 10 bytes, Stack size 8 bytes, fsmc.o(i.HAL_SRAM_MspInit))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_SRAM_MspInit ⇒ HAL_FSMC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_FSMC_MspInit
  [Called By]
  - >> HAL_SRAM_Init

  HAL_SYSTICK_Config (Thumb, 52 bytes, Stack size 16 bytes, stm32f4xx_hal_cortex.o(i.HAL_SYSTICK_Config))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_SYSTICK_Config ⇒ __NVIC_SetPriority
  [Calls]
  - >> __NVIC_SetPriority
  [Called By]
  - >> HAL_InitTick

  HAL_UART_Init (Thumb, 114 bytes, Stack size 8 bytes, stm32f4xx_hal_uart.o(i.HAL_UART_Init))
  [Stack]

  - Max Depth = 88
  - Call Chain = HAL_UART_Init ⇒ UART_SetConfig ⇒ __aeabi_uldivmod
  [Calls]
  - >> HAL_UART_MspInit
  - >> UART_SetConfig
  [Called By]
  - >> MX_USART6_UART_Init

  HAL_UART_MspInit (Thumb, 122 bytes, Stack size 32 bytes, usart.o(i.HAL_UART_MspInit))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  - >> __aeabi_memclr4
  [Called By]
  - >> HAL_UART_Init

  HAL_UART_Transmit (Thumb, 210 bytes, Stack size 40 bytes, stm32f4xx_hal_uart.o(i.HAL_UART_Transmit))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  - >> UART_WaitOnFlagUntilTimeout
  [Called By]
  - >> fputc

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.HardFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  MLX90640_BadPixelsCorrection (Thumb, 700 bytes, Stack size 56 bytes, mlx90640_api.o(i.MLX90640_BadPixelsCorrection))
  [Stack]

  - Max Depth = 108
  - Call Chain = MLX90640_BadPixelsCorrection ⇒ GetMedian(float*, int) ⇒ __aeabi_fadd ⇒ _float_epilogue
  [Calls]
  - >> __aeabi_fsub
  - >> __aeabi_fdiv
  - >> __aeabi_fadd
  - >> __aeabi_cfrcmple
  - >> std::fabs(float)
  - >> GetMedian(float*, int)
  - >> IsPixelBad(unsigned short, paramsMLX90640*)
  [Called By]
  - >> main

  MLX90640_CalculateTo (Thumb, 1968 bytes, Stack size 184 bytes, mlx90640_api.o(i.MLX90640_CalculateTo))
  [Stack]

  - Max Depth = 544
  - Call Chain = MLX90640_CalculateTo ⇒ MLX90640_GetTa ⇒ MLX90640_GetVdd ⇒ pow ⇒ __kernel_poly ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_d2f
  - >> MLX90640_GetVdd
  - >> MLX90640_GetTa
  - >> __aeabi_ui2d
  - >> __aeabi_ui2f
  - >> __aeabi_i2f
  - >> __aeabi_fsub
  - >> __aeabi_frsub
  - >> __aeabi_fmul
  - >> __aeabi_fdiv
  - >> __aeabi_fadd
  - >> __aeabi_cfrcmple
  - >> std::sqrt(float)
  - >> pow
  [Called By]
  - >> main

  MLX90640_DumpEE (Thumb, 24 bytes, Stack size 16 bytes, mlx90640_api.o(i.MLX90640_DumpEE))
  [Stack]

  - Max Depth = 168
  - Call Chain = MLX90640_DumpEE ⇒ MLX90640_I2CRead ⇒ HAL_I2C_Mem_Read ⇒ I2C_RequestMemoryRead ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> MLX90640_I2CRead
  [Called By]
  - >> main

  MLX90640_ExtractParameters (Thumb, 126 bytes, Stack size 16 bytes, mlx90640_api.o(i.MLX90640_ExtractParameters))
  [Stack]

  - Max Depth = 3624
  - Call Chain = MLX90640_ExtractParameters ⇒ ExtractAlphaParameters(unsigned short*, paramsMLX90640*) ⇒ pow ⇒ __kernel_poly ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> ExtractResolutionParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractKtaPixelParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractKvPixelParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractOffsetParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractDeviatingPixels(unsigned short*, paramsMLX90640*)
  - >> ExtractAlphaParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractPTATParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractKsToParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractKsTaParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractGainParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractCILCParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractVDDParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractTgcParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractCPParameters(unsigned short*, paramsMLX90640*)
  [Called By]
  - >> main

  MLX90640_GetFrameData (Thumb, 196 bytes, Stack size 32 bytes, mlx90640_api.o(i.MLX90640_GetFrameData))
  [Stack]

  - Max Depth = 224
  - Call Chain = MLX90640_GetFrameData ⇒ MLX90640_I2CWrite ⇒ MLX90640_I2CRead ⇒ HAL_I2C_Mem_Read ⇒ I2C_RequestMemoryRead ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> MLX90640_I2CWrite
  - >> MLX90640_I2CRead
  [Called By]
  - >> main

  MLX90640_GetRefreshRate (Thumb, 38 bytes, Stack size 24 bytes, mlx90640_api.o(i.MLX90640_GetRefreshRate))
  [Stack]

  - Max Depth = 176
  - Call Chain = MLX90640_GetRefreshRate ⇒ MLX90640_I2CRead ⇒ HAL_I2C_Mem_Read ⇒ I2C_RequestMemoryRead ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> MLX90640_I2CRead
  [Called By]
  - >> main

  MLX90640_GetTa (Thumb, 232 bytes, Stack size 72 bytes, mlx90640_api.o(i.MLX90640_GetTa))
  [Stack]

  - Max Depth = 360
  - Call Chain = MLX90640_GetTa ⇒ MLX90640_GetVdd ⇒ pow ⇒ __kernel_poly ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_f2d
  - >> __aeabi_d2f
  - >> MLX90640_GetVdd
  - >> __aeabi_dmul
  - >> __aeabi_ui2f
  - >> __aeabi_fsub
  - >> __aeabi_fmul
  - >> __aeabi_fdiv
  - >> __aeabi_fadd
  - >> __aeabi_cfrcmple
  - >> pow
  [Called By]
  - >> MLX90640_CalculateTo
  - >> main

  MLX90640_GetVdd (Thumb, 184 bytes, Stack size 64 bytes, mlx90640_api.o(i.MLX90640_GetVdd))
  [Stack]

  - Max Depth = 288
  - Call Chain = MLX90640_GetVdd ⇒ pow ⇒ __kernel_poly ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_d2f
  - >> __aeabi_ui2d
  - >> __aeabi_ui2f
  - >> __aeabi_i2f
  - >> __aeabi_i2d
  - >> __aeabi_fsub
  - >> __aeabi_fmul
  - >> __aeabi_fdiv
  - >> __aeabi_fadd
  - >> __aeabi_ddiv
  - >> __aeabi_cfrcmple
  - >> pow
  [Called By]
  - >> MLX90640_GetTa
  - >> MLX90640_CalculateTo
  - >> main

  MLX90640_I2CInit (Thumb, 8 bytes, Stack size 8 bytes, mlx90640_i2c_driver.o(i.MLX90640_I2CInit))
  [Stack]

  - Max Depth = 88
  - Call Chain = MLX90640_I2CInit ⇒ MX_I2C2_Init ⇒ HAL_I2C_Init ⇒ HAL_I2C_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> MX_I2C2_Init
  [Called By]
  - >> main

  MLX90640_I2CRead (Thumb, 90 bytes, Stack size 48 bytes, mlx90640_i2c_driver.o(i.MLX90640_I2CRead))
  [Stack]

  - Max Depth = 152
  - Call Chain = MLX90640_I2CRead ⇒ HAL_I2C_Mem_Read ⇒ I2C_RequestMemoryRead ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> HAL_I2C_Mem_Read
  [Called By]
  - >> MLX90640_SetRefreshRate
  - >> MLX90640_SetChessMode
  - >> MLX90640_GetRefreshRate
  - >> MLX90640_GetFrameData
  - >> MLX90640_DumpEE
  - >> MLX90640_I2CWrite

  MLX90640_I2CWrite (Thumb, 108 bytes, Stack size 40 bytes, mlx90640_i2c_driver.o(i.MLX90640_I2CWrite))
  [Stack]

  - Max Depth = 192
  - Call Chain = MLX90640_I2CWrite ⇒ MLX90640_I2CRead ⇒ HAL_I2C_Mem_Read ⇒ I2C_RequestMemoryRead ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> HAL_I2C_Mem_Write
  - >> MLX90640_I2CRead
  [Called By]
  - >> MLX90640_SetRefreshRate
  - >> MLX90640_SetChessMode
  - >> MLX90640_GetFrameData

  MLX90640_SetChessMode (Thumb, 48 bytes, Stack size 24 bytes, mlx90640_api.o(i.MLX90640_SetChessMode))
  [Stack]

  - Max Depth = 216
  - Call Chain = MLX90640_SetChessMode ⇒ MLX90640_I2CWrite ⇒ MLX90640_I2CRead ⇒ HAL_I2C_Mem_Read ⇒ I2C_RequestMemoryRead ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> MLX90640_I2CWrite
  - >> MLX90640_I2CRead
  [Called By]
  - >> main

  MLX90640_SetRefreshRate (Thumb, 58 bytes, Stack size 24 bytes, mlx90640_api.o(i.MLX90640_SetRefreshRate))
  [Stack]

  - Max Depth = 216
  - Call Chain = MLX90640_SetRefreshRate ⇒ MLX90640_I2CWrite ⇒ MLX90640_I2CRead ⇒ HAL_I2C_Mem_Read ⇒ I2C_RequestMemoryRead ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> MLX90640_I2CWrite
  - >> MLX90640_I2CRead
  [Called By]
  - >> main

  MSC_BOT_CplClrFeature (Thumb, 68 bytes, Stack size 16 bytes, usbd_msc_bot.o(i.MSC_BOT_CplClrFeature))
  [Stack]

  - Max Depth = 148
  - Call Chain = MSC_BOT_CplClrFeature ⇒ MSC_BOT_SendCSW ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> MSC_BOT_SendCSW
  - >> USBD_LL_StallEP
  [Called By]
  - >> USBD_MSC_Setup

  MSC_BOT_DataIn (Thumb, 86 bytes, Stack size 16 bytes, usbd_msc_bot.o(i.MSC_BOT_DataIn))
  [Stack]

  - Max Depth = 220
  - Call Chain = MSC_BOT_DataIn ⇒ SCSI_ProcessCmd ⇒ SCSI_Write12 ⇒ SCSI_ProcessWrite ⇒ MSC_BOT_SendCSW ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> SCSI_ProcessCmd
  - >> MSC_BOT_SendCSW
  [Called By]
  - >> USBD_MSC_DataIn

  MSC_BOT_DataOut (Thumb, 76 bytes, Stack size 16 bytes, usbd_msc_bot.o(i.MSC_BOT_DataOut))
  [Stack]

  - Max Depth = 236
  - Call Chain = MSC_BOT_DataOut ⇒ MSC_BOT_CBW_Decode ⇒ SCSI_ProcessCmd ⇒ SCSI_Write12 ⇒ SCSI_ProcessWrite ⇒ MSC_BOT_SendCSW ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> SCSI_ProcessCmd
  - >> MSC_BOT_SendCSW
  - >> MSC_BOT_CBW_Decode
  [Called By]
  - >> USBD_MSC_DataOut

  MSC_BOT_DeInit (Thumb, 14 bytes, Stack size 0 bytes, usbd_msc_bot.o(i.MSC_BOT_DeInit))
  [Called By]

  - >> USBD_MSC_DeInit

  MSC_BOT_Init (Thumb, 80 bytes, Stack size 16 bytes, usbd_msc_bot.o(i.MSC_BOT_Init))
  [Stack]

  - Max Depth = 132
  - Call Chain = MSC_BOT_Init ⇒ USBD_LL_PrepareReceive ⇒ HAL_PCD_EP_Receive ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_PrepareReceive
  - >> USBD_LL_FlushEP
  [Called By]
  - >> USBD_MSC_Init

  MSC_BOT_Reset (Thumb, 56 bytes, Stack size 16 bytes, usbd_msc_bot.o(i.MSC_BOT_Reset))
  [Stack]

  - Max Depth = 132
  - Call Chain = MSC_BOT_Reset ⇒ USBD_LL_PrepareReceive ⇒ HAL_PCD_EP_Receive ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_PrepareReceive
  - >> USBD_LL_ClearStallEP
  [Called By]
  - >> USBD_MSC_Setup

  MSC_BOT_SendCSW (Thumb, 66 bytes, Stack size 16 bytes, usbd_msc_bot.o(i.MSC_BOT_SendCSW))
  [Stack]

  - Max Depth = 132
  - Call Chain = MSC_BOT_SendCSW ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_Transmit
  - >> USBD_LL_PrepareReceive
  [Called By]
  - >> SCSI_ProcessWrite
  - >> MSC_BOT_CBW_Decode
  - >> MSC_BOT_DataOut
  - >> MSC_BOT_DataIn
  - >> MSC_BOT_CplClrFeature

  MX_ADC1_Init (Thumb, 100 bytes, Stack size 24 bytes, adc.o(i.MX_ADC1_Init))
  [Stack]

  - Max Depth = 96
  - Call Chain = MX_ADC1_Init ⇒ HAL_ADC_Init ⇒ HAL_ADC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_ADC_Init
  - >> HAL_ADC_ConfigChannel
  - >> Error_Handler
  [Called By]
  - >> main

  MX_FATFS_Init (Thumb, 16 bytes, Stack size 8 bytes, fatfs_1.o(i.MX_FATFS_Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = MX_FATFS_Init ⇒ FATFS_LinkDriver ⇒ FATFS_LinkDriverEx
  [Calls]
  - >> FATFS_LinkDriver
  [Called By]
  - >> main

  MX_FSMC_Init (Thumb, 114 bytes, Stack size 32 bytes, fsmc.o(i.MX_FSMC_Init))
  [Stack]

  - Max Depth = 112
  - Call Chain = MX_FSMC_Init ⇒ HAL_SRAM_Init ⇒ HAL_SRAM_MspInit ⇒ HAL_FSMC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_SRAM_Init
  - >> Error_Handler
  - >> __aeabi_memclr4
  [Called By]
  - >> main

  MX_GPIO_Init (Thumb, 392 bytes, Stack size 32 bytes, gpio.o(i.MX_GPIO_Init))
  [Stack]

  - Max Depth = 80
  - Call Chain = MX_GPIO_Init ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  - >> HAL_GPIO_WritePin
  - >> HAL_GPIO_Init
  - >> __aeabi_memclr4
  [Called By]
  - >> main

  MX_I2C2_Init (Thumb, 48 bytes, Stack size 8 bytes, i2c.o(i.MX_I2C2_Init))
  [Stack]

  - Max Depth = 80
  - Call Chain = MX_I2C2_Init ⇒ HAL_I2C_Init ⇒ HAL_I2C_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_I2C_Init
  - >> Error_Handler
  [Called By]
  - >> MLX90640_I2CInit
  - >> main

  MX_SPI3_Init (Thumb, 60 bytes, Stack size 8 bytes, spi.o(i.MX_SPI3_Init))
  [Stack]

  - Max Depth = 72
  - Call Chain = MX_SPI3_Init ⇒ HAL_SPI_Init ⇒ HAL_SPI_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_SPI_Init
  - >> Error_Handler
  [Called By]
  - >> main

  MX_USART6_UART_Init (Thumb, 46 bytes, Stack size 8 bytes, usart.o(i.MX_USART6_UART_Init))
  [Stack]

  - Max Depth = 96
  - Call Chain = MX_USART6_UART_Init ⇒ HAL_UART_Init ⇒ UART_SetConfig ⇒ __aeabi_uldivmod
  [Calls]
  - >> HAL_UART_Init
  - >> Error_Handler
  [Called By]
  - >> main

  MX_USB_DEVICE_Init (Thumb, 60 bytes, Stack size 8 bytes, usb_device.o(i.MX_USB_DEVICE_Init))
  [Stack]

  - Max Depth = 176
  - Call Chain = MX_USB_DEVICE_Init ⇒ USBD_Init ⇒ USBD_LL_Init ⇒ HAL_PCD_Init ⇒ HAL_PCD_MspInit ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> Error_Handler
  - >> USBD_Start
  - >> USBD_RegisterClass
  - >> USBD_MSC_RegisterStorage
  - >> USBD_Init
  [Called By]
  - >> main

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.MemManage_Handler))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  MySPI_Init (Thumb, 14 bytes, Stack size 8 bytes, w25q64.o(i.MySPI_Init))
  [Stack]

  - Max Depth = 8
  - Call Chain = MySPI_Init
  [Calls]
  - >> HAL_GPIO_WritePin
  [Called By]
  - >> W25Q64_Init

  MySPI_Start (Thumb, 16 bytes, Stack size 8 bytes, w25q64.o(i.MySPI_Start))
  [Stack]

  - Max Depth = 8
  - Call Chain = MySPI_Start
  [Calls]
  - >> HAL_GPIO_WritePin
  [Called By]
  - >> W25Q64_Read
  - >> W25Q64_WriteEnable
  - >> W25Q64_WaitBusy
  - >> W25Q64_SectorErase
  - >> W25Q64_ReadID
  - >> W25Q64_PageProgram

  MySPI_Stop (Thumb, 14 bytes, Stack size 8 bytes, w25q64.o(i.MySPI_Stop))
  [Stack]

  - Max Depth = 8
  - Call Chain = MySPI_Stop
  [Calls]
  - >> HAL_GPIO_WritePin
  [Called By]
  - >> W25Q64_Read
  - >> W25Q64_WriteEnable
  - >> W25Q64_WaitBusy
  - >> W25Q64_SectorErase
  - >> W25Q64_ReadID
  - >> W25Q64_PageProgram

  MySPI_SwapByte (Thumb, 30 bytes, Stack size 16 bytes, w25q64.o(i.MySPI_SwapByte))
  [Stack]

  - Max Depth = 136
  - Call Chain = MySPI_SwapByte ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_SPI_TransmitReceive
  [Called By]
  - >> W25Q64_Read
  - >> W25Q64_WriteEnable
  - >> W25Q64_WaitBusy
  - >> W25Q64_SectorErase
  - >> W25Q64_ReadID
  - >> W25Q64_PageProgram

  NMI_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  OTG_FS_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, stm32f4xx_it.o(i.OTG_FS_IRQHandler))
  [Stack]

  - Max Depth = 284
  - Call Chain = OTG_FS_IRQHandler ⇒ HAL_PCD_IRQHandler ⇒ PCD_EP_OutSetupPacket_int ⇒ HAL_PCD_SetupStageCallback ⇒ USBD_LL_SetupStage ⇒ USBD_StdDevReq ⇒ USBD_GetDescriptor ⇒ USBD_CtlSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> HAL_PCD_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f407xx.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  SCSI_ProcessCmd (Thumb, 336 bytes, Stack size 24 bytes, usbd_msc_scsi.o(i.SCSI_ProcessCmd))
  [Stack]

  - Max Depth = 204
  - Call Chain = SCSI_ProcessCmd ⇒ SCSI_Write12 ⇒ SCSI_ProcessWrite ⇒ MSC_BOT_SendCSW ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> SCSI_Write12
  - >> SCSI_Write10
  - >> SCSI_Verify10
  - >> SCSI_TestUnitReady
  - >> SCSI_StartStopUnit
  - >> SCSI_RequestSense
  - >> SCSI_ReadFormatCapacity
  - >> SCSI_ReadCapacity16
  - >> SCSI_ReadCapacity10
  - >> SCSI_Read12
  - >> SCSI_Read10
  - >> SCSI_ModeSense6
  - >> SCSI_ModeSense10
  - >> SCSI_Inquiry
  - >> SCSI_AllowPreventRemovable
  - >> SCSI_SenseCode
  [Called By]
  - >> MSC_BOT_CBW_Decode
  - >> MSC_BOT_DataOut
  - >> MSC_BOT_DataIn

  SCSI_SenseCode (Thumb, 94 bytes, Stack size 20 bytes, usbd_msc_scsi.o(i.SCSI_SenseCode))
  [Stack]

  - Max Depth = 20
  - Call Chain = SCSI_SenseCode
  [Called By]
  - >> SCSI_Write12
  - >> SCSI_Write10
  - >> SCSI_Verify10
  - >> SCSI_TestUnitReady
  - >> SCSI_StartStopUnit
  - >> SCSI_RequestSense
  - >> SCSI_ReadFormatCapacity
  - >> SCSI_ReadCapacity16
  - >> SCSI_ReadCapacity10
  - >> SCSI_Read12
  - >> SCSI_Read10
  - >> SCSI_ProcessWrite
  - >> SCSI_ProcessRead
  - >> SCSI_Inquiry
  - >> SCSI_CheckAddressRange
  - >> SCSI_ProcessCmd
  - >> MSC_BOT_CBW_Decode

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  SaveScreenBMP (Thumb, 500 bytes, Stack size 5800 bytes, main.o(i.SaveScreenBMP))
  [Stack]

  - Max Depth = 6120
  - Call Chain = SaveScreenBMP ⇒ f_open ⇒ follow_path ⇒ dir_find ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write
  [Calls]
  - >> lcd_read_point
  - >> f_write
  - >> f_sync
  - >> f_open
  - >> f_close
  - >> __aeabi_memcpy4
  - >> __aeabi_memcpy
  - >> __2sprintf
  - >> __2printf
  [Called By]
  - >> main

  SysTick_Handler (Thumb, 8 bytes, Stack size 8 bytes, stm32f4xx_it.o(i.SysTick_Handler))
  [Stack]

  - Max Depth = 8
  - Call Chain = SysTick_Handler
  [Calls]
  - >> HAL_IncTick
  [Address Reference Count : 1]
  - startup_stm32f407xx.o(RESET)

  SystemClock_Config (Thumb, 172 bytes, Stack size 80 bytes, main.o(i.SystemClock_Config))
  [Stack]

  - Max Depth = 168
  - Call Chain = SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uldivmod
  [Calls]
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  - >> Error_Handler
  - >> __aeabi_memclr4
  [Called By]
  - >> main

  SystemInit (Thumb, 2 bytes, Stack size 0 bytes, system_stm32f4xx.o(i.SystemInit))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(.text)

  USBD_ClrClassConfig (Thumb, 28 bytes, Stack size 16 bytes, usbd_core.o(i.USBD_ClrClassConfig))
  [Stack]

  - Max Depth = 16
  - Call Chain = USBD_ClrClassConfig
  [Called By]
  - >> USBD_SetConfig

  USBD_CtlContinueRx (Thumb, 24 bytes, Stack size 16 bytes, usbd_ioreq.o(i.USBD_CtlContinueRx))
  [Stack]

  - Max Depth = 132
  - Call Chain = USBD_CtlContinueRx ⇒ USBD_LL_PrepareReceive ⇒ HAL_PCD_EP_Receive ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_PrepareReceive
  [Called By]
  - >> USBD_LL_DataOutStage

  USBD_CtlContinueSendData (Thumb, 24 bytes, Stack size 16 bytes, usbd_ioreq.o(i.USBD_CtlContinueSendData))
  [Stack]

  - Max Depth = 132
  - Call Chain = USBD_CtlContinueSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_Transmit
  [Called By]
  - >> USBD_LL_DataInStage

  USBD_CtlError (Thumb, 24 bytes, Stack size 16 bytes, usbd_ctlreq.o(i.USBD_CtlError))
  [Stack]

  - Max Depth = 72
  - Call Chain = USBD_CtlError ⇒ USBD_LL_StallEP ⇒ HAL_PCD_EP_SetStall ⇒ USB_EP0_OutStart
  [Calls]
  - >> USBD_LL_StallEP
  [Called By]
  - >> USBD_MSC_Setup
  - >> USBD_SetConfig
  - >> USBD_SetAddress
  - >> USBD_GetStatus
  - >> USBD_GetDescriptor
  - >> USBD_GetConfig
  - >> USBD_ClrFeature
  - >> USBD_StdItfReq
  - >> USBD_StdEPReq
  - >> USBD_StdDevReq

  USBD_CtlReceiveStatus (Thumb, 26 bytes, Stack size 8 bytes, usbd_ioreq.o(i.USBD_CtlReceiveStatus))
  [Stack]

  - Max Depth = 124
  - Call Chain = USBD_CtlReceiveStatus ⇒ USBD_LL_PrepareReceive ⇒ HAL_PCD_EP_Receive ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_PrepareReceive
  [Called By]
  - >> USBD_LL_DataInStage

  USBD_CtlSendData (Thumb, 34 bytes, Stack size 16 bytes, usbd_ioreq.o(i.USBD_CtlSendData))
  [Stack]

  - Max Depth = 132
  - Call Chain = USBD_CtlSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_Transmit
  [Called By]
  - >> USBD_MSC_Setup
  - >> USBD_GetStatus
  - >> USBD_GetDescriptor
  - >> USBD_GetConfig
  - >> USBD_StdEPReq

  USBD_CtlSendStatus (Thumb, 26 bytes, Stack size 8 bytes, usbd_ioreq.o(i.USBD_CtlSendStatus))
  [Stack]

  - Max Depth = 124
  - Call Chain = USBD_CtlSendStatus ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_Transmit
  [Called By]
  - >> USBD_LL_DataOutStage
  - >> USBD_SetFeature
  - >> USBD_SetConfig
  - >> USBD_SetAddress
  - >> USBD_GetDescriptor
  - >> USBD_ClrFeature
  - >> USBD_StdItfReq
  - >> USBD_StdEPReq

  USBD_FS_ConfigStrDescriptor (Thumb, 34 bytes, Stack size 16 bytes, usbd_desc.o(i.USBD_FS_ConfigStrDescriptor))
  [Stack]

  - Max Depth = 40
  - Call Chain = USBD_FS_ConfigStrDescriptor ⇒ USBD_GetString
  [Calls]
  - >> USBD_GetString
  [Address Reference Count : 1]
  - usbd_desc.o(.data)

  USBD_FS_DeviceDescriptor (Thumb, 10 bytes, Stack size 0 bytes, usbd_desc.o(i.USBD_FS_DeviceDescriptor))
  [Address Reference Count : 1]

  - usbd_desc.o(.data)

  USBD_FS_InterfaceStrDescriptor (Thumb, 34 bytes, Stack size 16 bytes, usbd_desc.o(i.USBD_FS_InterfaceStrDescriptor))
  [Stack]

  - Max Depth = 40
  - Call Chain = USBD_FS_InterfaceStrDescriptor ⇒ USBD_GetString
  [Calls]
  - >> USBD_GetString
  [Address Reference Count : 1]
  - usbd_desc.o(.data)

  USBD_FS_LangIDStrDescriptor (Thumb, 10 bytes, Stack size 0 bytes, usbd_desc.o(i.USBD_FS_LangIDStrDescriptor))
  [Address Reference Count : 1]

  - usbd_desc.o(.data)

  USBD_FS_ManufacturerStrDescriptor (Thumb, 20 bytes, Stack size 16 bytes, usbd_desc.o(i.USBD_FS_ManufacturerStrDescriptor))
  [Stack]

  - Max Depth = 40
  - Call Chain = USBD_FS_ManufacturerStrDescriptor ⇒ USBD_GetString
  [Calls]
  - >> USBD_GetString
  [Address Reference Count : 1]
  - usbd_desc.o(.data)

  USBD_FS_ProductStrDescriptor (Thumb, 34 bytes, Stack size 16 bytes, usbd_desc.o(i.USBD_FS_ProductStrDescriptor))
  [Stack]

  - Max Depth = 40
  - Call Chain = USBD_FS_ProductStrDescriptor ⇒ USBD_GetString
  [Calls]
  - >> USBD_GetString
  [Address Reference Count : 1]
  - usbd_desc.o(.data)

  USBD_FS_SerialStrDescriptor (Thumb, 18 bytes, Stack size 16 bytes, usbd_desc.o(i.USBD_FS_SerialStrDescriptor))
  [Stack]

  - Max Depth = 44
  - Call Chain = USBD_FS_SerialStrDescriptor ⇒ Get_SerialNum ⇒ IntToUnicode
  [Calls]
  - >> Get_SerialNum
  [Address Reference Count : 1]
  - usbd_desc.o(.data)

  USBD_GetString (Thumb, 84 bytes, Stack size 24 bytes, usbd_ctlreq.o(i.USBD_GetString))
  [Stack]

  - Max Depth = 24
  - Call Chain = USBD_GetString
  [Calls]
  - >> USBD_GetLen
  [Called By]
  - >> USBD_FS_ProductStrDescriptor
  - >> USBD_FS_ManufacturerStrDescriptor
  - >> USBD_FS_InterfaceStrDescriptor
  - >> USBD_FS_ConfigStrDescriptor

  USBD_Get_USB_Status (Thumb, 44 bytes, Stack size 0 bytes, usbd_conf.o(i.USBD_Get_USB_Status))
  [Called By]

  - >> USBD_LL_Transmit
  - >> USBD_LL_Start
  - >> USBD_LL_StallEP
  - >> USBD_LL_SetUSBAddress
  - >> USBD_LL_PrepareReceive
  - >> USBD_LL_OpenEP
  - >> USBD_LL_FlushEP
  - >> USBD_LL_CloseEP
  - >> USBD_LL_ClearStallEP

  USBD_Init (Thumb, 58 bytes, Stack size 24 bytes, usbd_core.o(i.USBD_Init))
  [Stack]

  - Max Depth = 168
  - Call Chain = USBD_Init ⇒ USBD_LL_Init ⇒ HAL_PCD_Init ⇒ HAL_PCD_MspInit ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> USBD_LL_Init
  [Called By]
  - >> MX_USB_DEVICE_Init

  USBD_LL_ClearStallEP (Thumb, 38 bytes, Stack size 24 bytes, usbd_conf.o(i.USBD_LL_ClearStallEP))
  [Stack]

  - Max Depth = 52
  - Call Chain = USBD_LL_ClearStallEP ⇒ HAL_PCD_EP_ClrStall ⇒ USB_EPClearStall
  [Calls]
  - >> HAL_PCD_EP_ClrStall
  - >> USBD_Get_USB_Status
  [Called By]
  - >> MSC_BOT_Reset
  - >> USBD_StdEPReq

  USBD_LL_CloseEP (Thumb, 38 bytes, Stack size 24 bytes, usbd_conf.o(i.USBD_LL_CloseEP))
  [Stack]

  - Max Depth = 56
  - Call Chain = USBD_LL_CloseEP ⇒ HAL_PCD_EP_Close ⇒ USB_DeactivateEndpoint
  [Calls]
  - >> HAL_PCD_EP_Close
  - >> USBD_Get_USB_Status
  [Called By]
  - >> USBD_MSC_DeInit

  USBD_LL_DataInStage (Thumb, 226 bytes, Stack size 24 bytes, usbd_core.o(i.USBD_LL_DataInStage))
  [Stack]

  - Max Depth = 156
  - Call Chain = USBD_LL_DataInStage ⇒ USBD_CtlContinueSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_StallEP
  - >> USBD_LL_PrepareReceive
  - >> USBD_CtlReceiveStatus
  - >> USBD_CtlContinueSendData
  - >> USBD_RunTestMode
  [Called By]
  - >> HAL_PCD_DataInStageCallback

  USBD_LL_DataOutStage (Thumb, 142 bytes, Stack size 24 bytes, usbd_core.o(i.USBD_LL_DataOutStage))
  [Stack]

  - Max Depth = 156
  - Call Chain = USBD_LL_DataOutStage ⇒ USBD_CtlContinueRx ⇒ USBD_LL_PrepareReceive ⇒ HAL_PCD_EP_Receive ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_CtlSendStatus
  - >> USBD_CtlContinueRx
  [Called By]
  - >> HAL_PCD_DataOutStageCallback

  USBD_LL_DevConnected (Thumb, 6 bytes, Stack size 0 bytes, usbd_core.o(i.USBD_LL_DevConnected))
  [Called By]

  - >> HAL_PCD_ConnectCallback

  USBD_LL_DevDisconnected (Thumb, 32 bytes, Stack size 8 bytes, usbd_core.o(i.USBD_LL_DevDisconnected))
  [Stack]

  - Max Depth = 8
  - Call Chain = USBD_LL_DevDisconnected
  [Called By]
  - >> HAL_PCD_DisconnectCallback

  USBD_LL_FlushEP (Thumb, 38 bytes, Stack size 24 bytes, usbd_conf.o(i.USBD_LL_FlushEP))
  [Stack]

  - Max Depth = 48
  - Call Chain = USBD_LL_FlushEP ⇒ HAL_PCD_EP_Flush ⇒ USB_FlushTxFifo
  [Calls]
  - >> HAL_PCD_EP_Flush
  - >> USBD_Get_USB_Status
  [Called By]
  - >> MSC_BOT_Init
  - >> USBD_MSC_Setup

  USBD_LL_GetRxDataSize (Thumb, 18 bytes, Stack size 16 bytes, usbd_conf.o(i.USBD_LL_GetRxDataSize))
  [Stack]

  - Max Depth = 16
  - Call Chain = USBD_LL_GetRxDataSize
  [Calls]
  - >> HAL_PCD_EP_GetRxCount
  [Called By]
  - >> MSC_BOT_CBW_Decode

  USBD_LL_Init (Thumb, 100 bytes, Stack size 8 bytes, usbd_conf.o(i.USBD_LL_Init))
  [Stack]

  - Max Depth = 144
  - Call Chain = USBD_LL_Init ⇒ HAL_PCD_Init ⇒ HAL_PCD_MspInit ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> Error_Handler
  - >> HAL_PCD_Init
  - >> HAL_PCDEx_SetTxFiFo
  - >> HAL_PCDEx_SetRxFiFo
  [Called By]
  - >> USBD_Init

  USBD_LL_IsStallEP (Thumb, 56 bytes, Stack size 8 bytes, usbd_conf.o(i.USBD_LL_IsStallEP))
  [Stack]

  - Max Depth = 8
  - Call Chain = USBD_LL_IsStallEP
  [Called By]
  - >> USBD_StdEPReq

  USBD_LL_IsoINIncomplete (Thumb, 48 bytes, Stack size 16 bytes, usbd_core.o(i.USBD_LL_IsoINIncomplete))
  [Stack]

  - Max Depth = 16
  - Call Chain = USBD_LL_IsoINIncomplete
  [Called By]
  - >> HAL_PCD_ISOINIncompleteCallback

  USBD_LL_IsoOUTIncomplete (Thumb, 48 bytes, Stack size 16 bytes, usbd_core.o(i.USBD_LL_IsoOUTIncomplete))
  [Stack]

  - Max Depth = 16
  - Call Chain = USBD_LL_IsoOUTIncomplete
  [Called By]
  - >> HAL_PCD_ISOOUTIncompleteCallback

  USBD_LL_OpenEP (Thumb, 48 bytes, Stack size 32 bytes, usbd_conf.o(i.USBD_LL_OpenEP))
  [Stack]

  - Max Depth = 80
  - Call Chain = USBD_LL_OpenEP ⇒ HAL_PCD_EP_Open ⇒ USB_ActivateEndpoint
  [Calls]
  - >> HAL_PCD_EP_Open
  - >> USBD_Get_USB_Status
  [Called By]
  - >> USBD_MSC_Init
  - >> USBD_LL_Reset

  USBD_LL_PrepareReceive (Thumb, 48 bytes, Stack size 32 bytes, usbd_conf.o(i.USBD_LL_PrepareReceive))
  [Stack]

  - Max Depth = 116
  - Call Chain = USBD_LL_PrepareReceive ⇒ HAL_PCD_EP_Receive ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> HAL_PCD_EP_Receive
  - >> USBD_Get_USB_Status
  [Called By]
  - >> SCSI_Write12
  - >> SCSI_Write10
  - >> SCSI_ProcessWrite
  - >> MSC_BOT_SendCSW
  - >> MSC_BOT_Reset
  - >> MSC_BOT_Init
  - >> USBD_LL_DataInStage
  - >> USBD_CtlReceiveStatus
  - >> USBD_CtlContinueRx

  USBD_LL_Reset (Thumb, 108 bytes, Stack size 8 bytes, usbd_core.o(i.USBD_LL_Reset))
  [Stack]

  - Max Depth = 88
  - Call Chain = USBD_LL_Reset ⇒ USBD_LL_OpenEP ⇒ HAL_PCD_EP_Open ⇒ USB_ActivateEndpoint
  [Calls]
  - >> USBD_LL_OpenEP
  [Called By]
  - >> HAL_PCD_ResetCallback

  USBD_LL_Resume (Thumb, 22 bytes, Stack size 0 bytes, usbd_core.o(i.USBD_LL_Resume))
  [Called By]

  - >> HAL_PCD_ResumeCallback

  USBD_LL_SOF (Thumb, 44 bytes, Stack size 8 bytes, usbd_core.o(i.USBD_LL_SOF))
  [Stack]

  - Max Depth = 8
  - Call Chain = USBD_LL_SOF
  [Called By]
  - >> HAL_PCD_SOFCallback

  USBD_LL_SetSpeed (Thumb, 8 bytes, Stack size 0 bytes, usbd_core.o(i.USBD_LL_SetSpeed))
  [Called By]

  - >> HAL_PCD_ResetCallback

  USBD_LL_SetUSBAddress (Thumb, 38 bytes, Stack size 24 bytes, usbd_conf.o(i.USBD_LL_SetUSBAddress))
  [Stack]

  - Max Depth = 48
  - Call Chain = USBD_LL_SetUSBAddress ⇒ HAL_PCD_SetAddress ⇒ USB_SetDevAddress
  [Calls]
  - >> HAL_PCD_SetAddress
  - >> USBD_Get_USB_Status
  [Called By]
  - >> USBD_SetAddress

  USBD_LL_SetupStage (Thumb, 118 bytes, Stack size 16 bytes, usbd_core.o(i.USBD_LL_SetupStage))
  [Stack]

  - Max Depth = 188
  - Call Chain = USBD_LL_SetupStage ⇒ USBD_StdDevReq ⇒ USBD_GetDescriptor ⇒ USBD_CtlSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_StallEP
  - >> USBD_StdItfReq
  - >> USBD_StdEPReq
  - >> USBD_StdDevReq
  - >> USBD_ParseSetupRequest
  [Called By]
  - >> HAL_PCD_SetupStageCallback

  USBD_LL_StallEP (Thumb, 38 bytes, Stack size 24 bytes, usbd_conf.o(i.USBD_LL_StallEP))
  [Stack]

  - Max Depth = 56
  - Call Chain = USBD_LL_StallEP ⇒ HAL_PCD_EP_SetStall ⇒ USB_EP0_OutStart
  [Calls]
  - >> HAL_PCD_EP_SetStall
  - >> USBD_Get_USB_Status
  [Called By]
  - >> MSC_BOT_Abort
  - >> MSC_BOT_CplClrFeature
  - >> USBD_CtlError
  - >> USBD_LL_SetupStage
  - >> USBD_LL_DataInStage
  - >> USBD_StdEPReq

  USBD_LL_Start (Thumb, 30 bytes, Stack size 16 bytes, usbd_conf.o(i.USBD_LL_Start))
  [Stack]

  - Max Depth = 32
  - Call Chain = USBD_LL_Start ⇒ HAL_PCD_Start
  [Calls]
  - >> HAL_PCD_Start
  - >> USBD_Get_USB_Status
  [Called By]
  - >> USBD_Start

  USBD_LL_Suspend (Thumb, 20 bytes, Stack size 0 bytes, usbd_core.o(i.USBD_LL_Suspend))
  [Called By]

  - >> HAL_PCD_SuspendCallback

  USBD_LL_Transmit (Thumb, 48 bytes, Stack size 32 bytes, usbd_conf.o(i.USBD_LL_Transmit))
  [Stack]

  - Max Depth = 116
  - Call Chain = USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> HAL_PCD_EP_Transmit
  - >> USBD_Get_USB_Status
  [Called By]
  - >> SCSI_ProcessRead
  - >> MSC_BOT_SendCSW
  - >> MSC_BOT_SendData
  - >> USBD_CtlSendData
  - >> USBD_CtlSendStatus
  - >> USBD_CtlContinueSendData

  USBD_MSC_DataIn (Thumb, 18 bytes, Stack size 16 bytes, usbd_msc.o(i.USBD_MSC_DataIn))
  [Stack]

  - Max Depth = 236
  - Call Chain = USBD_MSC_DataIn ⇒ MSC_BOT_DataIn ⇒ SCSI_ProcessCmd ⇒ SCSI_Write12 ⇒ SCSI_ProcessWrite ⇒ MSC_BOT_SendCSW ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> MSC_BOT_DataIn
  [Address Reference Count : 1]
  - usbd_msc.o(.data)

  USBD_MSC_DataOut (Thumb, 18 bytes, Stack size 16 bytes, usbd_msc.o(i.USBD_MSC_DataOut))
  [Stack]

  - Max Depth = 252
  - Call Chain = USBD_MSC_DataOut ⇒ MSC_BOT_DataOut ⇒ MSC_BOT_CBW_Decode ⇒ SCSI_ProcessCmd ⇒ SCSI_Write12 ⇒ SCSI_ProcessWrite ⇒ MSC_BOT_SendCSW ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> MSC_BOT_DataOut
  [Address Reference Count : 1]
  - usbd_msc.o(.data)

  USBD_MSC_DeInit (Thumb, 62 bytes, Stack size 16 bytes, usbd_msc.o(i.USBD_MSC_DeInit))
  [Stack]

  - Max Depth = 72
  - Call Chain = USBD_MSC_DeInit ⇒ USBD_LL_CloseEP ⇒ HAL_PCD_EP_Close ⇒ USB_DeactivateEndpoint
  [Calls]
  - >> MSC_BOT_DeInit
  - >> USBD_static_free
  - >> USBD_LL_CloseEP
  [Address Reference Count : 1]
  - usbd_msc.o(.data)

  USBD_MSC_GetDeviceQualifierDescriptor (Thumb, 10 bytes, Stack size 0 bytes, usbd_msc.o(i.USBD_MSC_GetDeviceQualifierDescriptor))
  [Address Reference Count : 1]

  - usbd_msc.o(.data)

  USBD_MSC_GetFSCfgDesc (Thumb, 10 bytes, Stack size 0 bytes, usbd_msc.o(i.USBD_MSC_GetFSCfgDesc))
  [Address Reference Count : 1]

  - usbd_msc.o(.data)

  USBD_MSC_GetHSCfgDesc (Thumb, 10 bytes, Stack size 0 bytes, usbd_msc.o(i.USBD_MSC_GetHSCfgDesc))
  [Address Reference Count : 1]

  - usbd_msc.o(.data)

  USBD_MSC_GetOtherSpeedCfgDesc (Thumb, 10 bytes, Stack size 0 bytes, usbd_msc.o(i.USBD_MSC_GetOtherSpeedCfgDesc))
  [Address Reference Count : 1]

  - usbd_msc.o(.data)

  USBD_MSC_Init (Thumb, 118 bytes, Stack size 16 bytes, usbd_msc.o(i.USBD_MSC_Init))
  [Stack]

  - Max Depth = 148
  - Call Chain = USBD_MSC_Init ⇒ MSC_BOT_Init ⇒ USBD_LL_PrepareReceive ⇒ HAL_PCD_EP_Receive ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> MSC_BOT_Init
  - >> USBD_static_malloc
  - >> USBD_LL_OpenEP
  [Address Reference Count : 1]
  - usbd_msc.o(.data)

  USBD_MSC_RegisterStorage (Thumb, 16 bytes, Stack size 0 bytes, usbd_msc.o(i.USBD_MSC_RegisterStorage))
  [Called By]

  - >> MX_USB_DEVICE_Init

  USBD_MSC_Setup (Thumb, 330 bytes, Stack size 24 bytes, usbd_msc.o(i.USBD_MSC_Setup))
  [Stack]

  - Max Depth = 172
  - Call Chain = USBD_MSC_Setup ⇒ MSC_BOT_CplClrFeature ⇒ MSC_BOT_SendCSW ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> MSC_BOT_Reset
  - >> MSC_BOT_CplClrFeature
  - >> USBD_CtlSendData
  - >> USBD_CtlError
  - >> USBD_LL_FlushEP
  [Address Reference Count : 1]
  - usbd_msc.o(.data)

  USBD_ParseSetupRequest (Thumb, 54 bytes, Stack size 16 bytes, usbd_ctlreq.o(i.USBD_ParseSetupRequest))
  [Stack]

  - Max Depth = 28
  - Call Chain = USBD_ParseSetupRequest ⇒ SWAPBYTE
  [Calls]
  - >> SWAPBYTE
  [Called By]
  - >> USBD_LL_SetupStage

  USBD_RegisterClass (Thumb, 46 bytes, Stack size 16 bytes, usbd_core.o(i.USBD_RegisterClass))
  [Stack]

  - Max Depth = 16
  - Call Chain = USBD_RegisterClass
  [Called By]
  - >> MX_USB_DEVICE_Init

  USBD_RunTestMode (Thumb, 6 bytes, Stack size 0 bytes, usbd_core.o(i.USBD_RunTestMode))
  [Called By]

  - >> USBD_LL_DataInStage

  USBD_SetClassConfig (Thumb, 32 bytes, Stack size 16 bytes, usbd_core.o(i.USBD_SetClassConfig))
  [Stack]

  - Max Depth = 16
  - Call Chain = USBD_SetClassConfig
  [Called By]
  - >> USBD_SetConfig

  USBD_Start (Thumb, 12 bytes, Stack size 8 bytes, usbd_core.o(i.USBD_Start))
  [Stack]

  - Max Depth = 40
  - Call Chain = USBD_Start ⇒ USBD_LL_Start ⇒ HAL_PCD_Start
  [Calls]
  - >> USBD_LL_Start
  [Called By]
  - >> MX_USB_DEVICE_Init

  USBD_StdDevReq (Thumb, 166 bytes, Stack size 16 bytes, usbd_ctlreq.o(i.USBD_StdDevReq))
  [Stack]

  - Max Depth = 172
  - Call Chain = USBD_StdDevReq ⇒ USBD_GetDescriptor ⇒ USBD_CtlSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_CtlError
  - >> USBD_SetFeature
  - >> USBD_SetConfig
  - >> USBD_SetAddress
  - >> USBD_GetStatus
  - >> USBD_GetDescriptor
  - >> USBD_GetConfig
  - >> USBD_ClrFeature
  [Called By]
  - >> USBD_LL_SetupStage

  USBD_StdEPReq (Thumb, 556 bytes, Stack size 24 bytes, usbd_ctlreq.o(i.USBD_StdEPReq))
  [Stack]

  - Max Depth = 156
  - Call Chain = USBD_StdEPReq ⇒ USBD_CtlSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_CtlSendData
  - >> USBD_CtlError
  - >> USBD_LL_StallEP
  - >> USBD_LL_IsStallEP
  - >> USBD_LL_ClearStallEP
  - >> USBD_CtlSendStatus
  [Called By]
  - >> USBD_LL_SetupStage

  USBD_StdItfReq (Thumb, 126 bytes, Stack size 16 bytes, usbd_ctlreq.o(i.USBD_StdItfReq))
  [Stack]

  - Max Depth = 140
  - Call Chain = USBD_StdItfReq ⇒ USBD_CtlSendStatus ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_CtlError
  - >> USBD_CtlSendStatus
  [Called By]
  - >> USBD_LL_SetupStage

  USBD_static_free (Thumb, 2 bytes, Stack size 0 bytes, usbd_conf.o(i.USBD_static_free))
  [Called By]

  - >> USBD_MSC_DeInit

  USBD_static_malloc (Thumb, 6 bytes, Stack size 0 bytes, usbd_conf.o(i.USBD_static_malloc))
  [Called By]

  - >> USBD_MSC_Init

  USB_ActivateEndpoint (Thumb, 202 bytes, Stack size 16 bytes, stm32f4xx_ll_usb.o(i.USB_ActivateEndpoint))
  [Stack]

  - Max Depth = 16
  - Call Chain = USB_ActivateEndpoint
  [Called By]
  - >> HAL_PCD_EP_Open

  USB_ActivateSetup (Thumb, 40 bytes, Stack size 0 bytes, stm32f4xx_ll_usb.o(i.USB_ActivateSetup))
  [Called By]

  - >> HAL_PCD_IRQHandler

  USB_CoreInit (Thumb, 128 bytes, Stack size 32 bytes, stm32f4xx_ll_usb.o(i.USB_CoreInit))
  [Stack]

  - Max Depth = 40
  - Call Chain = USB_CoreInit ⇒ USB_CoreReset
  [Calls]
  - >> USB_CoreReset
  [Called By]
  - >> HAL_PCD_Init

  USB_DeactivateEndpoint (Thumb, 318 bytes, Stack size 16 bytes, stm32f4xx_ll_usb.o(i.USB_DeactivateEndpoint))
  [Stack]

  - Max Depth = 16
  - Call Chain = USB_DeactivateEndpoint
  [Called By]
  - >> HAL_PCD_EP_Close

  USB_DevConnect (Thumb, 36 bytes, Stack size 0 bytes, stm32f4xx_ll_usb.o(i.USB_DevConnect))
  [Called By]

  - >> HAL_PCD_Start

  USB_DevDisconnect (Thumb, 36 bytes, Stack size 0 bytes, stm32f4xx_ll_usb.o(i.USB_DevDisconnect))
  [Called By]

  - >> HAL_PCD_Init

  USB_DevInit (Thumb, 472 bytes, Stack size 36 bytes, stm32f4xx_ll_usb.o(i.USB_DevInit))
  [Stack]

  - Max Depth = 44
  - Call Chain = USB_DevInit ⇒ USB_FlushTxFifo
  [Calls]
  - >> USB_FlushTxFifo
  - >> USB_FlushRxFifo
  - >> USB_SetDevSpeed
  [Called By]
  - >> HAL_PCD_Init

  USB_DisableGlobalInt (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_ll_usb.o(i.USB_DisableGlobalInt))
  [Called By]

  - >> HAL_PCD_Init

  USB_EP0StartXfer (Thumb, 468 bytes, Stack size 20 bytes, stm32f4xx_ll_usb.o(i.USB_EP0StartXfer))
  [Stack]

  - Max Depth = 20
  - Call Chain = USB_EP0StartXfer
  [Called By]
  - >> HAL_PCD_EP_Transmit
  - >> HAL_PCD_EP_Receive

  USB_EP0_OutStart (Thumb, 106 bytes, Stack size 16 bytes, stm32f4xx_ll_usb.o(i.USB_EP0_OutStart))
  [Stack]

  - Max Depth = 16
  - Call Chain = USB_EP0_OutStart
  [Called By]
  - >> HAL_PCD_IRQHandler
  - >> PCD_EP_OutXfrComplete_int
  - >> PCD_EP_OutSetupPacket_int
  - >> HAL_PCD_EP_SetStall

  USB_EPClearStall (Thumb, 142 bytes, Stack size 12 bytes, stm32f4xx_ll_usb.o(i.USB_EPClearStall))
  [Stack]

  - Max Depth = 12
  - Call Chain = USB_EPClearStall
  [Called By]
  - >> HAL_PCD_EP_ClrStall

  USB_EPSetStall (Thumb, 154 bytes, Stack size 12 bytes, stm32f4xx_ll_usb.o(i.USB_EPSetStall))
  [Stack]

  - Max Depth = 12
  - Call Chain = USB_EPSetStall
  [Called By]
  - >> HAL_PCD_EP_SetStall

  USB_EPStartXfer (Thumb, 832 bytes, Stack size 32 bytes, stm32f4xx_ll_usb.o(i.USB_EPStartXfer))
  [Stack]

  - Max Depth = 60
  - Call Chain = USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USB_WritePacket
  [Called By]
  - >> HAL_PCD_EP_Transmit
  - >> HAL_PCD_EP_Receive

  USB_EnableGlobalInt (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_ll_usb.o(i.USB_EnableGlobalInt))
  [Called By]

  - >> HAL_PCD_Start

  USB_FlushRxFifo (Thumb, 44 bytes, Stack size 8 bytes, stm32f4xx_ll_usb.o(i.USB_FlushRxFifo))
  [Stack]

  - Max Depth = 8
  - Call Chain = USB_FlushRxFifo
  [Called By]
  - >> USB_DevInit
  - >> HAL_PCD_EP_Flush

  USB_FlushTxFifo (Thumb, 48 bytes, Stack size 8 bytes, stm32f4xx_ll_usb.o(i.USB_FlushTxFifo))
  [Stack]

  - Max Depth = 8
  - Call Chain = USB_FlushTxFifo
  [Called By]
  - >> HAL_PCD_IRQHandler
  - >> USB_DevInit
  - >> HAL_PCD_EP_Flush

  USB_GetDevSpeed (Thumb, 38 bytes, Stack size 8 bytes, stm32f4xx_ll_usb.o(i.USB_GetDevSpeed))
  [Stack]

  - Max Depth = 8
  - Call Chain = USB_GetDevSpeed
  [Called By]
  - >> HAL_PCD_IRQHandler

  USB_GetMode (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_ll_usb.o(i.USB_GetMode))
  [Called By]

  - >> HAL_PCD_IRQHandler
  - >> USB_SetCurrentMode

  USB_ReadDevAllInEpInterrupt (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_ll_usb.o(i.USB_ReadDevAllInEpInterrupt))
  [Called By]

  - >> HAL_PCD_IRQHandler

  USB_ReadDevAllOutEpInterrupt (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_ll_usb.o(i.USB_ReadDevAllOutEpInterrupt))
  [Called By]

  - >> HAL_PCD_IRQHandler

  USB_ReadDevInEPInterrupt (Thumb, 50 bytes, Stack size 16 bytes, stm32f4xx_ll_usb.o(i.USB_ReadDevInEPInterrupt))
  [Stack]

  - Max Depth = 16
  - Call Chain = USB_ReadDevInEPInterrupt
  [Called By]
  - >> HAL_PCD_IRQHandler

  USB_ReadDevOutEPInterrupt (Thumb, 26 bytes, Stack size 8 bytes, stm32f4xx_ll_usb.o(i.USB_ReadDevOutEPInterrupt))
  [Stack]

  - Max Depth = 8
  - Call Chain = USB_ReadDevOutEPInterrupt
  [Called By]
  - >> HAL_PCD_IRQHandler

  USB_ReadInterrupts (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_ll_usb.o(i.USB_ReadInterrupts))
  [Called By]

  - >> HAL_PCD_IRQHandler

  USB_ReadPacket (Thumb, 96 bytes, Stack size 24 bytes, stm32f4xx_ll_usb.o(i.USB_ReadPacket))
  [Stack]

  - Max Depth = 24
  - Call Chain = USB_ReadPacket
  [Called By]
  - >> HAL_PCD_IRQHandler

  USB_SetCurrentMode (Thumb, 104 bytes, Stack size 16 bytes, stm32f4xx_ll_usb.o(i.USB_SetCurrentMode))
  [Stack]

  - Max Depth = 32
  - Call Chain = USB_SetCurrentMode ⇒ HAL_Delay
  [Calls]
  - >> HAL_Delay
  - >> USB_GetMode
  [Called By]
  - >> HAL_PCD_Init

  USB_SetDevAddress (Thumb, 42 bytes, Stack size 8 bytes, stm32f4xx_ll_usb.o(i.USB_SetDevAddress))
  [Stack]

  - Max Depth = 8
  - Call Chain = USB_SetDevAddress
  [Called By]
  - >> HAL_PCD_SetAddress

  USB_SetDevSpeed (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_ll_usb.o(i.USB_SetDevSpeed))
  [Called By]

  - >> USB_DevInit

  USB_SetTurnaroundTime (Thumb, 192 bytes, Stack size 12 bytes, stm32f4xx_ll_usb.o(i.USB_SetTurnaroundTime))
  [Stack]

  - Max Depth = 12
  - Call Chain = USB_SetTurnaroundTime
  [Called By]
  - >> HAL_PCD_IRQHandler

  USB_WritePacket (Thumb, 68 bytes, Stack size 28 bytes, stm32f4xx_ll_usb.o(i.USB_WritePacket))
  [Stack]

  - Max Depth = 28
  - Call Chain = USB_WritePacket
  [Called By]
  - >> USB_EPStartXfer
  - >> PCD_WriteEmptyTxFifo

  USER_initialize (Thumb, 20 bytes, Stack size 8 bytes, user_diskio_1.o(i.USER_initialize))
  [Stack]

  - Max Depth = 160
  - Call Chain = USER_initialize ⇒ USER_status ⇒ W25Q64_ReadID ⇒ MySPI_SwapByte ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> USER_status
  [Address Reference Count : 1]
  - user_diskio_1.o(.data)

  USER_ioctl (Thumb, 54 bytes, Stack size 8 bytes, user_diskio_1.o(i.USER_ioctl))
  [Stack]

  - Max Depth = 8
  - Call Chain = USER_ioctl
  [Address Reference Count : 1]
  - user_diskio_1.o(.data)

  USER_read (Thumb, 34 bytes, Stack size 32 bytes, user_diskio_1.o(i.USER_read))
  [Stack]

  - Max Depth = 192
  - Call Chain = USER_read ⇒ W25Q64_Read ⇒ MySPI_SwapByte ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> W25Q64_Read
  [Address Reference Count : 1]
  - user_diskio_1.o(.data)

  USER_status (Thumb, 34 bytes, Stack size 8 bytes, user_diskio_1.o(i.USER_status))
  [Stack]

  - Max Depth = 152
  - Call Chain = USER_status ⇒ W25Q64_ReadID ⇒ MySPI_SwapByte ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> W25Q64_ReadID
  [Called By]
  - >> USER_initialize
  [Address Reference Count : 1]
  - user_diskio_1.o(.data)

  USER_write (Thumb, 36 bytes, Stack size 32 bytes, user_diskio_1.o(i.USER_write))
  [Stack]

  - Max Depth = 264
  - Call Chain = USER_write ⇒ W25Q64_Write ⇒ W25Q64_Write_NoCheck ⇒ W25Q64_PageProgram ⇒ W25Q64_WriteEnable ⇒ MySPI_SwapByte ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> W25Q64_Write
  [Address Reference Count : 1]
  - user_diskio_1.o(.data)

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.UsageFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f407xx.o(RESET)

  W25Q64_Init (Thumb, 8 bytes, Stack size 8 bytes, w25q64.o(i.W25Q64_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = W25Q64_Init ⇒ MySPI_Init
  [Calls]
  - >> MySPI_Init
  [Called By]
  - >> main
  - >> STORAGE_Init_FS

  W25Q64_PageProgram (Thumb, 76 bytes, Stack size 24 bytes, w25q64.o(i.W25Q64_PageProgram))
  [Stack]

  - Max Depth = 168
  - Call Chain = W25Q64_PageProgram ⇒ W25Q64_WriteEnable ⇒ MySPI_SwapByte ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> W25Q64_WriteEnable
  - >> W25Q64_WaitBusy
  - >> MySPI_SwapByte
  - >> MySPI_Stop
  - >> MySPI_Start
  [Called By]
  - >> W25Q64_Write_NoCheck

  W25Q64_Read (Thumb, 70 bytes, Stack size 24 bytes, w25q64.o(i.W25Q64_Read))
  [Stack]

  - Max Depth = 160
  - Call Chain = W25Q64_Read ⇒ MySPI_SwapByte ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> MySPI_SwapByte
  - >> MySPI_Stop
  - >> MySPI_Start
  [Called By]
  - >> W25Q64_Write
  - >> STORAGE_Read_FS
  - >> USER_read

  W25Q64_ReadID (Thumb, 48 bytes, Stack size 8 bytes, w25q64.o(i.W25Q64_ReadID))
  [Stack]

  - Max Depth = 144
  - Call Chain = W25Q64_ReadID ⇒ MySPI_SwapByte ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> MySPI_SwapByte
  - >> MySPI_Stop
  - >> MySPI_Start
  [Called By]
  - >> USER_status

  W25Q64_SectorErase (Thumb, 52 bytes, Stack size 8 bytes, w25q64.o(i.W25Q64_SectorErase))
  [Stack]

  - Max Depth = 152
  - Call Chain = W25Q64_SectorErase ⇒ W25Q64_WriteEnable ⇒ MySPI_SwapByte ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> W25Q64_WriteEnable
  - >> W25Q64_WaitBusy
  - >> MySPI_SwapByte
  - >> MySPI_Stop
  - >> MySPI_Start
  [Called By]
  - >> W25Q64_Write

  W25Q64_WaitBusy (Thumb, 44 bytes, Stack size 8 bytes, w25q64.o(i.W25Q64_WaitBusy))
  [Stack]

  - Max Depth = 144
  - Call Chain = W25Q64_WaitBusy ⇒ MySPI_SwapByte ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> MySPI_SwapByte
  - >> MySPI_Stop
  - >> MySPI_Start
  [Called By]
  - >> W25Q64_SectorErase
  - >> W25Q64_PageProgram

  W25Q64_Write (Thumb, 180 bytes, Stack size 40 bytes, w25q64.o(i.W25Q64_Write))
  [Stack]

  - Max Depth = 232
  - Call Chain = W25Q64_Write ⇒ W25Q64_Write_NoCheck ⇒ W25Q64_PageProgram ⇒ W25Q64_WriteEnable ⇒ MySPI_SwapByte ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> W25Q64_Read
  - >> W25Q64_Write_NoCheck
  - >> W25Q64_SectorErase
  [Called By]
  - >> STORAGE_Write_FS
  - >> USER_write

  W25Q64_WriteEnable (Thumb, 18 bytes, Stack size 8 bytes, w25q64.o(i.W25Q64_WriteEnable))
  [Stack]

  - Max Depth = 144
  - Call Chain = W25Q64_WriteEnable ⇒ MySPI_SwapByte ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> MySPI_SwapByte
  - >> MySPI_Stop
  - >> MySPI_Start
  [Called By]
  - >> W25Q64_SectorErase
  - >> W25Q64_PageProgram

  W25Q64_Write_NoCheck (Thumb, 70 bytes, Stack size 24 bytes, w25q64.o(i.W25Q64_Write_NoCheck))
  [Stack]

  - Max Depth = 192
  - Call Chain = W25Q64_Write_NoCheck ⇒ W25Q64_PageProgram ⇒ W25Q64_WriteEnable ⇒ MySPI_SwapByte ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> W25Q64_PageProgram
  [Called By]
  - >> W25Q64_Write

  IsPixelBad(unsigned short, paramsMLX90640*) (Thumb, 50 bytes, Stack size 0 bytes, mlx90640_api.o(i._Z10IsPixelBadtP14paramsMLX90640))
  [Called By]

  - >> MLX90640_BadPixelsCorrection

  CheckAdjacentPixels(unsigned short, unsigned short) (Thumb, 58 bytes, Stack size 0 bytes, mlx90640_api.o(i._Z19CheckAdjacentPixelstt))
  [Called By]

  - >> ExtractDeviatingPixels(unsigned short*, paramsMLX90640*)

  ExtractCPParameters(unsigned short*, paramsMLX90640*) (Thumb, 494 bytes, Stack size 80 bytes, mlx90640_api.o(i._Z19ExtractCPParametersPtP14paramsMLX90640))
  [Stack]

  - Max Depth = 304
  - Call Chain = ExtractCPParameters(unsigned short*, paramsMLX90640*) ⇒ pow ⇒ __kernel_poly ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_f2d
  - >> __aeabi_d2f
  - >> __aeabi_ui2d
  - >> __aeabi_i2f
  - >> __aeabi_fsub
  - >> __aeabi_fmul
  - >> __aeabi_fdiv
  - >> __aeabi_fadd
  - >> __aeabi_ddiv
  - >> __aeabi_cfrcmple
  - >> pow
  [Called By]
  - >> MLX90640_ExtractParameters

  ExtractTgcParameters(unsigned short*, paramsMLX90640*) (Thumb, 54 bytes, Stack size 16 bytes, mlx90640_api.o(i._Z20ExtractTgcParametersPtP14paramsMLX90640))
  [Stack]

  - Max Depth = 36
  - Call Chain = ExtractTgcParameters(unsigned short*, paramsMLX90640*) ⇒ __aeabi_fsub ⇒ __aeabi_fadd ⇒ _float_epilogue
  [Calls]
  - >> __aeabi_i2f
  - >> __aeabi_fsub
  - >> __aeabi_fdiv
  - >> __aeabi_cfrcmple
  [Called By]
  - >> MLX90640_ExtractParameters

  ExtractVDDParameters(unsigned short*, paramsMLX90640*) (Thumb, 52 bytes, Stack size 12 bytes, mlx90640_api.o(i._Z20ExtractVDDParametersPtP14paramsMLX90640))
  [Stack]

  - Max Depth = 12
  - Call Chain = ExtractVDDParameters(unsigned short*, paramsMLX90640*)
  [Called By]
  - >> MLX90640_ExtractParameters

  ExtractCILCParameters(unsigned short*, paramsMLX90640*) (Thumb, 194 bytes, Stack size 32 bytes, mlx90640_api.o(i._Z21ExtractCILCParametersPtP14paramsMLX90640))
  [Stack]

  - Max Depth = 52
  - Call Chain = ExtractCILCParameters(unsigned short*, paramsMLX90640*) ⇒ __aeabi_fsub ⇒ __aeabi_fadd ⇒ _float_epilogue
  [Calls]
  - >> __aeabi_i2f
  - >> __aeabi_fsub
  - >> __aeabi_fdiv
  - >> __aeabi_cfrcmple
  [Called By]
  - >> MLX90640_ExtractParameters

  ExtractGainParameters(unsigned short*, paramsMLX90640*) (Thumb, 20 bytes, Stack size 0 bytes, mlx90640_api.o(i._Z21ExtractGainParametersPtP14paramsMLX90640))
  [Called By]

  - >> MLX90640_ExtractParameters

  ExtractKsTaParameters(unsigned short*, paramsMLX90640*) (Thumb, 56 bytes, Stack size 16 bytes, mlx90640_api.o(i._Z21ExtractKsTaParametersPtP14paramsMLX90640))
  [Stack]

  - Max Depth = 36
  - Call Chain = ExtractKsTaParameters(unsigned short*, paramsMLX90640*) ⇒ __aeabi_fsub ⇒ __aeabi_fadd ⇒ _float_epilogue
  [Calls]
  - >> __aeabi_i2f
  - >> __aeabi_fsub
  - >> __aeabi_fdiv
  - >> __aeabi_cfrcmple
  [Called By]
  - >> MLX90640_ExtractParameters

  ExtractKsToParameters(unsigned short*, paramsMLX90640*) (Thumb, 240 bytes, Stack size 32 bytes, mlx90640_api.o(i._Z21ExtractKsToParametersPtP14paramsMLX90640))
  [Stack]

  - Max Depth = 52
  - Call Chain = ExtractKsToParameters(unsigned short*, paramsMLX90640*) ⇒ __aeabi_fsub ⇒ __aeabi_fadd ⇒ _float_epilogue
  [Calls]
  - >> __aeabi_i2f
  - >> __aeabi_fsub
  - >> __aeabi_fdiv
  - >> __aeabi_cfrcmple
  [Called By]
  - >> MLX90640_ExtractParameters

  ExtractPTATParameters(unsigned short*, paramsMLX90640*) (Thumb, 194 bytes, Stack size 64 bytes, mlx90640_api.o(i._Z21ExtractPTATParametersPtP14paramsMLX90640))
  [Stack]

  - Max Depth = 288
  - Call Chain = ExtractPTATParameters(unsigned short*, paramsMLX90640*) ⇒ pow ⇒ __kernel_poly ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_d2f
  - >> __aeabi_i2f
  - >> __aeabi_i2d
  - >> __aeabi_fsub
  - >> __aeabi_fdiv
  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> __aeabi_cfrcmple
  - >> pow
  [Called By]
  - >> MLX90640_ExtractParameters

  ExtractAlphaParameters(unsigned short*, paramsMLX90640*) (Thumb, 826 bytes, Stack size 3384 bytes, mlx90640_api.o(i._Z22ExtractAlphaParametersPtP14paramsMLX90640))
  [Stack]

  - Max Depth = 3608
  - Call Chain = ExtractAlphaParameters(unsigned short*, paramsMLX90640*) ⇒ pow ⇒ __kernel_poly ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_f2d
  - >> __aeabi_d2f
  - >> __aeabi_ui2d
  - >> __aeabi_dmul
  - >> __aeabi_i2f
  - >> __aeabi_fsub
  - >> __aeabi_frsub
  - >> __aeabi_fmul
  - >> __aeabi_fdiv
  - >> __aeabi_fadd
  - >> __aeabi_f2uiz
  - >> __aeabi_ddiv
  - >> __aeabi_cfrcmple
  - >> __aeabi_cfcmple
  - >> pow
  [Called By]
  - >> MLX90640_ExtractParameters

  ExtractDeviatingPixels(unsigned short*, paramsMLX90640*) (Thumb, 350 bytes, Stack size 32 bytes, mlx90640_api.o(i._Z22ExtractDeviatingPixelsPtP14paramsMLX90640))
  [Stack]

  - Max Depth = 32
  - Call Chain = ExtractDeviatingPixels(unsigned short*, paramsMLX90640*)
  [Calls]
  - >> CheckAdjacentPixels(unsigned short, unsigned short)
  [Called By]
  - >> MLX90640_ExtractParameters

  ExtractOffsetParameters(unsigned short*, paramsMLX90640*) (Thumb, 448 bytes, Stack size 252 bytes, mlx90640_api.o(i._Z23ExtractOffsetParametersPtP14paramsMLX90640))
  [Stack]

  - Max Depth = 252
  - Call Chain = ExtractOffsetParameters(unsigned short*, paramsMLX90640*)
  [Called By]
  - >> MLX90640_ExtractParameters

  ExtractKvPixelParameters(unsigned short*, paramsMLX90640*) (Thumb, 566 bytes, Stack size 3160 bytes, mlx90640_api.o(i._Z24ExtractKvPixelParametersPtP14paramsMLX90640))
  [Stack]

  - Max Depth = 3384
  - Call Chain = ExtractKvPixelParameters(unsigned short*, paramsMLX90640*) ⇒ pow ⇒ __kernel_poly ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_f2d
  - >> __aeabi_d2f
  - >> __aeabi_ui2d
  - >> __aeabi_dmul
  - >> __aeabi_i2f
  - >> __aeabi_fsub
  - >> __aeabi_fmul
  - >> __aeabi_fadd
  - >> __aeabi_f2iz
  - >> __aeabi_ddiv
  - >> __aeabi_cfrcmple
  - >> __aeabi_cfcmple
  - >> std::fabs(float)
  - >> pow
  [Called By]
  - >> MLX90640_ExtractParameters

  ExtractKtaPixelParameters(unsigned short*, paramsMLX90640*) (Thumb, 670 bytes, Stack size 3168 bytes, mlx90640_api.o(i._Z25ExtractKtaPixelParametersPtP14paramsMLX90640))
  [Stack]

  - Max Depth = 3392
  - Call Chain = ExtractKtaPixelParameters(unsigned short*, paramsMLX90640*) ⇒ pow ⇒ __kernel_poly ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_f2d
  - >> __aeabi_d2f
  - >> __aeabi_ui2d
  - >> __aeabi_dmul
  - >> __aeabi_i2f
  - >> __aeabi_fsub
  - >> __aeabi_fmul
  - >> __aeabi_fadd
  - >> __aeabi_f2iz
  - >> __aeabi_ddiv
  - >> __aeabi_cfrcmple
  - >> __aeabi_cfcmple
  - >> std::fabs(float)
  - >> pow
  [Called By]
  - >> MLX90640_ExtractParameters

  ExtractResolutionParameters(unsigned short*, paramsMLX90640*) (Thumb, 14 bytes, Stack size 0 bytes, mlx90640_api.o(i._Z27ExtractResolutionParametersPtP14paramsMLX90640))
  [Called By]

  - >> MLX90640_ExtractParameters

  GetMedian(float*, int) (Thumb, 132 bytes, Stack size 32 bytes, mlx90640_api.o(i._Z9GetMedianPfi))
  [Stack]

  - Max Depth = 52
  - Call Chain = GetMedian(float*, int) ⇒ __aeabi_fadd ⇒ _float_epilogue
  [Calls]
  - >> __aeabi_fdiv
  - >> __aeabi_fadd
  - >> __aeabi_cfcmple
  [Called By]
  - >> MLX90640_BadPixelsCorrection

  std::fabs(float) (Thumb, 8 bytes, Stack size 0 bytes, mlx90640_api.o(i._ZSt4fabsf))
  [Called By]

  - >> MLX90640_BadPixelsCorrection
  - >> ExtractKtaPixelParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractKvPixelParameters(unsigned short*, paramsMLX90640*)

  std::sqrt(float) (Thumb, 12 bytes, Stack size 8 bytes, mlx90640_api.o(i._ZSt4sqrtf))
  [Stack]

  - Max Depth = 40
  - Call Chain = std::sqrt(float) ⇒ sqrtf ⇒ _fsqrt
  [Calls]
  - >> sqrtf
  [Called By]
  - >> MLX90640_CalculateTo

  __0printf (Thumb, 22 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)
  [Calls]

  - >> _printf_core

  __1printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)

  __2printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2printf
  [Called By]
  - >> main
  - >> SaveScreenBMP
  - >> HAL_GPIO_EXTI_Callback

  __c89printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)

  printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)

  __0sprintf (Thumb, 34 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)
  [Calls]

  - >> _sputc
  - >> _printf_core

  __1sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)

  __2sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2sprintf
  [Called By]
  - >> Disp_TempPic
  - >> SaveScreenBMP

  __c89sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)

  sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)

  __ARM_fpclassify (Thumb, 40 bytes, Stack size 0 bytes, fpclassify.o(i.__ARM_fpclassify))
  [Called By]

  - >> pow

  __kernel_poly (Thumb, 170 bytes, Stack size 24 bytes, poly.o(i.__kernel_poly))
  [Stack]

  - Max Depth = 112
  - Call Chain = __kernel_poly ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_dmul
  - >> __aeabi_dadd
  [Called By]
  - >> pow

  __mathlib_dbl_divzero (Thumb, 12 bytes, Stack size 0 bytes, dunder.o(i.__mathlib_dbl_divzero))
  [Stack]

  - Max Depth = 40
  - Call Chain = __mathlib_dbl_divzero ⇒ __aeabi_ddiv ⇒ _double_round
  [Calls]
  - >> __aeabi_ddiv
  [Called By]
  - >> pow

  __mathlib_dbl_infnan2 (Thumb, 4 bytes, Stack size 0 bytes, dunder.o(i.__mathlib_dbl_infnan2))
  [Stack]

  - Max Depth = 88
  - Call Chain = __mathlib_dbl_infnan2 ⇒ __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_dadd
  [Called By]
  - >> pow

  __mathlib_dbl_invalid (Thumb, 12 bytes, Stack size 0 bytes, dunder.o(i.__mathlib_dbl_invalid))
  [Stack]

  - Max Depth = 40
  - Call Chain = __mathlib_dbl_invalid ⇒ __aeabi_ddiv ⇒ _double_round
  [Calls]
  - >> __aeabi_ddiv
  [Called By]
  - >> pow

  __mathlib_dbl_overflow (Thumb, 14 bytes, Stack size 0 bytes, dunder.o(i.__mathlib_dbl_overflow))
  [Stack]

  - Max Depth = 16
  - Call Chain = __mathlib_dbl_overflow ⇒ __ARM_scalbn
  [Calls]
  - >> __ARM_scalbn
  [Called By]
  - >> pow

  __mathlib_dbl_underflow (Thumb, 10 bytes, Stack size 0 bytes, dunder.o(i.__mathlib_dbl_underflow))
  [Stack]

  - Max Depth = 16
  - Call Chain = __mathlib_dbl_underflow ⇒ __ARM_scalbn
  [Calls]
  - >> __ARM_scalbn
  [Called By]
  - >> pow

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  __set_errno (Thumb, 6 bytes, Stack size 0 bytes, errno.o(i.__set_errno))
  [Called By]

  - >> sqrtf
  - >> pow
  - >> sqrt

  disk_initialize (Thumb, 40 bytes, Stack size 16 bytes, diskio.o(i.disk_initialize))
  [Stack]

  - Max Depth = 16
  - Call Chain = disk_initialize
  [Called By]
  - >> f_mkfs
  - >> find_volume

  disk_ioctl (Thumb, 36 bytes, Stack size 24 bytes, diskio.o(i.disk_ioctl))
  [Stack]

  - Max Depth = 24
  - Call Chain = disk_ioctl
  [Called By]
  - >> f_mkfs
  - >> sync_fs

  disk_read (Thumb, 42 bytes, Stack size 24 bytes, diskio.o(i.disk_read))
  [Stack]

  - Max Depth = 24
  - Call Chain = disk_read
  [Called By]
  - >> f_write
  - >> f_read
  - >> f_open
  - >> move_window

  disk_status (Thumb, 24 bytes, Stack size 16 bytes, diskio.o(i.disk_status))
  [Stack]

  - Max Depth = 16
  - Call Chain = disk_status
  [Called By]
  - >> validate
  - >> find_volume

  disk_write (Thumb, 42 bytes, Stack size 24 bytes, diskio.o(i.disk_write))
  [Stack]

  - Max Depth = 24
  - Call Chain = disk_write
  [Called By]
  - >> f_write
  - >> f_sync
  - >> f_read
  - >> f_mkfs
  - >> sync_window
  - >> sync_fs

  f_close (Thumb, 44 bytes, Stack size 16 bytes, ff.o(i.f_close))
  [Stack]

  - Max Depth = 104
  - Call Chain = f_close ⇒ f_sync ⇒ sync_fs ⇒ sync_window ⇒ disk_write
  [Calls]
  - >> f_sync
  - >> dec_lock
  - >> validate
  [Called By]
  - >> main
  - >> SaveScreenBMP

  f_mkfs (Thumb, 1654 bytes, Stack size 136 bytes, ff.o(i.f_mkfs))
  [Stack]

  - Max Depth = 160
  - Call Chain = f_mkfs ⇒ disk_write
  [Calls]
  - >> disk_write
  - >> disk_ioctl
  - >> disk_initialize
  - >> get_fattime
  - >> st_word
  - >> st_dword
  - >> mem_set
  - >> mem_cpy
  - >> get_ldnumber
  [Called By]
  - >> main

  f_mount (Thumb, 92 bytes, Stack size 40 bytes, ff.o(i.f_mount))
  [Stack]

  - Max Depth = 208
  - Call Chain = f_mount ⇒ find_volume ⇒ check_fs ⇒ move_window ⇒ sync_window ⇒ disk_write
  [Calls]
  - >> clear_lock
  - >> get_ldnumber
  - >> find_volume
  [Called By]
  - >> main

  f_open (Thumb, 560 bytes, Stack size 104 bytes, ff.o(i.f_open))
  [Stack]

  - Max Depth = 320
  - Call Chain = f_open ⇒ follow_path ⇒ dir_find ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write
  [Calls]
  - >> enq_lock
  - >> dir_register
  - >> clust2sect
  - >> chk_lock
  - >> disk_read
  - >> get_fattime
  - >> st_dword
  - >> st_clust
  - >> remove_chain
  - >> move_window
  - >> mem_set
  - >> ld_dword
  - >> ld_clust
  - >> inc_lock
  - >> get_fat
  - >> follow_path
  - >> find_volume
  [Called By]
  - >> main
  - >> SaveScreenBMP

  f_read (Thumb, 428 bytes, Stack size 72 bytes, ff.o(i.f_read))
  [Stack]

  - Max Depth = 168
  - Call Chain = f_read ⇒ get_fat ⇒ move_window ⇒ sync_window ⇒ disk_write
  [Calls]
  - >> clust2sect
  - >> clmt_clust
  - >> disk_write
  - >> disk_read
  - >> validate
  - >> mem_cpy
  - >> get_fat
  [Called By]
  - >> main

  f_sync (Thumb, 160 bytes, Stack size 24 bytes, ff.o(i.f_sync))
  [Stack]

  - Max Depth = 88
  - Call Chain = f_sync ⇒ sync_fs ⇒ sync_window ⇒ disk_write
  [Calls]
  - >> disk_write
  - >> get_fattime
  - >> validate
  - >> sync_fs
  - >> st_word
  - >> st_dword
  - >> st_clust
  - >> move_window
  [Called By]
  - >> f_close
  - >> SaveScreenBMP

  f_write (Thumb, 494 bytes, Stack size 64 bytes, ff.o(i.f_write))
  [Stack]

  - Max Depth = 192
  - Call Chain = f_write ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write
  [Calls]
  - >> create_chain
  - >> clust2sect
  - >> clmt_clust
  - >> disk_write
  - >> disk_read
  - >> validate
  - >> mem_cpy
  [Called By]
  - >> main
  - >> SaveScreenBMP

  fputc (Thumb, 22 bytes, Stack size 16 bytes, usart.o(i.fputc))
  [Stack]

  - Max Depth = 80
  - Call Chain = fputc ⇒ HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_UART_Transmit
  [Address Reference Count : 1]
  - printfa.o(i.__0printf)

  get_fattime (Thumb, 4 bytes, Stack size 0 bytes, fatfs_1.o(i.get_fattime))
  [Called By]

  - >> f_sync
  - >> f_open
  - >> f_mkfs

  lcd_clear (Thumb, 42 bytes, Stack size 16 bytes, lcd.o(i.lcd_clear))
  [Stack]

  - Max Depth = 32
  - Call Chain = lcd_clear ⇒ lcd_set_cursor ⇒ lcd_wr_regno
  [Calls]
  - >> lcd_write_ram_prepare
  - >> lcd_set_cursor
  [Called By]
  - >> lcd_init
  - >> main

  lcd_display_dir (Thumb, 360 bytes, Stack size 8 bytes, lcd.o(i.lcd_display_dir))
  [Stack]

  - Max Depth = 36
  - Call Chain = lcd_display_dir ⇒ lcd_scan_dir ⇒ lcd_wr_regno
  [Calls]
  - >> lcd_scan_dir
  [Called By]
  - >> lcd_init

  lcd_draw_point (Thumb, 26 bytes, Stack size 16 bytes, lcd.o(i.lcd_draw_point))
  [Stack]

  - Max Depth = 32
  - Call Chain = lcd_draw_point ⇒ lcd_set_cursor ⇒ lcd_wr_regno
  [Calls]
  - >> lcd_write_ram_prepare
  - >> lcd_set_cursor
  [Called By]
  - >> lcd_show_char
  - >> DrawValueMarker
  - >> DrawTopRows
  - >> DrawCrosshair
  - >> Draw2x2Block

  lcd_ex_ili9341_reginit (Thumb, 556 bytes, Stack size 8 bytes, lcd.o(i.lcd_ex_ili9341_reginit))
  [Stack]

  - Max Depth = 24
  - Call Chain = lcd_ex_ili9341_reginit ⇒ HAL_Delay
  [Calls]
  - >> HAL_Delay
  - >> lcd_wr_regno
  - >> lcd_wr_data
  [Called By]
  - >> lcd_init

  lcd_ex_ili9806_reginit (Thumb, 832 bytes, Stack size 8 bytes, lcd.o(i.lcd_ex_ili9806_reginit))
  [Stack]

  - Max Depth = 24
  - Call Chain = lcd_ex_ili9806_reginit ⇒ HAL_Delay
  [Calls]
  - >> HAL_Delay
  - >> lcd_wr_regno
  - >> lcd_wr_data
  [Called By]
  - >> lcd_init

  lcd_ex_nt35310_reginit (Thumb, 3826 bytes, Stack size 8 bytes, lcd.o(i.lcd_ex_nt35310_reginit))
  [Stack]

  - Max Depth = 24
  - Call Chain = lcd_ex_nt35310_reginit ⇒ HAL_Delay
  [Calls]
  - >> HAL_Delay
  - >> lcd_wr_regno
  - >> lcd_wr_data
  [Called By]
  - >> lcd_init

  lcd_ex_nt35510_reginit (Thumb, 3950 bytes, Stack size 8 bytes, lcd.o(i.lcd_ex_nt35510_reginit))
  [Stack]

  - Max Depth = 24
  - Call Chain = lcd_ex_nt35510_reginit ⇒ HAL_Delay
  [Calls]
  - >> HAL_Delay
  - >> lcd_write_reg
  - >> lcd_wr_regno
  [Called By]
  - >> lcd_init

  lcd_ex_ssd1963_reginit (Thumb, 360 bytes, Stack size 8 bytes, lcd.o(i.lcd_ex_ssd1963_reginit))
  [Stack]

  - Max Depth = 24
  - Call Chain = lcd_ex_ssd1963_reginit ⇒ HAL_Delay
  [Calls]
  - >> HAL_Delay
  - >> lcd_wr_regno
  - >> lcd_wr_data
  [Called By]
  - >> lcd_init

  lcd_ex_st7789_reginit (Thumb, 424 bytes, Stack size 8 bytes, lcd.o(i.lcd_ex_st7789_reginit))
  [Stack]

  - Max Depth = 24
  - Call Chain = lcd_ex_st7789_reginit ⇒ HAL_Delay
  [Calls]
  - >> HAL_Delay
  - >> lcd_wr_regno
  - >> lcd_wr_data
  [Called By]
  - >> lcd_init

  lcd_ex_st7796_reginit (Thumb, 454 bytes, Stack size 8 bytes, lcd.o(i.lcd_ex_st7796_reginit))
  [Stack]

  - Max Depth = 24
  - Call Chain = lcd_ex_st7796_reginit ⇒ HAL_Delay
  [Calls]
  - >> HAL_Delay
  - >> lcd_wr_regno
  - >> lcd_wr_data
  [Called By]
  - >> lcd_init

  lcd_init (Thumb, 1348 bytes, Stack size 88 bytes, lcd.o(i.lcd_init))
  [Stack]

  - Max Depth = 208
  - Call Chain = lcd_init ⇒ lcd_ssd_backlight_set ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> HAL_SRAM_Init
  - >> HAL_GPIO_WritePin
  - >> HAL_GPIO_Init
  - >> lcd_clear
  - >> HAL_Delay
  - >> lcd_write_reg
  - >> lcd_wr_regno
  - >> lcd_ssd_backlight_set
  - >> lcd_ex_st7796_reginit
  - >> lcd_ex_st7789_reginit
  - >> lcd_ex_ssd1963_reginit
  - >> lcd_ex_nt35510_reginit
  - >> lcd_ex_nt35310_reginit
  - >> lcd_ex_ili9806_reginit
  - >> lcd_ex_ili9341_reginit
  - >> lcd_display_dir
  - >> lcd_rd_data
  - >> FSMC_NORSRAM_Extended_Timing_Init
  [Called By]
  - >> main

  lcd_read_point (Thumb, 148 bytes, Stack size 24 bytes, lcd.o(i.lcd_read_point))
  [Stack]

  - Max Depth = 40
  - Call Chain = lcd_read_point ⇒ lcd_set_cursor ⇒ lcd_wr_regno
  [Calls]
  - >> lcd_wr_regno
  - >> lcd_set_cursor
  - >> lcd_rd_data
  [Called By]
  - >> SaveScreenBMP

  lcd_scan_dir (Thumb, 568 bytes, Stack size 20 bytes, lcd.o(i.lcd_scan_dir))
  [Stack]

  - Max Depth = 28
  - Call Chain = lcd_scan_dir ⇒ lcd_wr_regno
  [Calls]
  - >> lcd_write_reg
  - >> lcd_wr_regno
  - >> lcd_wr_data
  [Called By]
  - >> lcd_display_dir

  lcd_set_cursor (Thumb, 282 bytes, Stack size 8 bytes, lcd.o(i.lcd_set_cursor))
  [Stack]

  - Max Depth = 16
  - Call Chain = lcd_set_cursor ⇒ lcd_wr_regno
  [Calls]
  - >> lcd_wr_regno
  - >> lcd_wr_data
  [Called By]
  - >> lcd_read_point
  - >> lcd_clear
  - >> lcd_draw_point

  lcd_set_window (Thumb, 362 bytes, Stack size 24 bytes, lcd.o(i.lcd_set_window))
  [Stack]

  - Max Depth = 32
  - Call Chain = lcd_set_window ⇒ lcd_wr_regno
  [Calls]
  - >> lcd_wr_regno
  - >> lcd_wr_data
  [Called By]
  - >> Disp_TempPic
  - >> main

  lcd_show_char (Thumb, 294 bytes, Stack size 44 bytes, lcd.o(i.lcd_show_char))
  [Stack]

  - Max Depth = 76
  - Call Chain = lcd_show_char ⇒ lcd_draw_point ⇒ lcd_set_cursor ⇒ lcd_wr_regno
  [Calls]
  - >> lcd_draw_point
  [Called By]
  - >> lcd_show_string
  - >> lcd_show_string_transparent

  lcd_show_string (Thumb, 106 bytes, Stack size 44 bytes, lcd.o(i.lcd_show_string))
  [Stack]

  - Max Depth = 120
  - Call Chain = lcd_show_string ⇒ lcd_show_char ⇒ lcd_draw_point ⇒ lcd_set_cursor ⇒ lcd_wr_regno
  [Calls]
  - >> lcd_show_char
  [Called By]
  - >> main

  lcd_ssd_backlight_set (Thumb, 80 bytes, Stack size 32 bytes, lcd.o(i.lcd_ssd_backlight_set))
  [Stack]

  - Max Depth = 120
  - Call Chain = lcd_ssd_backlight_set ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_ui2d
  - >> __aeabi_dmul
  - >> __aeabi_d2uiz
  - >> lcd_wr_regno
  - >> lcd_wr_data
  [Called By]
  - >> lcd_init

  lcd_wr_data (Thumb, 18 bytes, Stack size 8 bytes, lcd.o(i.lcd_wr_data))
  [Stack]

  - Max Depth = 8
  - Call Chain = lcd_wr_data
  [Called By]
  - >> lcd_set_window
  - >> lcd_ssd_backlight_set
  - >> lcd_set_cursor
  - >> lcd_scan_dir
  - >> lcd_ex_st7796_reginit
  - >> lcd_ex_st7789_reginit
  - >> lcd_ex_ssd1963_reginit
  - >> lcd_ex_nt35310_reginit
  - >> lcd_ex_ili9806_reginit
  - >> lcd_ex_ili9341_reginit

  lcd_wr_regno (Thumb, 18 bytes, Stack size 8 bytes, lcd.o(i.lcd_wr_regno))
  [Stack]

  - Max Depth = 8
  - Call Chain = lcd_wr_regno
  [Called By]
  - >> lcd_set_window
  - >> lcd_read_point
  - >> lcd_init
  - >> lcd_ssd_backlight_set
  - >> lcd_set_cursor
  - >> lcd_scan_dir
  - >> lcd_ex_st7796_reginit
  - >> lcd_ex_st7789_reginit
  - >> lcd_ex_ssd1963_reginit
  - >> lcd_ex_nt35510_reginit
  - >> lcd_ex_nt35310_reginit
  - >> lcd_ex_ili9806_reginit
  - >> lcd_ex_ili9341_reginit

  lcd_write_ram_prepare (Thumb, 10 bytes, Stack size 0 bytes, lcd.o(i.lcd_write_ram_prepare))
  [Called By]

  - >> lcd_clear
  - >> lcd_draw_point

  lcd_write_reg (Thumb, 14 bytes, Stack size 0 bytes, lcd.o(i.lcd_write_reg))
  [Called By]

  - >> lcd_init
  - >> lcd_scan_dir
  - >> lcd_ex_nt35510_reginit

  led_init (Thumb, 80 bytes, Stack size 32 bytes, gpio.o(i.led_init))
  [Stack]

  - Max Depth = 56
  - Call Chain = led_init ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> HAL_GPIO_Init
  [Called By]
  - >> main

  main (Thumb, 868 bytes, Stack size 8448 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 14568
  - Call Chain = main ⇒ SaveScreenBMP ⇒ f_open ⇒ follow_path ⇒ dir_find ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write
  [Calls]
  - >> led_init
  - >> lcd_show_string
  - >> lcd_set_window
  - >> lcd_init
  - >> lcd_clear
  - >> f_write
  - >> f_read
  - >> f_open
  - >> f_mount
  - >> f_mkfs
  - >> f_close
  - >> __aeabi_f2d
  - >> __aeabi_dsub
  - >> __aeabi_d2f
  - >> W25Q64_Init
  - >> MX_USB_DEVICE_Init
  - >> MX_USART6_UART_Init
  - >> MX_SPI3_Init
  - >> MX_I2C2_Init
  - >> MX_GPIO_Init
  - >> MX_FSMC_Init
  - >> MX_FATFS_Init
  - >> MX_ADC1_Init
  - >> MLX90640_SetRefreshRate
  - >> MLX90640_SetChessMode
  - >> MLX90640_I2CInit
  - >> MLX90640_GetVdd
  - >> MLX90640_GetTa
  - >> MLX90640_GetRefreshRate
  - >> MLX90640_GetFrameData
  - >> MLX90640_ExtractParameters
  - >> MLX90640_DumpEE
  - >> MLX90640_CalculateTo
  - >> MLX90640_BadPixelsCorrection
  - >> HAL_Init
  - >> HAL_GPIO_TogglePin
  - >> HAL_Delay
  - >> Disp_TempPic
  - >> SystemClock_Config
  - >> SaveScreenBMP
  - >> strlen
  - >> __aeabi_memclr4
  - >> __aeabi_memcpy4
  - >> __2printf
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  pow (Thumb, 2478 bytes, Stack size 112 bytes, pow.o(i.pow))
  [Stack]

  - Max Depth = 224
  - Call Chain = pow ⇒ __kernel_poly ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_dsub
  - >> __aeabi_dmul
  - >> __aeabi_i2d
  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> __aeabi_drsub
  - >> __aeabi_cdrcmple
  - >> __ARM_scalbn
  - >> __set_errno
  - >> sqrt
  - >> __kernel_poly
  - >> __ARM_fpclassify
  - >> __mathlib_dbl_underflow
  - >> __mathlib_dbl_overflow
  - >> __mathlib_dbl_invalid
  - >> __mathlib_dbl_infnan2
  - >> __mathlib_dbl_divzero
  [Called By]
  - >> MLX90640_GetVdd
  - >> MLX90640_GetTa
  - >> MLX90640_CalculateTo
  - >> ExtractKtaPixelParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractKvPixelParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractAlphaParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractPTATParameters(unsigned short*, paramsMLX90640*)
  - >> ExtractCPParameters(unsigned short*, paramsMLX90640*)

  sqrt (Thumb, 76 bytes, Stack size 24 bytes, sqrt.o(i.sqrt))
  [Stack]

  - Max Depth = 64
  - Call Chain = sqrt ⇒ _dsqrt ⇒ _double_round
  [Calls]
  - >> __set_errno
  - >> _dsqrt
  [Called By]
  - >> pow

  sqrtf (Thumb, 44 bytes, Stack size 16 bytes, sqrtf.o(i.sqrtf))
  [Stack]

  - Max Depth = 32
  - Call Chain = sqrtf ⇒ _fsqrt
  [Calls]
  - >> _fsqrt
  - >> __set_errno
  [Called By]
  - >> std::sqrt(float)

  ### Local Symbols

  HAL_FSMC_MspInit (Thumb, 182 bytes, Stack size 32 bytes, fsmc.o(i.HAL_FSMC_MspInit))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_FSMC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  - >> __aeabi_memclr4
  [Called By]
  - >> HAL_SRAM_MspInit

  Get_SerialNum (Thumb, 42 bytes, Stack size 16 bytes, usbd_desc.o(i.Get_SerialNum))
  [Stack]

  - Max Depth = 28
  - Call Chain = Get_SerialNum ⇒ IntToUnicode
  [Calls]
  - >> IntToUnicode
  [Called By]
  - >> USBD_FS_SerialStrDescriptor

  IntToUnicode (Thumb, 62 bytes, Stack size 12 bytes, usbd_desc.o(i.IntToUnicode))
  [Stack]

  - Max Depth = 12
  - Call Chain = IntToUnicode
  [Called By]
  - >> Get_SerialNum

  STORAGE_GetCapacity_FS (Thumb, 16 bytes, Stack size 0 bytes, usbd_storage_if.o(i.STORAGE_GetCapacity_FS))
  [Address Reference Count : 1]

  - usbd_storage_if.o(.data)

  STORAGE_GetMaxLun_FS (Thumb, 4 bytes, Stack size 0 bytes, usbd_storage_if.o(i.STORAGE_GetMaxLun_FS))
  [Address Reference Count : 1]

  - usbd_storage_if.o(.data)

  STORAGE_Init_FS (Thumb, 12 bytes, Stack size 8 bytes, usbd_storage_if.o(i.STORAGE_Init_FS))
  [Stack]

  - Max Depth = 24
  - Call Chain = STORAGE_Init_FS ⇒ W25Q64_Init ⇒ MySPI_Init
  [Calls]
  - >> W25Q64_Init
  [Address Reference Count : 1]
  - usbd_storage_if.o(.data)

  STORAGE_IsReady_FS (Thumb, 6 bytes, Stack size 0 bytes, usbd_storage_if.o(i.STORAGE_IsReady_FS))
  [Address Reference Count : 1]

  - usbd_storage_if.o(.data)

  STORAGE_IsWriteProtected_FS (Thumb, 6 bytes, Stack size 0 bytes, usbd_storage_if.o(i.STORAGE_IsWriteProtected_FS))
  [Address Reference Count : 1]

  - usbd_storage_if.o(.data)

  STORAGE_Read_FS (Thumb, 38 bytes, Stack size 24 bytes, usbd_storage_if.o(i.STORAGE_Read_FS))
  [Stack]

  - Max Depth = 184
  - Call Chain = STORAGE_Read_FS ⇒ W25Q64_Read ⇒ MySPI_SwapByte ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> W25Q64_Read
  [Address Reference Count : 1]
  - usbd_storage_if.o(.data)

  STORAGE_Write_FS (Thumb, 44 bytes, Stack size 24 bytes, usbd_storage_if.o(i.STORAGE_Write_FS))
  [Stack]

  - Max Depth = 256
  - Call Chain = STORAGE_Write_FS ⇒ W25Q64_Write ⇒ W25Q64_Write_NoCheck ⇒ W25Q64_PageProgram ⇒ W25Q64_WriteEnable ⇒ MySPI_SwapByte ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> W25Q64_Write
  [Address Reference Count : 1]
  - usbd_storage_if.o(.data)

  PCD_EP_OutSetupPacket_int (Thumb, 94 bytes, Stack size 32 bytes, stm32f4xx_hal_pcd.o(i.PCD_EP_OutSetupPacket_int))
  [Stack]

  - Max Depth = 228
  - Call Chain = PCD_EP_OutSetupPacket_int ⇒ HAL_PCD_SetupStageCallback ⇒ USBD_LL_SetupStage ⇒ USBD_StdDevReq ⇒ USBD_GetDescriptor ⇒ USBD_CtlSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USB_EP0_OutStart
  - >> HAL_PCD_SetupStageCallback
  [Called By]
  - >> HAL_PCD_IRQHandler

  PCD_EP_OutXfrComplete_int (Thumb, 372 bytes, Stack size 32 bytes, stm32f4xx_hal_pcd.o(i.PCD_EP_OutXfrComplete_int))
  [Stack]

  - Max Depth = 204
  - Call Chain = PCD_EP_OutXfrComplete_int ⇒ HAL_PCD_DataOutStageCallback ⇒ USBD_LL_DataOutStage ⇒ USBD_CtlContinueRx ⇒ USBD_LL_PrepareReceive ⇒ HAL_PCD_EP_Receive ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USB_EP0_OutStart
  - >> HAL_PCD_DataOutStageCallback
  [Called By]
  - >> HAL_PCD_IRQHandler

  PCD_WriteEmptyTxFifo (Thumb, 182 bytes, Stack size 40 bytes, stm32f4xx_hal_pcd.o(i.PCD_WriteEmptyTxFifo))
  [Stack]

  - Max Depth = 68
  - Call Chain = PCD_WriteEmptyTxFifo ⇒ USB_WritePacket
  [Calls]
  - >> USB_WritePacket
  [Called By]
  - >> HAL_PCD_IRQHandler

  USB_CoreReset (Thumb, 80 bytes, Stack size 8 bytes, stm32f4xx_ll_usb.o(i.USB_CoreReset))
  [Stack]

  - Max Depth = 8
  - Call Chain = USB_CoreReset
  [Called By]
  - >> USB_CoreInit

  __NVIC_GetPriorityGrouping (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_hal_cortex.o(i.__NVIC_GetPriorityGrouping))
  [Called By]

  - >> HAL_NVIC_SetPriority

  __NVIC_SetPriority (Thumb, 32 bytes, Stack size 8 bytes, stm32f4xx_hal_cortex.o(i.__NVIC_SetPriority))
  [Stack]

  - Max Depth = 8
  - Call Chain = __NVIC_SetPriority
  [Called By]
  - >> HAL_NVIC_SetPriority
  - >> HAL_SYSTICK_Config

  ADC_Init (Thumb, 344 bytes, Stack size 0 bytes, stm32f4xx_hal_adc.o(i.ADC_Init))
  [Called By]

  - >> HAL_ADC_Init

  I2C_IsAcknowledgeFailed (Thumb, 62 bytes, Stack size 0 bytes, stm32f4xx_hal_i2c.o(i.I2C_IsAcknowledgeFailed))
  [Called By]

  - >> I2C_WaitOnTXEFlagUntilTimeout
  - >> I2C_WaitOnBTFFlagUntilTimeout

  I2C_RequestMemoryRead (Thumb, 348 bytes, Stack size 32 bytes, stm32f4xx_hal_i2c.o(i.I2C_RequestMemoryRead))
  [Stack]

  - Max Depth = 56
  - Call Chain = I2C_RequestMemoryRead ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> I2C_WaitOnTXEFlagUntilTimeout
  - >> I2C_WaitOnMasterAddressFlagUntilTimeout
  - >> I2C_WaitOnFlagUntilTimeout
  [Called By]
  - >> HAL_I2C_Mem_Read

  I2C_RequestMemoryWrite (Thumb, 220 bytes, Stack size 32 bytes, stm32f4xx_hal_i2c.o(i.I2C_RequestMemoryWrite))
  [Stack]

  - Max Depth = 56
  - Call Chain = I2C_RequestMemoryWrite ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> I2C_WaitOnTXEFlagUntilTimeout
  - >> I2C_WaitOnMasterAddressFlagUntilTimeout
  - >> I2C_WaitOnFlagUntilTimeout
  [Called By]
  - >> HAL_I2C_Mem_Write

  I2C_WaitOnBTFFlagUntilTimeout (Thumb, 92 bytes, Stack size 16 bytes, stm32f4xx_hal_i2c.o(i.I2C_WaitOnBTFFlagUntilTimeout))
  [Stack]

  - Max Depth = 16
  - Call Chain = I2C_WaitOnBTFFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  - >> I2C_IsAcknowledgeFailed
  [Called By]
  - >> HAL_I2C_Mem_Write

  I2C_WaitOnFlagUntilTimeout (Thumb, 134 bytes, Stack size 24 bytes, stm32f4xx_hal_i2c.o(i.I2C_WaitOnFlagUntilTimeout))
  [Stack]

  - Max Depth = 24
  - Call Chain = I2C_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_I2C_Mem_Write
  - >> HAL_I2C_Mem_Read
  - >> I2C_RequestMemoryWrite
  - >> I2C_RequestMemoryRead

  I2C_WaitOnMasterAddressFlagUntilTimeout (Thumb, 196 bytes, Stack size 24 bytes, stm32f4xx_hal_i2c.o(i.I2C_WaitOnMasterAddressFlagUntilTimeout))
  [Stack]

  - Max Depth = 24
  - Call Chain = I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> I2C_RequestMemoryWrite
  - >> I2C_RequestMemoryRead

  I2C_WaitOnRXNEFlagUntilTimeout (Thumb, 128 bytes, Stack size 16 bytes, stm32f4xx_hal_i2c.o(i.I2C_WaitOnRXNEFlagUntilTimeout))
  [Stack]

  - Max Depth = 16
  - Call Chain = I2C_WaitOnRXNEFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_I2C_Mem_Read

  I2C_WaitOnTXEFlagUntilTimeout (Thumb, 92 bytes, Stack size 16 bytes, stm32f4xx_hal_i2c.o(i.I2C_WaitOnTXEFlagUntilTimeout))
  [Stack]

  - Max Depth = 16
  - Call Chain = I2C_WaitOnTXEFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  - >> I2C_IsAcknowledgeFailed
  [Called By]
  - >> HAL_I2C_Mem_Write
  - >> I2C_RequestMemoryWrite
  - >> I2C_RequestMemoryRead

  SPI_EndRxTxTransaction (Thumb, 100 bytes, Stack size 24 bytes, stm32f4xx_hal_spi.o(i.SPI_EndRxTxTransaction))
  [Stack]

  - Max Depth = 64
  - Call Chain = SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SPI_WaitFlagStateUntilTimeout
  [Called By]
  - >> HAL_SPI_TransmitReceive

  SPI_WaitFlagStateUntilTimeout (Thumb, 210 bytes, Stack size 40 bytes, stm32f4xx_hal_spi.o(i.SPI_WaitFlagStateUntilTimeout))
  [Stack]

  - Max Depth = 40
  - Call Chain = SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> SPI_EndRxTxTransaction

  UART_SetConfig (Thumb, 546 bytes, Stack size 40 bytes, stm32f4xx_hal_uart.o(i.UART_SetConfig))
  [Stack]

  - Max Depth = 80
  - Call Chain = UART_SetConfig ⇒ __aeabi_uldivmod
  [Calls]
  - >> HAL_RCC_GetPCLK2Freq
  - >> HAL_RCC_GetPCLK1Freq
  - >> __aeabi_uldivmod
  [Called By]
  - >> HAL_UART_Init

  UART_WaitOnFlagUntilTimeout (Thumb, 146 bytes, Stack size 24 bytes, stm32f4xx_hal_uart.o(i.UART_WaitOnFlagUntilTimeout))
  [Stack]

  - Max Depth = 24
  - Call Chain = UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_UART_Transmit

  SWAPBYTE (Thumb, 18 bytes, Stack size 12 bytes, usbd_ctlreq.o(i.SWAPBYTE))
  [Stack]

  - Max Depth = 12
  - Call Chain = SWAPBYTE
  [Called By]
  - >> USBD_ParseSetupRequest

  USBD_ClrFeature (Thumb, 62 bytes, Stack size 16 bytes, usbd_ctlreq.o(i.USBD_ClrFeature))
  [Stack]

  - Max Depth = 140
  - Call Chain = USBD_ClrFeature ⇒ USBD_CtlSendStatus ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_CtlError
  - >> USBD_CtlSendStatus
  [Called By]
  - >> USBD_StdDevReq

  USBD_GetConfig (Thumb, 86 bytes, Stack size 16 bytes, usbd_ctlreq.o(i.USBD_GetConfig))
  [Stack]

  - Max Depth = 148
  - Call Chain = USBD_GetConfig ⇒ USBD_CtlSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_CtlSendData
  - >> USBD_CtlError
  [Called By]
  - >> USBD_StdDevReq

  USBD_GetDescriptor (Thumb, 508 bytes, Stack size 24 bytes, usbd_ctlreq.o(i.USBD_GetDescriptor))
  [Stack]

  - Max Depth = 156
  - Call Chain = USBD_GetDescriptor ⇒ USBD_CtlSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_CtlSendData
  - >> USBD_CtlError
  - >> USBD_CtlSendStatus
  [Called By]
  - >> USBD_StdDevReq

  USBD_GetLen (Thumb, 22 bytes, Stack size 0 bytes, usbd_ctlreq.o(i.USBD_GetLen))
  [Called By]

  - >> USBD_GetString

  USBD_GetStatus (Thumb, 90 bytes, Stack size 16 bytes, usbd_ctlreq.o(i.USBD_GetStatus))
  [Stack]

  - Max Depth = 148
  - Call Chain = USBD_GetStatus ⇒ USBD_CtlSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_CtlSendData
  - >> USBD_CtlError
  [Called By]
  - >> USBD_StdDevReq

  USBD_SetAddress (Thumb, 90 bytes, Stack size 16 bytes, usbd_ctlreq.o(i.USBD_SetAddress))
  [Stack]

  - Max Depth = 140
  - Call Chain = USBD_SetAddress ⇒ USBD_CtlSendStatus ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_CtlError
  - >> USBD_LL_SetUSBAddress
  - >> USBD_CtlSendStatus
  [Called By]
  - >> USBD_StdDevReq

  USBD_SetConfig (Thumb, 248 bytes, Stack size 16 bytes, usbd_ctlreq.o(i.USBD_SetConfig))
  [Stack]

  - Max Depth = 140
  - Call Chain = USBD_SetConfig ⇒ USBD_CtlSendStatus ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_CtlError
  - >> USBD_CtlSendStatus
  - >> USBD_SetClassConfig
  - >> USBD_ClrClassConfig
  [Called By]
  - >> USBD_StdDevReq

  USBD_SetFeature (Thumb, 24 bytes, Stack size 16 bytes, usbd_ctlreq.o(i.USBD_SetFeature))
  [Stack]

  - Max Depth = 140
  - Call Chain = USBD_SetFeature ⇒ USBD_CtlSendStatus ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_CtlSendStatus
  [Called By]
  - >> USBD_StdDevReq

  MSC_BOT_Abort (Thumb, 78 bytes, Stack size 16 bytes, usbd_msc_bot.o(i.MSC_BOT_Abort))
  [Stack]

  - Max Depth = 72
  - Call Chain = MSC_BOT_Abort ⇒ USBD_LL_StallEP ⇒ HAL_PCD_EP_SetStall ⇒ USB_EP0_OutStart
  [Calls]
  - >> USBD_LL_StallEP
  [Called By]
  - >> MSC_BOT_CBW_Decode

  MSC_BOT_CBW_Decode (Thumb, 246 bytes, Stack size 16 bytes, usbd_msc_bot.o(i.MSC_BOT_CBW_Decode))
  [Stack]

  - Max Depth = 220
  - Call Chain = MSC_BOT_CBW_Decode ⇒ SCSI_ProcessCmd ⇒ SCSI_Write12 ⇒ SCSI_ProcessWrite ⇒ MSC_BOT_SendCSW ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> SCSI_SenseCode
  - >> SCSI_ProcessCmd
  - >> MSC_BOT_SendCSW
  - >> MSC_BOT_SendData
  - >> MSC_BOT_Abort
  - >> USBD_LL_GetRxDataSize
  [Called By]
  - >> MSC_BOT_DataOut

  MSC_BOT_SendData (Thumb, 94 bytes, Stack size 24 bytes, usbd_msc_bot.o(i.MSC_BOT_SendData))
  [Stack]

  - Max Depth = 140
  - Call Chain = MSC_BOT_SendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_Transmit
  [Called By]
  - >> MSC_BOT_CBW_Decode

  SCSI_AllowPreventRemovable (Thumb, 48 bytes, Stack size 12 bytes, usbd_msc_scsi.o(i.SCSI_AllowPreventRemovable))
  [Stack]

  - Max Depth = 12
  - Call Chain = SCSI_AllowPreventRemovable
  [Called By]
  - >> SCSI_ProcessCmd

  SCSI_CheckAddressRange (Thumb, 60 bytes, Stack size 24 bytes, usbd_msc_scsi.o(i.SCSI_CheckAddressRange))
  [Stack]

  - Max Depth = 44
  - Call Chain = SCSI_CheckAddressRange ⇒ SCSI_SenseCode
  [Calls]
  - >> SCSI_SenseCode
  [Called By]
  - >> SCSI_Write12
  - >> SCSI_Write10
  - >> SCSI_Verify10
  - >> SCSI_Read12
  - >> SCSI_Read10

  SCSI_Inquiry (Thumb, 168 bytes, Stack size 32 bytes, usbd_msc_scsi.o(i.SCSI_Inquiry))
  [Stack]

  - Max Depth = 52
  - Call Chain = SCSI_Inquiry ⇒ SCSI_SenseCode
  [Calls]
  - >> SCSI_UpdateBotData
  - >> SCSI_SenseCode
  [Called By]
  - >> SCSI_ProcessCmd

  SCSI_ModeSense10 (Thumb, 48 bytes, Stack size 24 bytes, usbd_msc_scsi.o(i.SCSI_ModeSense10))
  [Stack]

  - Max Depth = 36
  - Call Chain = SCSI_ModeSense10 ⇒ SCSI_UpdateBotData
  [Calls]
  - >> SCSI_UpdateBotData
  [Called By]
  - >> SCSI_ProcessCmd

  SCSI_ModeSense6 (Thumb, 48 bytes, Stack size 24 bytes, usbd_msc_scsi.o(i.SCSI_ModeSense6))
  [Stack]

  - Max Depth = 36
  - Call Chain = SCSI_ModeSense6 ⇒ SCSI_UpdateBotData
  [Calls]
  - >> SCSI_UpdateBotData
  [Called By]
  - >> SCSI_ProcessCmd

  SCSI_ProcessRead (Thumb, 210 bytes, Stack size 24 bytes, usbd_msc_scsi.o(i.SCSI_ProcessRead))
  [Stack]

  - Max Depth = 140
  - Call Chain = SCSI_ProcessRead ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> SCSI_SenseCode
  - >> USBD_LL_Transmit
  [Called By]
  - >> SCSI_Read12
  - >> SCSI_Read10

  SCSI_ProcessWrite (Thumb, 258 bytes, Stack size 24 bytes, usbd_msc_scsi.o(i.SCSI_ProcessWrite))
  [Stack]

  - Max Depth = 156
  - Call Chain = SCSI_ProcessWrite ⇒ MSC_BOT_SendCSW ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> SCSI_SenseCode
  - >> MSC_BOT_SendCSW
  - >> USBD_LL_PrepareReceive
  [Called By]
  - >> SCSI_Write12
  - >> SCSI_Write10

  SCSI_Read10 (Thumb, 262 bytes, Stack size 24 bytes, usbd_msc_scsi.o(i.SCSI_Read10))
  [Stack]

  - Max Depth = 164
  - Call Chain = SCSI_Read10 ⇒ SCSI_ProcessRead ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> SCSI_ProcessRead
  - >> SCSI_CheckAddressRange
  - >> SCSI_SenseCode
  [Called By]
  - >> SCSI_ProcessCmd

  SCSI_Read12 (Thumb, 278 bytes, Stack size 24 bytes, usbd_msc_scsi.o(i.SCSI_Read12))
  [Stack]

  - Max Depth = 164
  - Call Chain = SCSI_Read12 ⇒ SCSI_ProcessRead ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> SCSI_ProcessRead
  - >> SCSI_CheckAddressRange
  - >> SCSI_SenseCode
  [Called By]
  - >> SCSI_ProcessCmd

  SCSI_ReadCapacity10 (Thumb, 168 bytes, Stack size 24 bytes, usbd_msc_scsi.o(i.SCSI_ReadCapacity10))
  [Stack]

  - Max Depth = 44
  - Call Chain = SCSI_ReadCapacity10 ⇒ SCSI_SenseCode
  [Calls]
  - >> SCSI_SenseCode
  [Called By]
  - >> SCSI_ProcessCmd

  SCSI_ReadCapacity16 (Thumb, 234 bytes, Stack size 32 bytes, usbd_msc_scsi.o(i.SCSI_ReadCapacity16))
  [Stack]

  - Max Depth = 52
  - Call Chain = SCSI_ReadCapacity16 ⇒ SCSI_SenseCode
  [Calls]
  - >> SCSI_SenseCode
  [Called By]
  - >> SCSI_ProcessCmd

  SCSI_ReadFormatCapacity (Thumb, 158 bytes, Stack size 40 bytes, usbd_msc_scsi.o(i.SCSI_ReadFormatCapacity))
  [Stack]

  - Max Depth = 60
  - Call Chain = SCSI_ReadFormatCapacity ⇒ SCSI_SenseCode
  [Calls]
  - >> SCSI_SenseCode
  [Called By]
  - >> SCSI_ProcessCmd

  SCSI_RequestSense (Thumb, 200 bytes, Stack size 24 bytes, usbd_msc_scsi.o(i.SCSI_RequestSense))
  [Stack]

  - Max Depth = 44
  - Call Chain = SCSI_RequestSense ⇒ SCSI_SenseCode
  [Calls]
  - >> SCSI_SenseCode
  [Called By]
  - >> SCSI_ProcessCmd

  SCSI_StartStopUnit (Thumb, 124 bytes, Stack size 20 bytes, usbd_msc_scsi.o(i.SCSI_StartStopUnit))
  [Stack]

  - Max Depth = 40
  - Call Chain = SCSI_StartStopUnit ⇒ SCSI_SenseCode
  [Calls]
  - >> SCSI_SenseCode
  [Called By]
  - >> SCSI_ProcessCmd

  SCSI_TestUnitReady (Thumb, 128 bytes, Stack size 24 bytes, usbd_msc_scsi.o(i.SCSI_TestUnitReady))
  [Stack]

  - Max Depth = 44
  - Call Chain = SCSI_TestUnitReady ⇒ SCSI_SenseCode
  [Calls]
  - >> SCSI_SenseCode
  [Called By]
  - >> SCSI_ProcessCmd

  SCSI_UpdateBotData (Thumb, 40 bytes, Stack size 12 bytes, usbd_msc_scsi.o(i.SCSI_UpdateBotData))
  [Stack]

  - Max Depth = 12
  - Call Chain = SCSI_UpdateBotData
  [Called By]
  - >> SCSI_ModeSense6
  - >> SCSI_ModeSense10
  - >> SCSI_Inquiry

  SCSI_Verify10 (Thumb, 88 bytes, Stack size 24 bytes, usbd_msc_scsi.o(i.SCSI_Verify10))
  [Stack]

  - Max Depth = 68
  - Call Chain = SCSI_Verify10 ⇒ SCSI_CheckAddressRange ⇒ SCSI_SenseCode
  [Calls]
  - >> SCSI_CheckAddressRange
  - >> SCSI_SenseCode
  [Called By]
  - >> SCSI_ProcessCmd

  SCSI_Write10 (Thumb, 332 bytes, Stack size 24 bytes, usbd_msc_scsi.o(i.SCSI_Write10))
  [Stack]

  - Max Depth = 180
  - Call Chain = SCSI_Write10 ⇒ SCSI_ProcessWrite ⇒ MSC_BOT_SendCSW ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> SCSI_ProcessWrite
  - >> SCSI_CheckAddressRange
  - >> SCSI_SenseCode
  - >> USBD_LL_PrepareReceive
  [Called By]
  - >> SCSI_ProcessCmd

  SCSI_Write12 (Thumb, 352 bytes, Stack size 24 bytes, usbd_msc_scsi.o(i.SCSI_Write12))
  [Stack]

  - Max Depth = 180
  - Call Chain = SCSI_Write12 ⇒ SCSI_ProcessWrite ⇒ MSC_BOT_SendCSW ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> SCSI_ProcessWrite
  - >> SCSI_CheckAddressRange
  - >> SCSI_SenseCode
  - >> USBD_LL_PrepareReceive
  [Called By]
  - >> SCSI_ProcessCmd

  lcd_opt_delay (Thumb, 12 bytes, Stack size 0 bytes, lcd.o(i.lcd_opt_delay))
  [Called By]

  - >> lcd_rd_data

  lcd_rd_data (Thumb, 20 bytes, Stack size 8 bytes, lcd.o(i.lcd_rd_data))
  [Stack]

  - Max Depth = 8
  - Call Chain = lcd_rd_data
  [Calls]
  - >> lcd_opt_delay
  [Called By]
  - >> lcd_read_point
  - >> lcd_init

  Draw2x2Block (Thumb, 72 bytes, Stack size 24 bytes, mlx90640.o(i.Draw2x2Block))
  [Stack]

  - Max Depth = 56
  - Call Chain = Draw2x2Block ⇒ lcd_draw_point ⇒ lcd_set_cursor ⇒ lcd_wr_regno
  [Calls]
  - >> lcd_draw_point
  [Called By]
  - >> DrawTopRows
  - >> DrawThermalRow

  DrawCrosshair (Thumb, 68 bytes, Stack size 24 bytes, mlx90640.o(i.DrawCrosshair))
  [Stack]

  - Max Depth = 56
  - Call Chain = DrawCrosshair ⇒ lcd_draw_point ⇒ lcd_set_cursor ⇒ lcd_wr_regno
  [Calls]
  - >> lcd_draw_point
  [Called By]
  - >> Disp_TempPic

  DrawFullThermalRegion (Thumb, 54 bytes, Stack size 32 bytes, mlx90640.o(i.DrawFullThermalRegion))
  [Stack]

  - Max Depth = 188
  - Call Chain = DrawFullThermalRegion ⇒ DrawThermalRow ⇒ GetThermalColor ⇒ __aeabi_fsub ⇒ __aeabi_fadd ⇒ _float_epilogue
  [Calls]
  - >> DrawThermalRow
  [Called By]
  - >> Disp_TempPic

  DrawThermalRow (Thumb, 62 bytes, Stack size 32 bytes, mlx90640.o(i.DrawThermalRow))
  [Stack]

  - Max Depth = 156
  - Call Chain = DrawThermalRow ⇒ GetThermalColor ⇒ __aeabi_fsub ⇒ __aeabi_fadd ⇒ _float_epilogue
  [Calls]
  - >> GetThermalColor
  - >> Draw2x2Block
  [Called By]
  - >> DrawFullThermalRegion

  DrawTopRows (Thumb, 214 bytes, Stack size 64 bytes, mlx90640.o(i.DrawTopRows))
  [Stack]

  - Max Depth = 188
  - Call Chain = DrawTopRows ⇒ GetThermalColor ⇒ __aeabi_fsub ⇒ __aeabi_fadd ⇒ _float_epilogue
  [Calls]
  - >> lcd_draw_point
  - >> GetThermalColor
  - >> Draw2x2Block
  [Called By]
  - >> Disp_TempPic

  DrawValueMarker (Thumb, 110 bytes, Stack size 24 bytes, mlx90640.o(i.DrawValueMarker))
  [Stack]

  - Max Depth = 56
  - Call Chain = DrawValueMarker ⇒ lcd_draw_point ⇒ lcd_set_cursor ⇒ lcd_wr_regno
  [Calls]
  - >> lcd_draw_point
  [Called By]
  - >> Disp_TempPic

  GetThermalColor (Thumb, 354 bytes, Stack size 104 bytes, mlx90640.o(i.GetThermalColor))
  [Stack]

  - Max Depth = 124
  - Call Chain = GetThermalColor ⇒ __aeabi_fsub ⇒ __aeabi_fadd ⇒ _float_epilogue
  [Calls]
  - >> SafeGetMLXData
  - >> __aeabi_ui2f
  - >> __aeabi_fsub
  - >> __aeabi_fmul
  - >> __aeabi_fdiv
  - >> __aeabi_fadd
  - >> __aeabi_f2iz
  [Called By]
  - >> DrawTopRows
  - >> DrawThermalRow

  SafeGetMLXData (Thumb, 24 bytes, Stack size 0 bytes, mlx90640.o(i.SafeGetMLXData))
  [Called By]

  - >> GetThermalColor

  lcd_show_string_transparent (Thumb, 60 bytes, Stack size 32 bytes, mlx90640.o(i.lcd_show_string_transparent))
  [Stack]

  - Max Depth = 108
  - Call Chain = lcd_show_string_transparent ⇒ lcd_show_char ⇒ lcd_draw_point ⇒ lcd_set_cursor ⇒ lcd_wr_regno
  [Calls]
  - >> lcd_show_char
  [Called By]
  - >> Disp_TempPic

  check_fs (Thumb, 116 bytes, Stack size 16 bytes, ff.o(i.check_fs))
  [Stack]

  - Max Depth = 80
  - Call Chain = check_fs ⇒ move_window ⇒ sync_window ⇒ disk_write
  [Calls]
  - >> move_window
  - >> ld_word
  - >> ld_dword
  [Called By]
  - >> find_volume

  chk_chr (Thumb, 20 bytes, Stack size 0 bytes, ff.o(i.chk_chr))
  [Called By]

  - >> create_name

  chk_lock (Thumb, 120 bytes, Stack size 12 bytes, ff.o(i.chk_lock))
  [Stack]

  - Max Depth = 12
  - Call Chain = chk_lock
  [Called By]
  - >> f_open

  clear_lock (Thumb, 36 bytes, Stack size 0 bytes, ff.o(i.clear_lock))
  [Called By]

  - >> f_mount
  - >> find_volume

  clmt_clust (Thumb, 50 bytes, Stack size 20 bytes, ff.o(i.clmt_clust))
  [Stack]

  - Max Depth = 20
  - Call Chain = clmt_clust
  [Called By]
  - >> f_write
  - >> f_read

  clust2sect (Thumb, 26 bytes, Stack size 0 bytes, ff.o(i.clust2sect))
  [Called By]

  - >> f_write
  - >> f_read
  - >> f_open
  - >> dir_sdi
  - >> dir_next

  create_chain (Thumb, 222 bytes, Stack size 32 bytes, ff.o(i.create_chain))
  [Stack]

  - Max Depth = 128
  - Call Chain = create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write
  [Calls]
  - >> put_fat
  - >> get_fat
  [Called By]
  - >> f_write
  - >> dir_next

  create_name (Thumb, 204 bytes, Stack size 40 bytes, ff.o(i.create_name))
  [Stack]

  - Max Depth = 48
  - Call Chain = create_name ⇒ mem_set
  [Calls]
  - >> chk_chr
  - >> mem_set
  [Called By]
  - >> follow_path

  dec_lock (Thumb, 64 bytes, Stack size 8 bytes, ff.o(i.dec_lock))
  [Stack]

  - Max Depth = 8
  - Call Chain = dec_lock
  [Called By]
  - >> f_close

  dir_alloc (Thumb, 96 bytes, Stack size 24 bytes, ff.o(i.dir_alloc))
  [Stack]

  - Max Depth = 184
  - Call Chain = dir_alloc ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write
  [Calls]
  - >> dir_sdi
  - >> dir_next
  - >> move_window
  [Called By]
  - >> dir_register

  dir_find (Thumb, 108 bytes, Stack size 24 bytes, ff.o(i.dir_find))
  [Stack]

  - Max Depth = 184
  - Call Chain = dir_find ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write
  [Calls]
  - >> dir_sdi
  - >> dir_next
  - >> move_window
  - >> mem_cmp
  [Called By]
  - >> follow_path

  dir_next (Thumb, 268 bytes, Stack size 32 bytes, ff.o(i.dir_next))
  [Stack]

  - Max Depth = 160
  - Call Chain = dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write
  [Calls]
  - >> create_chain
  - >> clust2sect
  - >> sync_window
  - >> mem_set
  - >> get_fat
  [Called By]
  - >> dir_find
  - >> dir_alloc

  dir_register (Thumb, 60 bytes, Stack size 16 bytes, ff.o(i.dir_register))
  [Stack]

  - Max Depth = 200
  - Call Chain = dir_register ⇒ dir_alloc ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write
  [Calls]
  - >> dir_alloc
  - >> move_window
  - >> mem_set
  - >> mem_cpy
  [Called By]
  - >> f_open

  dir_sdi (Thumb, 154 bytes, Stack size 24 bytes, ff.o(i.dir_sdi))
  [Stack]

  - Max Depth = 120
  - Call Chain = dir_sdi ⇒ get_fat ⇒ move_window ⇒ sync_window ⇒ disk_write
  [Calls]
  - >> clust2sect
  - >> get_fat
  [Called By]
  - >> dir_find
  - >> dir_alloc
  - >> follow_path

  enq_lock (Thumb, 34 bytes, Stack size 0 bytes, ff.o(i.enq_lock))
  [Called By]

  - >> f_open

  find_volume (Thumb, 750 bytes, Stack size 88 bytes, ff.o(i.find_volume))
  [Stack]

  - Max Depth = 168
  - Call Chain = find_volume ⇒ check_fs ⇒ move_window ⇒ sync_window ⇒ disk_write
  [Calls]
  - >> clear_lock
  - >> check_fs
  - >> disk_status
  - >> disk_initialize
  - >> move_window
  - >> ld_word
  - >> ld_dword
  - >> get_ldnumber
  [Called By]
  - >> f_open
  - >> f_mount

  follow_path (Thumb, 162 bytes, Stack size 32 bytes, ff.o(i.follow_path))
  [Stack]

  - Max Depth = 216
  - Call Chain = follow_path ⇒ dir_find ⇒ dir_next ⇒ create_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write
  [Calls]
  - >> dir_sdi
  - >> dir_find
  - >> create_name
  - >> ld_clust
  [Called By]
  - >> f_open

  get_fat (Thumb, 224 bytes, Stack size 32 bytes, ff.o(i.get_fat))
  [Stack]

  - Max Depth = 96
  - Call Chain = get_fat ⇒ move_window ⇒ sync_window ⇒ disk_write
  [Calls]
  - >> move_window
  - >> ld_word
  - >> ld_dword
  [Called By]
  - >> f_read
  - >> f_open
  - >> dir_sdi
  - >> dir_next
  - >> create_chain
  - >> remove_chain

  get_ldnumber (Thumb, 72 bytes, Stack size 16 bytes, ff.o(i.get_ldnumber))
  [Stack]

  - Max Depth = 16
  - Call Chain = get_ldnumber
  [Called By]
  - >> f_mount
  - >> f_mkfs
  - >> find_volume

  inc_lock (Thumb, 182 bytes, Stack size 8 bytes, ff.o(i.inc_lock))
  [Stack]

  - Max Depth = 8
  - Call Chain = inc_lock
  [Called By]
  - >> f_open

  ld_clust (Thumb, 38 bytes, Stack size 16 bytes, ff.o(i.ld_clust))
  [Stack]

  - Max Depth = 16
  - Call Chain = ld_clust
  [Calls]
  - >> ld_word
  [Called By]
  - >> f_open
  - >> follow_path

  ld_dword (Thumb, 24 bytes, Stack size 0 bytes, ff.o(i.ld_dword))
  [Called By]

  - >> f_open
  - >> check_fs
  - >> put_fat
  - >> get_fat
  - >> find_volume

  ld_word (Thumb, 12 bytes, Stack size 0 bytes, ff.o(i.ld_word))
  [Called By]

  - >> check_fs
  - >> ld_clust
  - >> get_fat
  - >> find_volume

  mem_cmp (Thumb, 36 bytes, Stack size 20 bytes, ff.o(i.mem_cmp))
  [Stack]

  - Max Depth = 20
  - Call Chain = mem_cmp
  [Called By]
  - >> dir_find

  mem_cpy (Thumb, 26 bytes, Stack size 12 bytes, ff.o(i.mem_cpy))
  [Stack]

  - Max Depth = 12
  - Call Chain = mem_cpy
  [Called By]
  - >> f_write
  - >> f_read
  - >> f_mkfs
  - >> dir_register

  mem_set (Thumb, 18 bytes, Stack size 8 bytes, ff.o(i.mem_set))
  [Stack]

  - Max Depth = 8
  - Call Chain = mem_set
  [Called By]
  - >> f_open
  - >> f_mkfs
  - >> dir_register
  - >> dir_next
  - >> create_name
  - >> sync_fs

  move_window (Thumb, 52 bytes, Stack size 16 bytes, ff.o(i.move_window))
  [Stack]

  - Max Depth = 64
  - Call Chain = move_window ⇒ sync_window ⇒ disk_write
  [Calls]
  - >> disk_read
  - >> sync_window
  [Called By]
  - >> f_sync
  - >> f_open
  - >> dir_register
  - >> dir_find
  - >> dir_alloc
  - >> check_fs
  - >> put_fat
  - >> get_fat
  - >> find_volume

  put_fat (Thumb, 312 bytes, Stack size 32 bytes, ff.o(i.put_fat))
  [Stack]

  - Max Depth = 96
  - Call Chain = put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write
  [Calls]
  - >> st_word
  - >> st_dword
  - >> move_window
  - >> ld_dword
  [Called By]
  - >> create_chain
  - >> remove_chain

  remove_chain (Thumb, 154 bytes, Stack size 32 bytes, ff.o(i.remove_chain))
  [Stack]

  - Max Depth = 128
  - Call Chain = remove_chain ⇒ put_fat ⇒ move_window ⇒ sync_window ⇒ disk_write
  [Calls]
  - >> put_fat
  - >> get_fat
  [Called By]
  - >> f_open

  st_clust (Thumb, 36 bytes, Stack size 16 bytes, ff.o(i.st_clust))
  [Stack]

  - Max Depth = 16
  - Call Chain = st_clust
  [Calls]
  - >> st_word
  [Called By]
  - >> f_sync
  - >> f_open

  st_dword (Thumb, 24 bytes, Stack size 0 bytes, ff.o(i.st_dword))
  [Called By]

  - >> f_sync
  - >> f_open
  - >> f_mkfs
  - >> sync_fs
  - >> put_fat

  st_word (Thumb, 12 bytes, Stack size 0 bytes, ff.o(i.st_word))
  [Called By]

  - >> f_sync
  - >> f_mkfs
  - >> sync_fs
  - >> st_clust
  - >> put_fat

  sync_fs (Thumb, 134 bytes, Stack size 16 bytes, ff.o(i.sync_fs))
  [Stack]

  - Max Depth = 64
  - Call Chain = sync_fs ⇒ sync_window ⇒ disk_write
  [Calls]
  - >> disk_write
  - >> disk_ioctl
  - >> sync_window
  - >> st_word
  - >> st_dword
  - >> mem_set
  [Called By]
  - >> f_sync

  sync_window (Thumb, 82 bytes, Stack size 24 bytes, ff.o(i.sync_window))
  [Stack]

  - Max Depth = 48
  - Call Chain = sync_window ⇒ disk_write
  [Calls]
  - >> disk_write
  [Called By]
  - >> dir_next
  - >> sync_fs
  - >> move_window

  validate (Thumb, 60 bytes, Stack size 16 bytes, ff.o(i.validate))
  [Stack]

  - Max Depth = 32
  - Call Chain = validate ⇒ disk_status
  [Calls]
  - >> disk_status
  [Called By]
  - >> f_write
  - >> f_sync
  - >> f_read
  - >> f_close

  _fp_digits (Thumb, 334 bytes, Stack size 56 bytes, printfa.o(i._fp_digits), UNUSED)
  [Calls]

  - >> __aeabi_dmul
  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> __aeabi_uldivmod
  - >> __aeabi_cdrcmple
  - >> __aeabi_d2ulz
  [Called By]
  - >> _printf_core

  _printf_core (Thumb, 1744 bytes, Stack size 136 bytes, printfa.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uldivmod
  - >> __aeabi_uidivmod
  - >> _printf_pre_padding
  - >> _printf_post_padding
  - >> _fp_digits
  [Called By]
  - >> __0sprintf
  - >> __0printf

  _printf_post_padding (Thumb, 36 bytes, Stack size 24 bytes, printfa.o(i._printf_post_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _printf_pre_padding (Thumb, 46 bytes, Stack size 24 bytes, printfa.o(i._printf_pre_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _sputc (Thumb, 10 bytes, Stack size 0 bytes, printfa.o(i._sputc))
  [Called By]

  - >> __0sprintf
  [Address Reference Count : 1]
  - printfa.o(i.__0sprintf)

  ### Undefined Global Symbols