.. _gdallocationinfo:

================================================================================
gdallocationinfo
================================================================================

.. only:: html

    Raster query tool

.. Index:: gdallocationinfo

Synopsis
--------

.. program-output:: gdallocationinfo --help-doc

Description
-----------

The :program:`gdallocationinfo` utility provide a mechanism to query information about
a pixel given its location in one of a variety of coordinate systems.  Several
reporting options are provided.

.. tip:: Equivalent in new "gdal" command line interface:

    See :ref:`gdal_raster_pixel_info`.

.. program:: gdallocationinfo

.. include:: options/help_and_help_general.rst

.. option:: -xml

    The output report will be XML formatted for convenient post processing.
    (:example:`xml`).

.. option:: -lifonly

    The only output is filenames production from the LocationInfo request
    against the database (i.e. for identifying impacted file from VRT).

.. option:: -valonly

    The only output is the pixel values of the selected pixel on each of
    the selected bands. By default, the value of each band is output on a
    separate line, unless :option:`-field_sep` is specified.

.. option:: -b <band>

    Selects a band to query.  Multiple bands can be listed.  By default all
    bands are queried.

.. option:: -r {nearest|bilinear|cubic|cubicspline}

    .. versionadded:: 3.10

    Select a sampling algorithm. The default is ``nearest``.

    The available methods are:

    ``nearest`` applies a nearest neighbour.

    ``bilinear`` applies a bilinear convolution kernel.

    ``cubic`` applies a cubic convolution kernel.

    ``cubicspline`` applies a B-Spline convolution kernel.

.. option:: -overview <overview_level>

    Query the (overview_level)th overview (overview_level=1 is the 1st overview),
    instead of the base band. Note that the x,y location (if the coordinate system is
    pixel/line) must still be given with respect to the base band.

.. option:: -l_srs <srs_def>

    The coordinate system of the input x, y location.

.. option:: -geoloc

    Indicates input x,y points are in the georeferencing system of the image.

.. option:: -wgs84

    Indicates input x,y points are WGS84 long, lat.

.. option:: -oo <NAME>=<VALUE>

    Dataset open option (format specific)

.. option:: -ignore_extra_input

    .. versionadded:: 3.9

    Set this flag to avoid extra non-numeric content at end of input lines to be
    appended to the output lines in -valonly mode (requires :option:`-field_sep`
    to be also defined), or as a dedicated field in default or :option:`-xml` modes.

.. option:: -E

    .. versionadded:: 3.9

    Enable Echo mode, where input coordinates are prepended to the output lines
    in :option:`-valonly` mode.

.. option:: -field_sep <sep>

    .. versionadded:: 3.9

    Defines the field separator, used in :option:`-valonly` mode, to separate different values.
    It defaults to the new-line character, which means that when querying
    a raster with several bands, the output will contain one value per line, which
    may make it hard to recognize which value belongs to which set of input x,y
    points when several ones are provided. Defining the field separator is also
    needed

.. option:: <srcfile>

    The source GDAL raster datasource name.

.. option:: <x>

    X location of target pixel.  By default the
    coordinate system is pixel/line unless -l_srs, -wgs84 or -geoloc supplied.

.. option:: <y>

    Y location of target pixel.  By default the
    coordinate system is pixel/line unless -l_srs, -wgs84 or -geoloc supplied.


This utility is intended to provide a variety of information about a
pixel.  Currently it reports:

- The location of the pixel in pixel/line space.
- The result of a LocationInfo metadata query against the datasource.
  This is implemented for VRT files which will report the
  file(s) used to satisfy requests for that pixel, and by the
  :ref:`raster.mbtiles` driver.
- The raster pixel value of that pixel for all or a subset of the bands.
- The unscaled pixel value if a Scale and/or Offset apply to the band.

The pixel selected is requested by x/y coordinate on the command line, or read
from stdin. More than one coordinate pair can be supplied when reading
coordinates from stdin. By default integer pixel/line coordinates are expected.
However with use of the :option:`-geoloc`, :option:`-wgs84`, or :option:`-l_srs` switches it is possible
to specify the location in other coordinate systems.

The default report is in a human readable text format.  It is possible to
instead request xml output with the -xml switch.

For scripting purposes, the -valonly and -lifonly switches are provided to
restrict output to the actual pixel values, or the LocationInfo files
identified for the pixel.

It is anticipated that additional reporting capabilities will be added to
gdallocationinfo in the future.

.. Return status code
.. ------------------

.. include:: return_code.rst

Examples
--------

.. example::
   :title: Reporting on pixel (256,256) on the file :file:`utm.tif`

   .. code-block:: console

       $ gdallocationinfo utm.tif 256 256
       Report:
       Location: (256P,256L)
       Band 1:
           Value: 115


.. example::
   :title: Querying a VRT file providing the location in WGS84, and getting the result in XML
   :id: xml

   .. code-block:: console

       $ gdallocationinfo -xml -wgs84 utm.vrt -117.5 33.75
       <Report pixel="217" line="282">
           <BandReport band="1">
               <LocationInfo>
               <File>utm.tif</File>
               </LocationInfo>
               <Value>16</Value>
           </BandReport>
       </Report>

.. example::
   :title: Reading locations from stdin

   .. code-block:: console

       $ cat coordinates.txt
       443020 3748359
       441197 3749005
       443852 3747743

       $ cat coordinates.txt | gdallocationinfo -geoloc utmsmall.tif
       Report:
         Location: (38P,49L)
         Band 1:
           Value: 214
       Report:
         Location: (7P,38L)
         Band 1:
           Value: 107
       Report:
         Location: (52P,59L)
         Band 1:
           Value: 148

       $ cat coordinates.txt | gdallocationinfo -geoloc -valonly -E -field_sep , utmsmall.tif
       443020,3748359,214
       441197,3749005,107
       443852,3747743,148
