# class LTEAuthenticationInfoListener

    @Keep
     interface LTEAuthenticationInfoListener

Package: | dji.v5.manager.aircraft.lte

##### Description:

Listener for LTE authentication information.
`Supported since MSDK 5.2.0`

##### Class Members:

method
onLTEAuthenticationInfoUpdate

###### method onLTEAuthenticationInfoUpdate

    void onLTEAuthenticationInfoUpdate(LTEAuthenticationInfo info)

Package: | dji.v5.manager.aircraft.lte

##### Description:

When the LTE authentication information changes, this method will be called back.
`Supported since MSDK 5.2.0`

##### Input Parameters:

LTEAuthenticationInfo info | LTE authentication information.

×

## Search Mobile SDK Document

{{searchCount}} Results

- ### {{{(item.highlights && item.highlights.title) || item.title}}}

  {{{(item.highlights && item.highlights.content[0]) || item.title}}}

Load More
Loading...
Not Found