# class LaserMeasureInformation

    class LaserMeasureInformation implements DJIValue, JNIProguardKeepTag, ByteStream

Package: | dji.sdk.keyvalue.value.camera

##### Description:

Laser measure information.

##### Class Members:

#### Members

method
getLocation3D

###### method getLocation3D

    LocationCoordinate3D getLocation3D()

Package: | dji.sdk.keyvalue.value.camera

##### Description:

Gets the location of the target point, including longitude, latitude and altitude.

##### Return:

LocationCoordinate3D | Returns the location of the target point.

method
getDistance

###### method getDistance

    Double getDistance()

Package: | dji.sdk.keyvalue.value.camera

##### Description:

Gets the distance of the target point from the laser sensor. The target point must be at least 3m away from The laser sensor.

##### Return:

Double | Returns the distance of the target point from the laser sensor.

method
getTargetPoint

###### method getTargetPoint

    DoublePoint2D getTargetPoint()

Package: | dji.sdk.keyvalue.value.camera

##### Description:

Gets the position of the target point on the camera screen. Range of x and y: [0,100]. [0,0] represents the upper left corner of the camera screen, [100,100] represents the lower right corner of the camera screen.

##### Return:

DoublePoint2D | Returns the position of the target point on the camera screen.

method
getLaserMeasureState

###### method getLaserMeasureState

    LaserMeasureState getLaserMeasureState()

Package: | dji.sdk.keyvalue.value.camera

##### Description:

Gets the laser measure status.

##### Return:

LaserMeasureState | Returns the laser measure status.

×

## Search Mobile SDK Document

{{searchCount}} Results

- ### {{{(item.highlights && item.highlights.title) || item.title}}}

  {{{(item.highlights && item.highlights.content[0]) || item.title}}}

Load More
Loading...
Not Found