# class CameraStorageStateMsg

    class CameraStorageStateMsg implements DJIValue, JNIProguardKeepTag, ByteStream

Package: | dji.sdk.keyvalue.value.camera

##### Description:

The storage information for camera SD card and onboard memory.

##### Class Members:

#### Members

method
getCurStorageType

###### method getCurStorageType

    Integer getCurStorageType()

Package: | dji.sdk.keyvalue.value.camera

##### Description:

Get the current storage location in use by the camera. 0 means that the SD card is currently being used to store media files. 1 indicates that the onboard memory is currently being used to store media files.

##### Return:

Integer | Returns the current storage location in use by the camera.

method
getStorageInfos

###### method getStorageInfos

    List<CameraStorageState> getStorageInfos()

Package: | dji.sdk.keyvalue.value.camera

##### Description:

To get the details of the current camera storage card, including the details of the SD Card and onboard memory.

##### Return:

List<CameraStorageState> | Returns details of the current camera storage card.

×

## Search Mobile SDK Document

{{searchCount}} Results

- ### {{{(item.highlights && item.highlights.title) || item.title}}}

  {{{(item.highlights && item.highlights.content[0]) || item.title}}}

Load More
Loading...
Not Found