# class MultiControlLockAuthorityInfo

    class MultiControlLockAuthorityInfo implements DJIValue, JNIProguardKeepTag, ByteStream

Package: | dji.sdk.keyvalue.value.common

##### Description:

This class is used to define control locking information.

##### Class Members:

method
getLockAuthorityType

###### method getLockAuthorityType

    MultiControlAuthorityTypeInfo getLockAuthorityType()

Package: | dji.sdk.keyvalue.value.common

##### Description:

Return the control type that needs to be locked.

##### Return:

MultiControlAuthorityTypeInfo | Return the control type that needs to be locked.

method
setLockAuthorityType

###### method setLockAuthorityType

    void setLockAuthorityType(MultiControlAuthorityTypeInfo lockAuthorityType)

Package: | dji.sdk.keyvalue.value.common

##### Description:

Set the control type that needs to be locked.

##### Input Parameters:

MultiControlAuthorityTypeInfo lockAuthorityType | Set the control type that needs to be locked.

method
getBLock

###### method getBLock

    Boolean getBLock()

Package: | dji.sdk.keyvalue.value.common

##### Description:

Get whether locking control is required.

##### Return:

Boolean | Return whether locking control is required.

method
setBLock

###### method setBLock

    void setBLock(Boolean bLock)

Package: | dji.sdk.keyvalue.value.common

##### Description:

Set whether locking control is required.

##### Input Parameters:

Boolean bLock | `true` means that locking control is required.

×

## Search Mobile SDK Document

{{searchCount}} Results

- ### {{{(item.highlights && item.highlights.title) || item.title}}}

  {{{(item.highlights && item.highlights.content[0]) || item.title}}}

Load More
Loading...
Not Found