# class RTKSystemState

    class RTKSystemState

Package: | dji.v5.manager.aircraft.rtk

##### Description:

RTK system state.
`Supported since MSDK 5.0.0`

##### Class Members:

#### Members

method
getRTKConnected

###### method getRTKConnected

    boolean getRTKConnected()

Package: | dji.v5.manager.aircraft.rtk

##### Description:

Get the connection status of the RTK module on the aircraft between the flight system. The default value is `true`, it will only become `false` when the RTK module on the aircraft has a circuit fault.
`Supported since MSDK 5.0.0`

##### Return:

boolean | `true`means the RTK moudle on the aircraft is connected with the flight system.

method
getRTKHealthy

###### method getRTKHealthy

    boolean getRTKHealthy()

Package: | dji.v5.manager.aircraft.rtk

##### Description:

Get the working status of the RTK module on the aircraft.
`Supported since MSDK 5.0.0`

##### Return:

boolean | `true`means the RTK module is working normally on the aircraft.

method
getSatelliteInfo

###### method getSatelliteInfo

    RTKSatelliteInfo getSatelliteInfo()

Package: | dji.v5.manager.aircraft.rtk

##### Description:

Get the satellite information of the RTK module on the aircraft.
`Supported since MSDK 5.0.0`

##### Return:

RTKSatelliteInfo | Return the satellite information of the RTK module on the aircraft.

×

## Search Mobile SDK Document

{{searchCount}} Results

- ### {{{(item.highlights && item.highlights.title) || item.title}}}

  {{{(item.highlights && item.highlights.content[0]) || item.title}}}

Load More
Loading...
Not Found