                                                          劇劅劅劅劅劅劅劅劅劉
                                                          劆IO95630  -V01L02劆
                                                          劋劅劅劅劅劅劅劅劅劊
























                       F2MC-8FX僼傽儈儕 MB95630僔儕乕僘梡
                          僒儞僾儖I/O儗僕僗僞僼傽僀儖
                              巊  梡  庤  堷  彂

                       晉巑捠僙儈僐儞僟僋僞乕姅幃夛幮

                                    V01L02

偼偠傔偵

  MB95630僔儕乕僘梡僒儞僾儖I/O儗僕僗僞僼傽僀儖偼丄I/O儗僕僗僞傪
俠尵岅偺曄悢偲偟偰愰尵丄偍傛傃掕媊偟偰偄傞僒儞僾儖僾儘僌儔儉偱偡丅
  杮彂偼丄I/O儗僕僗僞僼傽僀儖偺僼傽僀儖峔惉丄曄悢偺愰尵丄偍傛傃掕媊撪梕傪愢柧偟
偰偄傑偡丅




I/O儗僕僗僞僼傽僀儖傪偛棙梡偄偨偩偔応崌偺拲堄

  丒  I/O儗僕僗僞僼傽僀儖偼丄懳徾昳庬傪尷掕偟偰採嫙偟偰偄傑偡丅偟偨偑偭偰丄懠偺
    昳庬偵墳梡偝傟傞応崌偵偼丄採嫙偟偰偄傞昳庬偺僾儘僌儔儉傪嶲峫偵偟偰丄奩摉偡
    傞昳庬偺I/O儗僕僗僞僼傽僀儖傪嶌惉偟偰壓偝偄丅

  丒  I/O儗僕僗僞僼傽僀儖傪巊梡偟偰丄I/O儗僕僗僞偺憖嶌傪峴偆僾儘僌儔儉傪婰弎偡
    傞応崌丄I/O儗僕僗僞偺傾僋僙僗弴彉丄僞僀儈儞僌摍傪僔僗僥儉揑偵峫椂偡傞昁梫偑
    偁傝傑偡偺偱丄僴乕僪僂僃傾儅僯儏傾儖傪嶲徠偟偰壓偝偄丅

  丒  I/O儗僕僗僞僼傽僀儖偼丄墳梡僾儘僌儔儉傪奐敪偡傞帪偵丄栶棫偰偰偄偨偩偔偨傔
    偵嶌惉偟偨嶲峫僾儘僌儔儉偱偡丅尩枾偵偼丄屄乆偺僔僗僥儉偵墳偠偰僾儘僌儔儉偵
    庤傪壛偊傞昁梫偑弌偰偔傞応崌傕偁傝傑偡偺偱丄偛巊梡偺嵺偵偼廫暘昡壙偺忋偛巊
    梡壓偝偄丅

  丒  I/O儗僕僗僞僼傽僀儖偺岆傝偵偮偄偰偼丄愑擟傪晧偄偐偹傞応崌偑偁傝丄傑偨岆傝
    偑敪尒偝傟偰傕捈偪偵廋惓偱偒側偄応崌偑偁傝傑偡偺偱偛椆彸壓偝偄丅

仭嶲徠儅僯儏傾儖堦棗

  MB95630僔儕乕僘梡僒儞僾儖I/O儗僕僗僞僼傽僀儖(V01L02)偼丄埲壓偺僴乕僪僂僃傾
儅僯儏傾儖傪婎偵嶌惉偝傟偰偄傑偡丅

  丒乽MB95630H 僔儕乕僘 僴乕僪僂僃傾儅僯儏傾儖(MN702-00009-1v0-J)乿

栚師

戞侾復  I/O儗僕僗僞僼傽僀儖峔惉

戞俀復  I/O儗僕僗僞僼傽僀儖巊梡曽朄

戞俁復  I/O儗僕僗僞愰尵僼傽僀儖偺愰尵撪梕

戞係復  MB95630僔儕乕僘偱巊梡壜擻側僔儞儃儖柤偍傛傃儅僋儘柤

戞侾復  I/O儗僕僗僞僼傽僀儖峔惉

 ${FETOOL}              仼娐嫬曄悢'FETOOL'偵愝掕偝傟偰偄傞僨傿儗僋僩儕
  劘lib
    劘896
      劘include
        劘sample
          劘MB95630
            劙_f2mc8fx.h乮I/O儗僕僗僞愰尵僼傽僀儖乯
            劔
            劙mb95630.h乮MB95630僔儕乕僘梡I/O儗僕僗僞愰尵僼傽僀儖乯
            劔
            劘_f2mc8fx.c乮I/O儗僕僗僞掕媊僼傽僀儖乯

  仭I/O儗僕僗僞愰尵僼傽僀儖

      I/O儗僕僗僞曄悢乮I/O儗僕僗僞偵懳墳偡傞曄悢乯愰尵僼傽僀儖偱偡丅
    I/O儗僕僗僞傪憖嶌偡傞僾儘僌儔儉傪婰弎偡傞帪偼丄偙偺僼傽僀儖傪僀儞僋儖乕僪
    偟偰壓偝偄丅

  仭MB95630僔儕乕僘梡I/O儗僕僗僞愰尵僼傽僀儖

      MB95630僔儕乕僘偺I/O儗僕僗僞曄悢愰尵僼傽僀儖偱偡丅

  仭I/O儗僕僗僞掕媊僼傽僀儖

      MB95630僔儕乕僘偺I/O儗僕僗僞曄悢傪掕媊偟偰偄傞僼傽僀儖偱偡丅

戞俀復  I/O儗僕僗僞僼傽僀儖巊梡曽朄

  (1) 巊梡偡傞昳庬傪-cpu僆僾僔儑儞偵巜掕偟偰丄I/O儗僕僗僞掕媊僼傽僀儖傪僐儞
      僷僀儖偟偰壓偝偄丅

        椺丗 > fcc896s  -cpu mb***** -c _f2mc8fx.c

  (2) I/O儗僕僗僞曄悢傪嶲徠偡傞墳梡僾儘僌儔儉傪婰弎偡傞応崌丄I/O儗僕僗僞愰尵
      僼傽僀儖傪僀儞僋儖乕僪偟偰壓偝偄丅

        椺丗#include "_f2mc8fx.h"

            void func(){
                    .....
                IO_TCCS.bit.MODE = 1;
                    .....
            }

  (3) 巊梡偡傞昳庬傪-cpu僆僾僔儑儞偵巜掕偟偰丄墳梡僾儘僌儔儉傪僐儞僷僀儖偟偰
      壓偝偄丅

        椺丗 > fcc896s  -cpu mb***** -c sample.c

        拲) CPU僆僾僔儑儞偱巜掕偟偨昳庬偑丄I/O儗僕僗僞僼傽僀儖偑巊梡壜擻側昳庬
            偱側偄応崌丄僐儞僷僀儖帪偵壓婰偺僄儔乕儊僢僙乕僕傪弌椡偟傑偡丅

              #error "The I/O register file of the specified CPU option
                      does not exist"

  (4) 巊梡偡傞昳庬傪-cpu僆僾僔儑儞偵巜掕偟偰丄(1)偱嶌惉偟偨僆僽僕僃僋僩僼傽
      僀儖偲丄(3)偱嶌惉偟偨墳梡僾儘僌儔儉偺僆僽僕僃僋僩僼傽僀儖傪儕儞僋偟偰
      壓偝偄丅

        椺丗 > flnk896s -cpu mb***** -o sample.abs *.obj  -sc IO/IO=0x0000

        拲) "-sc IO/IO=0x0000" 偺曗懌愢柧

            埲壓偺Warning傪梷巭偡傞偨傔偵杮愝掕傪峴偭偰壓偝偄丅

            椺丗 儕儞僋偟偰偄傑偡...
                 *** W1373L: IO椞堟奜傊偺攝抲偱偡 (IO)

            Workbench偱偼丄埲壓偺傛偆偵愝掕偟偰壓偝偄丅

            [僾儘僕僃僋僩(P)]-[僾儘僕僃僋僩偺愝掕(J)]偺儕儞僇僞僌偱丄

            a)  僇僥僑儕(Y)偺乽攝抲/寢崌乿偱[僙僋僔儑儞愝掕]傪僋儕僢僋
            b)  ROM/RAM椞堟柤(R)傪乽傾僪儗僗偱巜掕乿偵曄峏
            c)  僙僋僔儑儞柤(S)偵乽IO乿傪擖椡
            d)  傾僪儗僗(A)偵乽0x0000乿傪擖椡
            e)  撪梕庬暿(T)偵乽IO乿傪慖戰
            f)  [愝掕(E)]傪僋儕僢僋
            g)  [OK]傪僋儕僢僋

            [僾儘僕僃僋僩偺愝掕(J)]偺[OK]傪僋儕僢僋偟偰廔椆

戞俁復  I/O儗僕僗僞愰尵僼傽僀儖偺愰尵撪梕

  僴乕僪僂僃傾儅僯儏傾儖偵婰嵹偝傟偰偄傞I/O儗僕僗僞柤媦傃價僢僩柤偵懳墳偡傞丄
I/O儗僕僗僞曄悢偍傛傃價僢僩僼傿乕儖僪儊儞僶傪丄埲壓偺傛偆偵愰尵偟偰偄傑偡丅

  仭價僢僩扨埵丄傑偨偼僶僀僩乛儚乕僪扨埵偱傾僋僙僗壜擻側I/O儗僕僗僞曄悢偼丄
    嫟梡懱宆 (堦晹傾僋僙僗偺搒崌忋丄峔憿懱宆) 偱愰尵

  仭慡價僢僩偑彂崬傒愱梡丄傑偨偼價僢僩扨埵偱傾僋僙僗偡傞堄枴偑側偄I/O儗僕僗僞
    曄悢偼丄惍悢宆偱愰尵

  仭I/O儗僕僗僞曄悢柤偼丄婎杮揑偵懳墳偡傞I/O儗僕僗僞柤偺愭摢偵 'IO_'傪晅壛偟
    偨宍偱愰尵乮堦晹丄俠尵岅曄悢愰尵忋偺栤戣傗丄傾僋僙僗偺搒崌側偳偱丄暋悢偺
    I/O儗僕僗僞傪侾偮偺曄悢柤偱愰尵偟偨傝丄曄悢柤傪庒姳曄峏偟偰愰尵乯

  仭價僢僩僼傿乕儖僪儊儞僶柤偼丄懳墳偡傞價僢僩柤偱愰尵
     (堦晹丄傾僋僙僗偺搒崌忋丄暋悢偺價僢僩傪侾偮偺儊儞僶柤偱愰尵) 


  亂椺亃I/O儗僕僗僞PDR0偵懳偡傞愰尵撪梕

    丒I/O儗僕僗僞峔惉

          7       6       5       4       3       2       1       0    bit No.
      劕劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劧劒劒劒劖
      劔  P07 劆  P06 劆  P05 劆  P04 劆  P03 劆  P02 劆  P01 劆  P00 劔PDR0
      劘劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劯劒劒劒劗

    丒愰尵撪梕

        typedef union {
                unsigned char    byte;
                struct {
                        unsigned char    P00:1;
                        unsigned char    P01:1;
                        unsigned char    P02:1;
                        unsigned char    P03:1;
                        unsigned char    P04:1;
                        unsigned char    P05:1;
                        unsigned char    P06:1;
                        unsigned char    P07:1;
                } bit;
        } PDR0STR;

        extern __io PDR0STR IO_PDR0;
        #define _pdr0    IO_PDR0
        #define PDR0     IO_PDR0.byte
        #define PDR0_P00 IO_PDR0.bit.P00
        #define PDR0_P01 IO_PDR0.bit.P01
        #define PDR0_P02 IO_PDR0.bit.P02
        #define PDR0_P03 IO_PDR0.bit.P03
        #define PDR0_P04 IO_PDR0.bit.P04
        #define PDR0_P05 IO_PDR0.bit.P05
        #define PDR0_P06 IO_PDR0.bit.P06
        #define PDR0_P07 IO_PDR0.bit.P07

  亙拲堄帠崁亜

        __io宆廋忺巕偑巜掕偝傟偨I/O偺價僢僩僼傿乕儖僪儊儞僶偵丄曄悢偺抣傪戙擖
      偡傞帪偼丄儕乕僪儌僨傿僼傽僀儔僀僩(RMW)宯柦椷(SETB,CLRB)偱偼側偔丄儘乕僪
      仺AND/OR仺僗僩傾張棟偲側傝傑偡丅
        儘乕僪仺AND/OR仺僗僩傾張棟拞偵丄偁傞摿掕偺價僢僩偑彂偒姺傢偭偨応崌偵丄
      梊婜偣偸岆徚嫀丄岆彂偒姺偊偑敪惗偡傞応崌偑偁傝傑偡丅
        偙傟傪杊巭偡傞偨傔偵丄戙擖偡傞曄悢偵偮偄偰偺0/1敾掕傪峴偄丄掕悢抣偱
      彂崬傒傪峴偆傛偆偵婰弎偟偰壓偝偄丅
        偨偩偟丄奼挘I/O椞堟(0F80H-0FFFH)偺応崌偼丄儕乕僪儌僨傿僼傽僀儔僀僩(RMW)
      宯柦椷(SETB,CLRB)偼丄惗惉偱偒傑偣傫丅

  亂椺亃I/O偺價僢僩僼傿乕儖僪儊儞僶偵曄悢傪戙擖偡傞椺丅

          埲壓偺傛偆偵婰弎偡傞偲丄儘乕僪仺AND/OR仺僗僩傾張棟偲側傞偨傔丄
        梊婜偣偸岆徚嫀丄岆彂偒姺偊偑敪惗偡傞応崌偑偁傝傑偡丅

        [C婰弎椺]
            IO_PDR0.bit.P00 = RAM_A;

        [ASM弌椡椺]
                    MOV     A, _RAM_A
                    AND     A, #1
                    MOV     A, _IO_PDR0
                    AND     A, #254
                    OR      A
                    MOV     _IO_PDR0, A

          偙傟傪夞旔偡傞偨傔偵丄戙擖偡傞曄悢偵偮偄偰偺0/1敾掕傪峴偄丄掕悢抣偱
        彂偒崬傓傛偆偵婰弎偟偰壓偝偄丅儕乕僪儌僨傿僼傽僀儔僀僩(RMW)宯柦椷(SETB,
        CLRB)偑弌椡偝傟丄梊婜偣偸岆徚嫀丄岆彂偒姺偊傪杊巭偱偒傑偡丅

        [儕乕僪儌僨傿僼傽僀儔僀僩(RMW)宯柦椷(SETB,CLRB)偑弌椡偝傟傞忦審]
            (1) I/O傪帵偡價僢僩僼傿乕儖僪偺宆偼丄1僶僀僩宆(char, signed char,
                unsigned char)偱偁傞丅偐偮
            (2) I/O傪帵偡價僢僩僼傿乕儖僪儊儞僶偺暆偼丄1價僢僩偱偁傞丅偐偮
            (3) 僟僀儗僋僩傾僪儗僔儞僌椞堟(0000H-007FH)偺I/O椞堟偵偁傞I/O儗僕
                僗僞偱偁傞丅

        [C婰弎椺]
            if (RAM_A) {
                IO_PDR0.bit.P00 = 1;
            } else {
                IO_PDR0.bit.P00 = 0;
            }

        [ASM弌椡椺]
                    MOV     A, _RAM_A
                    BEQ16   L_23
                    SETB    _IO_PDR0:0
                    JMP     L_24
            L_23:
                    CLRB    _IO_PDR0:0
            L_24:
                    RET

戞係復  MB95630僔儕乕僘偱巊梡壜擻側僔儞儃儖柤偍傛傃儅僋儘柤

  I/O儗僕僗僞柤 : PDR0                        傾僪儗僗丗0x0
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PDR0.byte                PDR0                          
  價僢僩          IO_PDR0.bit.P00             PDR0_P00                      
                  IO_PDR0.bit.P01             PDR0_P01                      
                  IO_PDR0.bit.P02             PDR0_P02                      
                  IO_PDR0.bit.P03             PDR0_P03                      
                  IO_PDR0.bit.P04             PDR0_P04                      
                  IO_PDR0.bit.P05             PDR0_P05                      
                  IO_PDR0.bit.P06             PDR0_P06                      
                  IO_PDR0.bit.P07             PDR0_P07                      
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : DDR0                        傾僪儗僗丗0x1
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_DDR0.byte                DDR0                          
  價僢僩          IO_DDR0.bit.P00             DDR0_P00                      
                  IO_DDR0.bit.P01             DDR0_P01                      
                  IO_DDR0.bit.P02             DDR0_P02                      
                  IO_DDR0.bit.P03             DDR0_P03                      
                  IO_DDR0.bit.P04             DDR0_P04                      
                  IO_DDR0.bit.P05             DDR0_P05                      
                  IO_DDR0.bit.P06             DDR0_P06                      
                  IO_DDR0.bit.P07             DDR0_P07                      
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : PDR1                        傾僪儗僗丗0x2
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PDR1.byte                PDR1                          
  價僢僩          IO_PDR1.bit.P10             PDR1_P10                      
                  IO_PDR1.bit.P11             PDR1_P11                      
                  IO_PDR1.bit.P12             PDR1_P12                      
                  IO_PDR1.bit.P13             PDR1_P13                      
                  IO_PDR1.bit.P14             PDR1_P14                      
                  IO_PDR1.bit.P15             PDR1_P15                      
                  IO_PDR1.bit.P16             PDR1_P16                      
                  IO_PDR1.bit.P17             PDR1_P17                      
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : DDR1                        傾僪儗僗丗0x3
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_DDR1.byte                DDR1                          
  價僢僩          IO_DDR1.bit.P10             DDR1_P10                      
                  IO_DDR1.bit.P11             DDR1_P11                      
                  IO_DDR1.bit.P12             DDR1_P12                      
                  IO_DDR1.bit.P13             DDR1_P13                      
                  IO_DDR1.bit.P14             DDR1_P14                      
                  IO_DDR1.bit.P15             DDR1_P15                      
                  IO_DDR1.bit.P16             DDR1_P16                      
                  IO_DDR1.bit.P17             DDR1_P17                      
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : WATR                        傾僪儗僗丗0x5
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_WATR.byte                WATR                          
  價僢僩          IO_WATR.bit.MWT0            WATR_MWT0                     
                  IO_WATR.bit.MWT1            WATR_MWT1                     
                  IO_WATR.bit.MWT2            WATR_MWT2                     
                  IO_WATR.bit.MWT3            WATR_MWT3                     
                  IO_WATR.bit.SWT0            WATR_SWT0                     
                  IO_WATR.bit.SWT1            WATR_SWT1                     
                  IO_WATR.bit.SWT2            WATR_SWT2                     
                  IO_WATR.bit.SWT3            WATR_SWT3                     
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : PLLC                        傾僪儗僗丗0x6
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PLLC.byte                PLLC                          
  價僢僩          IO_PLLC.bit.MPRDY           PLLC_MPRDY                    
                  IO_PLLC.bit.MPMC0           PLLC_MPMC0                    
                  IO_PLLC.bit.MPMC1           PLLC_MPMC1                    
                  IO_PLLC.bit.MPEN            PLLC_MPEN                     
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : SYCC                        傾僪儗僗丗0x7
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_SYCC.byte                SYCC                          
  價僢僩          IO_SYCC.bit.DIV0            SYCC_DIV0                     
                  IO_SYCC.bit.DIV1            SYCC_DIV1                     
                  IO_SYCC.bit.SCS0            SYCC_SCS0                     
                  IO_SYCC.bit.SCS1            SYCC_SCS1                     
                  IO_SYCC.bit.SCS2            SYCC_SCS2                     
                  IO_SYCC.bit.SCM0            SYCC_SCM0                     
                  IO_SYCC.bit.SCM1            SYCC_SCM1                     
                  IO_SYCC.bit.SCM2            SYCC_SCM2                     
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : STBC                        傾僪儗僗丗0x8
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_STBC.byte                STBC                          
  價僢僩          IO_STBC.bit.TMD             STBC_TMD                      
                  IO_STBC.bit.SRST            STBC_SRST                     
                  IO_STBC.bit.SPL             STBC_SPL                      
                  IO_STBC.bit.SLP             STBC_SLP                      
                  IO_STBC.bit.STP             STBC_STP                      
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : RSRR                        傾僪儗僗丗0x9
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_RSRR.byte                RSRR                          
  價僢僩          IO_RSRR.bit.SWR             RSRR_SWR                      
                  IO_RSRR.bit.HWR             RSRR_HWR                      
                  IO_RSRR.bit.PONR            RSRR_PONR                     
                  IO_RSRR.bit.WDTR            RSRR_WDTR                     
                  IO_RSRR.bit.EXTS            RSRR_EXTS                     
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : TBTC                        傾僪儗僗丗0xa
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_TBTC.byte                TBTC                          
  價僢僩          IO_TBTC.bit.TCLR            TBTC_TCLR                     
                  IO_TBTC.bit.TBC0            TBTC_TBC0                     
                  IO_TBTC.bit.TBC1            TBTC_TBC1                     
                  IO_TBTC.bit.TBC2            TBTC_TBC2                     
                  IO_TBTC.bit.TBC3            TBTC_TBC3                     
                  IO_TBTC.bit.TBIE            TBTC_TBIE                     
                  IO_TBTC.bit.TBIF            TBTC_TBIF                     
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : WPCR                        傾僪儗僗丗0xb
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_WPCR.byte                WPCR                          
  價僢僩          IO_WPCR.bit.WCLR            WPCR_WCLR                     
                  IO_WPCR.bit.WTC0            WPCR_WTC0                     
                  IO_WPCR.bit.WTC1            WPCR_WTC1                     
                  IO_WPCR.bit.WTC2            WPCR_WTC2                     
                  IO_WPCR.bit.WTIE            WPCR_WTIE                     
                  IO_WPCR.bit.WTIF            WPCR_WTIF                     
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : WDTC                        傾僪儗僗丗0xc
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_WDTC.byte                WDTC                          
  價僢僩          IO_WDTC.bit.WTE0            WDTC_WTE0                     
                  IO_WDTC.bit.WTE1            WDTC_WTE1                     
                  IO_WDTC.bit.WTE2            WDTC_WTE2                     
                  IO_WDTC.bit.WTE3            WDTC_WTE3                     
                  IO_WDTC.bit.HWWDT           WDTC_HWWDT                    
                  IO_WDTC.bit.CSP             WDTC_CSP                      
                  IO_WDTC.bit.CS0             WDTC_CS0                      
                  IO_WDTC.bit.CS1             WDTC_CS1                      
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : SYCC2                       傾僪儗僗丗0xd
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_SYCC2.byte               SYCC2                         
  價僢僩          IO_SYCC2.bit.MCRE           SYCC2_MCRE                    
                  IO_SYCC2.bit.SCRE           SYCC2_SCRE                    
                  IO_SYCC2.bit.MOSCE          SYCC2_MOSCE                   
                  IO_SYCC2.bit.SOSCE          SYCC2_SOSCE                   
                  IO_SYCC2.bit.MCRDY          SYCC2_MCRDY                   
                  IO_SYCC2.bit.SCRDY          SYCC2_SCRDY                   
                  IO_SYCC2.bit.MRDY           SYCC2_MRDY                    
                  IO_SYCC2.bit.SRDY           SYCC2_SRDY                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : STBC2                       傾僪儗僗丗0xe
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_STBC2.byte               STBC2                         
  價僢僩          IO_STBC2.bit.DSTBYX         STBC2_DSTBYX                  
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : PDR6                        傾僪儗僗丗0x16
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PDR6.byte                PDR6                          
  價僢僩          IO_PDR6.bit.P60             PDR6_P60                      
                  IO_PDR6.bit.P61             PDR6_P61                      
                  IO_PDR6.bit.P62             PDR6_P62                      
                  IO_PDR6.bit.P63             PDR6_P63                      
                  IO_PDR6.bit.P64             PDR6_P64                      
                  IO_PDR6.bit.P65             PDR6_P65                      
                  IO_PDR6.bit.P66             PDR6_P66                      
                  IO_PDR6.bit.P67             PDR6_P67                      
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : DDR6                        傾僪儗僗丗0x17
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_DDR6.byte                DDR6                          
  價僢僩          IO_DDR6.bit.P60             DDR6_P60                      
                  IO_DDR6.bit.P61             DDR6_P61                      
                  IO_DDR6.bit.P62             DDR6_P62                      
                  IO_DDR6.bit.P63             DDR6_P63                      
                  IO_DDR6.bit.P64             DDR6_P64                      
                  IO_DDR6.bit.P65             DDR6_P65                      
                  IO_DDR6.bit.P66             DDR6_P66                      
                  IO_DDR6.bit.P67             DDR6_P67                      
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : PDRF                        傾僪儗僗丗0x28
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PDRF.byte                PDRF                          
  價僢僩          IO_PDRF.bit.PF0             PDRF_PF0                      
                  IO_PDRF.bit.PF1             PDRF_PF1                      
                  IO_PDRF.bit.PF2             PDRF_PF2                      
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : DDRF                        傾僪儗僗丗0x29
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_DDRF.byte                DDRF                          
  價僢僩          IO_DDRF.bit.PF0             DDRF_PF0                      
                  IO_DDRF.bit.PF1             DDRF_PF1                      
                  IO_DDRF.bit.PF2             DDRF_PF2                      
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : PDRG                        傾僪儗僗丗0x2a
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PDRG.byte                PDRG                          
  價僢僩          IO_PDRG.bit.PG1             PDRG_PG1                      
                  IO_PDRG.bit.PG2             PDRG_PG2                      
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : DDRG                        傾僪儗僗丗0x2b
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_DDRG.byte                DDRG                          
  價僢僩          IO_DDRG.bit.PG1             DDRG_PG1                      
                  IO_DDRG.bit.PG2             DDRG_PG2                      
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : PUL0                        傾僪儗僗丗0x2c
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PUL0.byte                PUL0                          
  價僢僩          IO_PUL0.bit.P00             PUL0_P00                      
                  IO_PUL0.bit.P01             PUL0_P01                      
                  IO_PUL0.bit.P02             PUL0_P02                      
                  IO_PUL0.bit.P03             PUL0_P03                      
                  IO_PUL0.bit.P04             PUL0_P04                      
                  IO_PUL0.bit.P05             PUL0_P05                      
                  IO_PUL0.bit.P06             PUL0_P06                      
                  IO_PUL0.bit.P07             PUL0_P07                      
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : PUL1                        傾僪儗僗丗0x2d
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PUL1.byte                PUL1                          
  價僢僩          IO_PUL1.bit.P10             PUL1_P10                      
                  IO_PUL1.bit.P11             PUL1_P11                      
                  IO_PUL1.bit.P12             PUL1_P12                      
                  IO_PUL1.bit.P13             PUL1_P13                      
                  IO_PUL1.bit.P14             PUL1_P14                      
                  IO_PUL1.bit.P15             PUL1_P15                      
                  IO_PUL1.bit.P16             PUL1_P16                      
                  IO_PUL1.bit.P17             PUL1_P17                      
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : PUL6                        傾僪儗僗丗0x33
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PUL6.byte                PUL6                          
  價僢僩          IO_PUL6.bit.P62             PUL6_P62                      
                  IO_PUL6.bit.P63             PUL6_P63                      
                  IO_PUL6.bit.P64             PUL6_P64                      
                  IO_PUL6.bit.P65             PUL6_P65                      
                  IO_PUL6.bit.P66             PUL6_P66                      
                  IO_PUL6.bit.P67             PUL6_P67                      
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : PULG                        傾僪儗僗丗0x35
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PULG.byte                PULG                          
  價僢僩          IO_PULG.bit.PG1             PULG_PG1                      
                  IO_PULG.bit.PG2             PULG_PG2                      
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : T01CR1                      傾僪儗僗丗0x36
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_T01CR1.byte              T01CR1                        
  價僢僩          IO_T01CR1.bit.OE            T01CR1_OE                     
                  IO_T01CR1.bit.SO            T01CR1_SO                     
                  IO_T01CR1.bit.IF            T01CR1_IF                     
                  IO_T01CR1.bit.BF            T01CR1_BF                     
                  IO_T01CR1.bit.IR            T01CR1_IR                     
                  IO_T01CR1.bit.IE            T01CR1_IE                     
                  IO_T01CR1.bit.HO            T01CR1_HO                     
                  IO_T01CR1.bit.STA           T01CR1_STA                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : T00CR1                      傾僪儗僗丗0x37
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_T00CR1.byte              T00CR1                        
  價僢僩          IO_T00CR1.bit.OE            T00CR1_OE                     
                  IO_T00CR1.bit.SO            T00CR1_SO                     
                  IO_T00CR1.bit.IF            T00CR1_IF                     
                  IO_T00CR1.bit.BF            T00CR1_BF                     
                  IO_T00CR1.bit.IR            T00CR1_IR                     
                  IO_T00CR1.bit.IE            T00CR1_IE                     
                  IO_T00CR1.bit.HO            T00CR1_HO                     
                  IO_T00CR1.bit.STA           T00CR1_STA                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : T11CR1                      傾僪儗僗丗0x38
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_T11CR1.byte              T11CR1                        
  價僢僩          IO_T11CR1.bit.OE            T11CR1_OE                     
                  IO_T11CR1.bit.SO            T11CR1_SO                     
                  IO_T11CR1.bit.IF            T11CR1_IF                     
                  IO_T11CR1.bit.BF            T11CR1_BF                     
                  IO_T11CR1.bit.IR            T11CR1_IR                     
                  IO_T11CR1.bit.IE            T11CR1_IE                     
                  IO_T11CR1.bit.HO            T11CR1_HO                     
                  IO_T11CR1.bit.STA           T11CR1_STA                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : T10CR1                      傾僪儗僗丗0x39
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_T10CR1.byte              T10CR1                        
  價僢僩          IO_T10CR1.bit.OE            T10CR1_OE                     
                  IO_T10CR1.bit.SO            T10CR1_SO                     
                  IO_T10CR1.bit.IF            T10CR1_IF                     
                  IO_T10CR1.bit.BF            T10CR1_BF                     
                  IO_T10CR1.bit.IR            T10CR1_IR                     
                  IO_T10CR1.bit.IE            T10CR1_IE                     
                  IO_T10CR1.bit.HO            T10CR1_HO                     
                  IO_T10CR1.bit.STA           T10CR1_STA                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : PC01                        傾僪儗僗丗0x3a
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PC01.byte                PC01                          
  價僢僩          IO_PC01.bit.CKS10           PC01_CKS10                    
                  IO_PC01.bit.CKS11           PC01_CKS11                    
                  IO_PC01.bit.CKS12           PC01_CKS12                    
                  IO_PC01.bit.POEN1           PC01_POEN1                    
                  IO_PC01.bit.PUF1            PC01_PUF1                     
                  IO_PC01.bit.PIE1            PC01_PIE1                     
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : PC00                        傾僪儗僗丗0x3b
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PC00.byte                PC00                          
  價僢僩          IO_PC00.bit.CKS00           PC00_CKS00                    
                  IO_PC00.bit.CKS01           PC00_CKS01                    
                  IO_PC00.bit.CKS02           PC00_CKS02                    
                  IO_PC00.bit.POEN0           PC00_POEN0                    
                  IO_PC00.bit.PUF0            PC00_PUF0                     
                  IO_PC00.bit.PIE0            PC00_PIE0                     
                  IO_PC00.bit.MD0             PC00_MD0                      
                  IO_PC00.bit.MD1             PC00_MD1                      
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : PC11                        傾僪儗僗丗0x3c
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PC11.byte                PC11                          
  價僢僩          IO_PC11.bit.CKS10           PC11_CKS10                    
                  IO_PC11.bit.CKS11           PC11_CKS11                    
                  IO_PC11.bit.CKS12           PC11_CKS12                    
                  IO_PC11.bit.POEN1           PC11_POEN1                    
                  IO_PC11.bit.PUF1            PC11_PUF1                     
                  IO_PC11.bit.PIE1            PC11_PIE1                     
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : PC10                        傾僪儗僗丗0x3d
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PC10.byte                PC10                          
  價僢僩          IO_PC10.bit.CKS00           PC10_CKS00                    
                  IO_PC10.bit.CKS01           PC10_CKS01                    
                  IO_PC10.bit.CKS02           PC10_CKS02                    
                  IO_PC10.bit.POEN0           PC10_POEN0                    
                  IO_PC10.bit.PUF0            PC10_PUF0                     
                  IO_PC10.bit.PIE0            PC10_PIE0                     
                  IO_PC10.bit.MD0             PC10_MD0                      
                  IO_PC10.bit.MD1             PC10_MD1                      
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : PC21                        傾僪儗僗丗0x3e
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PC21.byte                PC21                          
  價僢僩          IO_PC21.bit.CKS10           PC21_CKS10                    
                  IO_PC21.bit.CKS11           PC21_CKS11                    
                  IO_PC21.bit.CKS12           PC21_CKS12                    
                  IO_PC21.bit.POEN1           PC21_POEN1                    
                  IO_PC21.bit.PUF1            PC21_PUF1                     
                  IO_PC21.bit.PIE1            PC21_PIE1                     
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : PC20                        傾僪儗僗丗0x3f
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PC20.byte                PC20                          
  價僢僩          IO_PC20.bit.CKS00           PC20_CKS00                    
                  IO_PC20.bit.CKS01           PC20_CKS01                    
                  IO_PC20.bit.CKS02           PC20_CKS02                    
                  IO_PC20.bit.POEN0           PC20_POEN0                    
                  IO_PC20.bit.PUF0            PC20_PUF0                     
                  IO_PC20.bit.PIE0            PC20_PIE0                     
                  IO_PC20.bit.MD0             PC20_MD0                      
                  IO_PC20.bit.MD1             PC20_MD1                      
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : TMCSRH1                     傾僪儗僗丗0x40
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_TMCSRH1.byte             TMCSRH1                       
  價僢僩          IO_TMCSRH1.bit.MOD0         TMCSRH1_MOD0                  
                  IO_TMCSRH1.bit.MOD1         TMCSRH1_MOD1                  
                  IO_TMCSRH1.bit.MOD2         TMCSRH1_MOD2                  
                  IO_TMCSRH1.bit.CSL0         TMCSRH1_CSL0                  
                  IO_TMCSRH1.bit.CSL1         TMCSRH1_CSL1                  
                  IO_TMCSRH1.bit.CSL2         TMCSRH1_CSL2                  
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : TMCSRL1                     傾僪儗僗丗0x41
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_TMCSRL1.byte             TMCSRL1                       
  價僢僩          IO_TMCSRL1.bit.TRG          TMCSRL1_TRG                   
                  IO_TMCSRL1.bit.CNTE         TMCSRL1_CNTE                  
                  IO_TMCSRL1.bit.UF           TMCSRL1_UF                    
                  IO_TMCSRL1.bit.INTE         TMCSRL1_INTE                  
                  IO_TMCSRL1.bit.RELD         TMCSRL1_RELD                  
                  IO_TMCSRL1.bit.OUTL         TMCSRL1_OUTL                  
                  IO_TMCSRL1.bit.OUTE         TMCSRL1_OUTE                  
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : CMR0C                       傾僪儗僗丗0x42
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_CMR0C.byte               CMR0C                         
  價僢僩          IO_CMR0C.bit.PD             CMR0C_PD                      
                  IO_CMR0C.bit.VCOE           CMR0C_VCOE                    
                  IO_CMR0C.bit.VCID           CMR0C_VCID                    
                  IO_CMR0C.bit.IE             CMR0C_IE                      
                  IO_CMR0C.bit.IF             CMR0C_IF                      
                  IO_CMR0C.bit.OS             CMR0C_OS                      
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : PCNTH1                      傾僪儗僗丗0x44
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PCNTH1.byte              PCNTH1                        
  價僢僩          IO_PCNTH1.bit.PGMS          PCNTH1_PGMS                   
                  IO_PCNTH1.bit.CKS0          PCNTH1_CKS0                   
                  IO_PCNTH1.bit.CKS1          PCNTH1_CKS1                   
                  IO_PCNTH1.bit.CKS2          PCNTH1_CKS2                   
                  IO_PCNTH1.bit.RTRG          PCNTH1_RTRG                   
                  IO_PCNTH1.bit.MDSE          PCNTH1_MDSE                   
                  IO_PCNTH1.bit.STRG          PCNTH1_STRG                   
                  IO_PCNTH1.bit.CNTE          PCNTH1_CNTE                   
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : PCNTL1                      傾僪儗僗丗0x45
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PCNTL1.byte              PCNTL1                        
  價僢僩          IO_PCNTL1.bit.OSEL          PCNTL1_OSEL                   
                  IO_PCNTL1.bit.POEN          PCNTL1_POEN                   
                  IO_PCNTL1.bit.IRS0          PCNTL1_IRS0                   
                  IO_PCNTL1.bit.IRS1          PCNTL1_IRS1                   
                  IO_PCNTL1.bit.IRQF          PCNTL1_IRQF                   
                  IO_PCNTL1.bit.IREN          PCNTL1_IREN                   
                  IO_PCNTL1.bit.EGS0          PCNTL1_EGS0                   
                  IO_PCNTL1.bit.EGS1          PCNTL1_EGS1                   
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : EIC00                       傾僪儗僗丗0x48
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_EIC00.byte               EIC00                         
  價僢僩          IO_EIC00.bit.EIE0           EIC00_EIE0                    
                  IO_EIC00.bit.SL00           EIC00_SL00                    
                  IO_EIC00.bit.SL01           EIC00_SL01                    
                  IO_EIC00.bit.EIR0           EIC00_EIR0                    
                  IO_EIC00.bit.EIE1           EIC00_EIE1                    
                  IO_EIC00.bit.SL10           EIC00_SL10                    
                  IO_EIC00.bit.SL11           EIC00_SL11                    
                  IO_EIC00.bit.EIR1           EIC00_EIR1                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : EIC10                       傾僪儗僗丗0x49
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_EIC10.byte               EIC10                         
  價僢僩          IO_EIC10.bit.EIE0           EIC10_EIE0                    
                  IO_EIC10.bit.SL00           EIC10_SL00                    
                  IO_EIC10.bit.SL01           EIC10_SL01                    
                  IO_EIC10.bit.EIR0           EIC10_EIR0                    
                  IO_EIC10.bit.EIE1           EIC10_EIE1                    
                  IO_EIC10.bit.SL10           EIC10_SL10                    
                  IO_EIC10.bit.SL11           EIC10_SL11                    
                  IO_EIC10.bit.EIR1           EIC10_EIR1                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : EIC20                       傾僪儗僗丗0x4a
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_EIC20.byte               EIC20                         
  價僢僩          IO_EIC20.bit.EIE0           EIC20_EIE0                    
                  IO_EIC20.bit.SL00           EIC20_SL00                    
                  IO_EIC20.bit.SL01           EIC20_SL01                    
                  IO_EIC20.bit.EIR0           EIC20_EIR0                    
                  IO_EIC20.bit.EIE1           EIC20_EIE1                    
                  IO_EIC20.bit.SL10           EIC20_SL10                    
                  IO_EIC20.bit.SL11           EIC20_SL11                    
                  IO_EIC20.bit.EIR1           EIC20_EIR1                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : EIC30                       傾僪儗僗丗0x4b
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_EIC30.byte               EIC30                         
  價僢僩          IO_EIC30.bit.EIE0           EIC30_EIE0                    
                  IO_EIC30.bit.SL00           EIC30_SL00                    
                  IO_EIC30.bit.SL01           EIC30_SL01                    
                  IO_EIC30.bit.EIR0           EIC30_EIR0                    
                  IO_EIC30.bit.EIE1           EIC30_EIE1                    
                  IO_EIC30.bit.SL10           EIC30_SL10                    
                  IO_EIC30.bit.SL11           EIC30_SL11                    
                  IO_EIC30.bit.EIR1           EIC30_EIR1                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : EIC01                       傾僪儗僗丗0x4c
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_EIC01.byte               EIC01                         
  價僢僩          IO_EIC01.bit.EIE0           EIC01_EIE0                    
                  IO_EIC01.bit.SL00           EIC01_SL00                    
                  IO_EIC01.bit.SL01           EIC01_SL01                    
                  IO_EIC01.bit.EIR0           EIC01_EIR0                    
                  IO_EIC01.bit.EIE1           EIC01_EIE1                    
                  IO_EIC01.bit.SL10           EIC01_SL10                    
                  IO_EIC01.bit.SL11           EIC01_SL11                    
                  IO_EIC01.bit.EIR1           EIC01_EIR1                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : LVDR                        傾僪儗僗丗0x4e
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_LVDR                     LVDR                          
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : SCR                         傾僪儗僗丗0x50
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_SCR.byte                 SCR                           
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : SMR                         傾僪儗僗丗0x51
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_SMR.byte                 SMR                           
  價僢僩          IO_SMR.bit.SOE              SMR_SOE                       
                  IO_SMR.bit.SCKE             SMR_SCKE                      
                  IO_SMR.bit.UPCL             SMR_UPCL                      
                  IO_SMR.bit.REST             SMR_REST                      
                  IO_SMR.bit.EXT              SMR_EXT                       
                  IO_SMR.bit.OTO              SMR_OTO                       
                  IO_SMR.bit.MD0              SMR_MD0                       
                  IO_SMR.bit.MD1              SMR_MD1                       
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : SSR                         傾僪儗僗丗0x52
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_SSR.byte                 SSR                           
  價僢僩          IO_SSR.bit.TIE              SSR_TIE                       
                  IO_SSR.bit.RIE              SSR_RIE                       
                  IO_SSR.bit.BDS              SSR_BDS                       
                  IO_SSR.bit.TDRE             SSR_TDRE                      
                  IO_SSR.bit.RDRF             SSR_RDRF                      
                  IO_SSR.bit.FRE              SSR_FRE                       
                  IO_SSR.bit.ORE              SSR_ORE                       
                  IO_SSR.bit.PE               SSR_PE                        
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : RDR_TDR                     傾僪儗僗丗0x53
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_RDR_TDR                  RDR_TDR                       
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : ESCR                        傾僪儗僗丗0x54
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_ESCR.byte                ESCR                          
  價僢僩          IO_ESCR.bit.SCES            ESCR_SCES                     
                  IO_ESCR.bit.CCO             ESCR_CCO                      
                  IO_ESCR.bit.SIOP            ESCR_SIOP                     
                  IO_ESCR.bit.SOPE            ESCR_SOPE                     
                  IO_ESCR.bit.LBL0            ESCR_LBL0                     
                  IO_ESCR.bit.LBL1            ESCR_LBL1                     
                  IO_ESCR.bit.LBD             ESCR_LBD                      
                  IO_ESCR.bit.LBIE            ESCR_LBIE                     
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : ECCR                        傾僪儗僗丗0x55
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_ECCR.byte                ECCR                          
  價僢僩          IO_ECCR.bit.TBI             ECCR_TBI                      
                  IO_ECCR.bit.RBI             ECCR_RBI                      
                  IO_ECCR.bit.SSM             ECCR_SSM                      
                  IO_ECCR.bit.SCDE            ECCR_SCDE                     
                  IO_ECCR.bit.MS              ECCR_MS                       
                  IO_ECCR.bit.LBR             ECCR_LBR                      
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : SMC10                       傾僪儗僗丗0x56
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_SMC10.byte               SMC10                         
  價僢僩          IO_SMC10.bit.MD             SMC10_MD                      
                  IO_SMC10.bit.CKS            SMC10_CKS                     
                  IO_SMC10.bit.CBL0           SMC10_CBL0                    
                  IO_SMC10.bit.CBL1           SMC10_CBL1                    
                  IO_SMC10.bit.SBL            SMC10_SBL                     
                  IO_SMC10.bit.TDP            SMC10_TDP                     
                  IO_SMC10.bit.PEN            SMC10_PEN                     
                  IO_SMC10.bit.BDS            SMC10_BDS                     
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : SMC20                       傾僪儗僗丗0x57
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_SMC20.byte               SMC20                         
  價僢僩          IO_SMC20.bit.TEIE           SMC20_TEIE                    
                  IO_SMC20.bit.TCIE           SMC20_TCIE                    
                  IO_SMC20.bit.RIE            SMC20_RIE                     
                  IO_SMC20.bit.TXE            SMC20_TXE                     
                  IO_SMC20.bit.RXE            SMC20_RXE                     
                  IO_SMC20.bit.RERC           SMC20_RERC                    
                  IO_SMC20.bit.TXOE           SMC20_TXOE                    
                  IO_SMC20.bit.SCKE           SMC20_SCKE                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : SSR0                        傾僪儗僗丗0x58
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_SSR0.byte                SSR0                          
  價僢僩          IO_SSR0.bit.TDRE            SSR0_TDRE                     
                  IO_SSR0.bit.TCPL            SSR0_TCPL                     
                  IO_SSR0.bit.RDRF            SSR0_RDRF                     
                  IO_SSR0.bit.FER             SSR0_FER                      
                  IO_SSR0.bit.OVE             SSR0_OVE                      
                  IO_SSR0.bit.PER             SSR0_PER                      
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : TDR0                        傾僪儗僗丗0x59
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_TDR0                     TDR0                          
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : RDR0                        傾僪儗僗丗0x5a
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_RDR0                     RDR0                          
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : IBCR00                      傾僪儗僗丗0x60
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_IBCR00.byte              IBCR00                        
  價僢僩          IO_IBCR00.bit.WUE           IBCR00_WUE                    
                  IO_IBCR00.bit.WUF           IBCR00_WUF                    
                  IO_IBCR00.bit.SPE           IBCR00_SPE                    
                  IO_IBCR00.bit.SPF           IBCR00_SPF                    
                  IO_IBCR00.bit.ALE           IBCR00_ALE                    
                  IO_IBCR00.bit.ALF           IBCR00_ALF                    
                  IO_IBCR00.bit.INTS          IBCR00_INTS                   
                  IO_IBCR00.bit.AACKX         IBCR00_AACKX                  
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : IBCR10                      傾僪儗僗丗0x61
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_IBCR10.byte              IBCR10                        
  價僢僩          IO_IBCR10.bit.INT           IBCR10_INT                    
                  IO_IBCR10.bit.INTE          IBCR10_INTE                   
                  IO_IBCR10.bit.GACKE         IBCR10_GACKE                  
                  IO_IBCR10.bit.DACKE         IBCR10_DACKE                  
                  IO_IBCR10.bit.MSS           IBCR10_MSS                    
                  IO_IBCR10.bit.SCC           IBCR10_SCC                    
                  IO_IBCR10.bit.BEIE          IBCR10_BEIE                   
                  IO_IBCR10.bit.BER           IBCR10_BER                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : IBSR0                       傾僪儗僗丗0x62
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_IBSR0.byte               IBSR0                         
  價僢僩          IO_IBSR0.bit.FBT            IBSR0_FBT                     
                  IO_IBSR0.bit.GCA            IBSR0_GCA                     
                  IO_IBSR0.bit.AAS            IBSR0_AAS                     
                  IO_IBSR0.bit.TRX            IBSR0_TRX                     
                  IO_IBSR0.bit.LRB            IBSR0_LRB                     
                  IO_IBSR0.bit.RSC            IBSR0_RSC                     
                  IO_IBSR0.bit.BB             IBSR0_BB                      
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : IDDR0                       傾僪儗僗丗0x63
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_IDDR0                    IDDR0                         
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : IAAR0                       傾僪儗僗丗0x64
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_IAAR0                    IAAR0                         
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : ICCR0                       傾僪儗僗丗0x65
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_ICCR0.byte               ICCR0                         
  價僢僩          IO_ICCR0.bit.CS0            ICCR0_CS0                     
                  IO_ICCR0.bit.CS1            ICCR0_CS1                     
                  IO_ICCR0.bit.CS2            ICCR0_CS2                     
                  IO_ICCR0.bit.CS3            ICCR0_CS3                     
                  IO_ICCR0.bit.CS4            ICCR0_CS4                     
                  IO_ICCR0.bit.EN             ICCR0_EN                      
                  IO_ICCR0.bit.DMBP           ICCR0_DMBP                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : OPCUR                       傾僪儗僗丗0x66
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_OPCUR.byte               OPCUR                         
  價僢僩          IO_OPCUR.bit.WTIE           OPCUR_WTIE                    
                  IO_OPCUR.bit.WTIF           OPCUR_WTIF                    
                  IO_OPCUR.bit.OPS0           OPCUR_OPS0                    
                  IO_OPCUR.bit.OPS1           OPCUR_OPS1                    
                  IO_OPCUR.bit.OPS2           OPCUR_OPS2                    
                  IO_OPCUR.bit.NRSL           OPCUR_NRSL                    
                  IO_OPCUR.bit.DTIF           OPCUR_DTIF                    
                  IO_OPCUR.bit.DTIE           OPCUR_DTIE                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : OPCLR                       傾僪儗僗丗0x67
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_OPCLR.byte               OPCLR                         
  價僢僩          IO_OPCLR.bit.OPE0           OPCLR_OPE0                    
                  IO_OPCLR.bit.OPE1           OPCLR_OPE1                    
                  IO_OPCLR.bit.OPE2           OPCLR_OPE2                    
                  IO_OPCLR.bit.OPE3           OPCLR_OPE3                    
                  IO_OPCLR.bit.OPE4           OPCLR_OPE4                    
                  IO_OPCLR.bit.OPE5           OPCLR_OPE5                    
                  IO_OPCLR.bit.PDIE           OPCLR_PDIE                    
                  IO_OPCLR.bit.PDIF           OPCLR_PDIF                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : IPCUR                       傾僪儗僗丗0x68
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_IPCUR.byte               IPCUR                         
  價僢僩          IO_IPCUR.bit.CMPE           IPCUR_CMPE                    
                  IO_IPCUR.bit.CPD0           IPCUR_CPD0                    
                  IO_IPCUR.bit.CPD1           IPCUR_CPD1                    
                  IO_IPCUR.bit.CPD2           IPCUR_CPD2                    
                  IO_IPCUR.bit.CPIE           IPCUR_CPIE                    
                  IO_IPCUR.bit.CPIF           IPCUR_CPIF                    
                  IO_IPCUR.bit.WTS0           IPCUR_WTS0                    
                  IO_IPCUR.bit.WTS1           IPCUR_WTS1                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : IPCLR                       傾僪儗僗丗0x69
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_IPCLR.byte               IPCLR                         
  價僢僩          IO_IPCLR.bit.SEE0           IPCLR_SEE0                    
                  IO_IPCLR.bit.SEE1           IPCLR_SEE1                    
                  IO_IPCLR.bit.SEE2           IPCLR_SEE2                    
                  IO_IPCLR.bit.SNC0           IPCLR_SNC0                    
                  IO_IPCLR.bit.SNC1           IPCLR_SNC1                    
                  IO_IPCLR.bit.SNC2           IPCLR_SNC2                    
                  IO_IPCLR.bit.CPE0           IPCLR_CPE0                    
                  IO_IPCLR.bit.CPE1           IPCLR_CPE1                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : NCCR                        傾僪儗僗丗0x6a
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_NCCR.byte                NCCR                          
  價僢僩          IO_NCCR.bit.D0              NCCR_D0                       
                  IO_NCCR.bit.D1              NCCR_D1                       
                  IO_NCCR.bit.S00             NCCR_S00                      
                  IO_NCCR.bit.S01             NCCR_S01                      
                  IO_NCCR.bit.S10             NCCR_S10                      
                  IO_NCCR.bit.S11             NCCR_S11                      
                  IO_NCCR.bit.S20             NCCR_S20                      
                  IO_NCCR.bit.S21             NCCR_S21                      
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : TCSR                        傾僪儗僗丗0x6b
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_TCSR.byte                TCSR                          
  價僢僩          IO_TCSR.bit.CLK0            TCSR_CLK0                     
                  IO_TCSR.bit.CLK1            TCSR_CLK1                     
                  IO_TCSR.bit.CLK2            TCSR_CLK2                     
                  IO_TCSR.bit.TMEN            TCSR_TMEN                     
                  IO_TCSR.bit.ICRE            TCSR_ICRE                     
                  IO_TCSR.bit.ICLR            TCSR_ICLR                     
                  IO_TCSR.bit.MODE            TCSR_MODE                     
                  IO_TCSR.bit.TCLR            TCSR_TCLR                     
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : ADC1                        傾僪儗僗丗0x6c
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_ADC1.byte                ADC1                          
  價僢僩          IO_ADC1.bit.AD              ADC1_AD                       
                  IO_ADC1.bit.ADMV            ADC1_ADMV                     
                  IO_ADC1.bit.ADI             ADC1_ADI                      
                  IO_ADC1.bit.ANS0            ADC1_ANS0                     
                  IO_ADC1.bit.ANS1            ADC1_ANS1                     
                  IO_ADC1.bit.ANS2            ADC1_ANS2                     
                  IO_ADC1.bit.ANS3            ADC1_ANS3                     
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : ADC2                        傾僪儗僗丗0x6d
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_ADC2.byte                ADC2                          
  價僢僩          IO_ADC2.bit.CKDIV0          ADC2_CKDIV0                   
                  IO_ADC2.bit.CKDIV1          ADC2_CKDIV1                   
                  IO_ADC2.bit.EXT             ADC2_EXT                      
                  IO_ADC2.bit.ADIE            ADC2_ADIE                     
                  IO_ADC2.bit.ADCK            ADC2_ADCK                     
                  IO_ADC2.bit.TIM0            ADC2_TIM0                     
                  IO_ADC2.bit.TIM1            ADC2_TIM1                     
                  IO_ADC2.bit.AD8             ADC2_AD8                      
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : ADD                         傾僪儗僗丗0x6e-0x6f
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_ADD.word                 ADD                           
  僶僀僩/儚乕僪   IO_ADD.byte.ADDH            ADD_ADDH                      
                  IO_ADD.byte.ADDL            ADD_ADDL                      
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : FSR2                        傾僪儗僗丗0x71
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_FSR2.byte                FSR2                          
  價僢僩          IO_FSR2.bit.ERSTO           FSR2_ERSTO                    
                  IO_FSR2.bit.ETIEN           FSR2_ETIEN                    
                  IO_FSR2.bit.ERSEND          FSR2_ERSEND                   
                  IO_FSR2.bit.EEIEN           FSR2_EEIEN                    
                  IO_FSR2.bit.PGMTO           FSR2_PGMTO                    
                  IO_FSR2.bit.PTIEN           FSR2_PTIEN                    
                  IO_FSR2.bit.PGMEND          FSR2_PGMEND                   
                  IO_FSR2.bit.PEIEN           FSR2_PEIEN                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : FSR                         傾僪儗僗丗0x72
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_FSR.byte                 FSR                           
  價僢僩          IO_FSR.bit.SSEN             FSR_SSEN                      
                  IO_FSR.bit.WRE              FSR_WRE                       
                  IO_FSR.bit.IRQEN            FSR_IRQEN                     
                  IO_FSR.bit.RDY              FSR_RDY                       
                  IO_FSR.bit.RDYIRQ           FSR_RDYIRQ                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : SWRE0                       傾僪儗僗丗0x73
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_SWRE0.byte               SWRE0                         
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯SWRE0儗僕僗僞傊彂崬傒傪峴偆帪偼丄梊栺價僢僩偵忢偵抣侽傪彂崬傓
    昁梫偑偁傞偨傔丄儊儞僶IO_SWRE0.byte偵丄曄悢枖偼掕悢傪扨弮戙擖幃
    偱戙擖偡傞偙偲偱峴偭偰壓偝偄丅


  I/O儗僕僗僞柤 : FSR3                        傾僪儗僗丗0x74
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_FSR3.byte                FSR3                          
  價僢僩          IO_FSR3.bit.HANG            FSR3_HANG                     
                  IO_FSR3.bit.PGMS            FSR3_PGMS                     
                  IO_FSR3.bit.SERS            FSR3_SERS                     
                  IO_FSR3.bit.ESPS            FSR3_ESPS                     
                  IO_FSR3.bit.CERS            FSR3_CERS                     
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : FSR4                        傾僪儗僗丗0x75
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_FSR4.byte                FSR4                          
  價僢僩          IO_FSR4.bit.CERTO           FSR4_CERTO                    
                  IO_FSR4.bit.CTIEN           FSR4_CTIEN                    
                  IO_FSR4.bit.CEREND          FSR4_CEREND                   
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : WREN                        傾僪儗僗丗0x76
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_WREN.byte                WREN                          
  價僢僩          IO_WREN.bit.EN0             WREN_EN0                      
                  IO_WREN.bit.EN1             WREN_EN1                      
                  IO_WREN.bit.EN2             WREN_EN2                      
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : WROR                        傾僪儗僗丗0x77
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_WROR.byte                WROR                          
  價僢僩          IO_WROR.bit.DRR0            WROR_DRR0                     
                  IO_WROR.bit.DRR1            WROR_DRR1                     
                  IO_WROR.bit.DRR2            WROR_DRR2                     
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : ILR0                        傾僪儗僗丗0x79
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_ILR0                     ILR0                          
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : ILR1                        傾僪儗僗丗0x7a
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_ILR1                     ILR1                          
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : ILR2                        傾僪儗僗丗0x7b
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_ILR2                     ILR2                          
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : ILR3                        傾僪儗僗丗0x7c
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_ILR3                     ILR3                          
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : ILR4                        傾僪儗僗丗0x7d
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_ILR4                     ILR4                          
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : ILR5                        傾僪儗僗丗0x7e
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_ILR5                     ILR5                          
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : WRAR0                       傾僪儗僗丗0xf80-0xf81
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_WRAR0                    WRAR0                         
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : WRDR0                       傾僪儗僗丗0xf82
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_WRDR0                    WRDR0                         
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : WRAR1                       傾僪儗僗丗0xf83-0xf84
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_WRAR1                    WRAR1                         
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : WRDR1                       傾僪儗僗丗0xf85
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_WRDR1                    WRDR1                         
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : WRAR2                       傾僪儗僗丗0xf86-0xf87
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_WRAR2                    WRAR2                         
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : WRDR2                       傾僪儗僗丗0xf88
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_WRDR2                    WRDR2                         
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : T01CR0                      傾僪儗僗丗0xf92
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_T01CR0.byte              T01CR0                        
  價僢僩          IO_T01CR0.bit.F0            T01CR0_F0                     
                  IO_T01CR0.bit.F1            T01CR0_F1                     
                  IO_T01CR0.bit.F2            T01CR0_F2                     
                  IO_T01CR0.bit.F3            T01CR0_F3                     
                  IO_T01CR0.bit.C0            T01CR0_C0                     
                  IO_T01CR0.bit.C1            T01CR0_C1                     
                  IO_T01CR0.bit.C2            T01CR0_C2                     
                  IO_T01CR0.bit.IFE           T01CR0_IFE                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : T00CR0                      傾僪儗僗丗0xf93
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_T00CR0.byte              T00CR0                        
  價僢僩          IO_T00CR0.bit.F0            T00CR0_F0                     
                  IO_T00CR0.bit.F1            T00CR0_F1                     
                  IO_T00CR0.bit.F2            T00CR0_F2                     
                  IO_T00CR0.bit.F3            T00CR0_F3                     
                  IO_T00CR0.bit.C0            T00CR0_C0                     
                  IO_T00CR0.bit.C1            T00CR0_C1                     
                  IO_T00CR0.bit.C2            T00CR0_C2                     
                  IO_T00CR0.bit.IFE           T00CR0_IFE                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : T01DR                       傾僪儗僗丗0xf94
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_T01DR                    T01DR                         
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : T00DR                       傾僪儗僗丗0xf95
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_T00DR                    T00DR                         
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : TMCR0                       傾僪儗僗丗0xf96
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_TMCR0.byte               TMCR0                         
  價僢僩          IO_TMCR0.bit.FE00           TMCR0_FE00                    
                  IO_TMCR0.bit.FE01           TMCR0_FE01                    
                  IO_TMCR0.bit.FE10           TMCR0_FE10                    
                  IO_TMCR0.bit.FE11           TMCR0_FE11                    
                  IO_TMCR0.bit.MOD            TMCR0_MOD                     
                  IO_TMCR0.bit.TIS            TMCR0_TIS                     
                  IO_TMCR0.bit.TO0            TMCR0_TO0                     
                  IO_TMCR0.bit.TO1            TMCR0_TO1                     
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : T11CR0                      傾僪儗僗丗0xf97
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_T11CR0.byte              T11CR0                        
  價僢僩          IO_T11CR0.bit.F0            T11CR0_F0                     
                  IO_T11CR0.bit.F1            T11CR0_F1                     
                  IO_T11CR0.bit.F2            T11CR0_F2                     
                  IO_T11CR0.bit.F3            T11CR0_F3                     
                  IO_T11CR0.bit.C0            T11CR0_C0                     
                  IO_T11CR0.bit.C1            T11CR0_C1                     
                  IO_T11CR0.bit.C2            T11CR0_C2                     
                  IO_T11CR0.bit.IFE           T11CR0_IFE                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : T10CR0                      傾僪儗僗丗0xf98
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_T10CR0.byte              T10CR0                        
  價僢僩          IO_T10CR0.bit.F0            T10CR0_F0                     
                  IO_T10CR0.bit.F1            T10CR0_F1                     
                  IO_T10CR0.bit.F2            T10CR0_F2                     
                  IO_T10CR0.bit.F3            T10CR0_F3                     
                  IO_T10CR0.bit.C0            T10CR0_C0                     
                  IO_T10CR0.bit.C1            T10CR0_C1                     
                  IO_T10CR0.bit.C2            T10CR0_C2                     
                  IO_T10CR0.bit.IFE           T10CR0_IFE                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : T11DR                       傾僪儗僗丗0xf99
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_T11DR                    T11DR                         
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : T10DR                       傾僪儗僗丗0xf9a
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_T10DR                    T10DR                         
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : TMCR1                       傾僪儗僗丗0xf9b
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_TMCR1.byte               TMCR1                         
  價僢僩          IO_TMCR1.bit.FE00           TMCR1_FE00                    
                  IO_TMCR1.bit.FE01           TMCR1_FE01                    
                  IO_TMCR1.bit.FE10           TMCR1_FE10                    
                  IO_TMCR1.bit.FE11           TMCR1_FE11                    
                  IO_TMCR1.bit.MOD            TMCR1_MOD                     
                  IO_TMCR1.bit.TIS            TMCR1_TIS                     
                  IO_TMCR1.bit.TO0            TMCR1_TO0                     
                  IO_TMCR1.bit.TO1            TMCR1_TO1                     
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : PPS01                       傾僪儗僗丗0xf9c
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PPS01                    PPS01                         
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : PPS00                       傾僪儗僗丗0xf9d
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PPS00                    PPS00                         
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : PDS01                       傾僪儗僗丗0xf9e
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PDS01                    PDS01                         
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : PDS00                       傾僪儗僗丗0xf9f
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PDS00                    PDS00                         
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : PPS11                       傾僪儗僗丗0xfa0
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PPS11                    PPS11                         
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : PPS10                       傾僪儗僗丗0xfa1
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PPS10                    PPS10                         
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : PDS11                       傾僪儗僗丗0xfa2
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PDS11                    PDS11                         
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : PDS10                       傾僪儗僗丗0xfa3
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PDS10                    PDS10                         
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : PPGS                        傾僪儗僗丗0xfa4
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PPGS.byte                PPGS                          
  價僢僩          IO_PPGS.bit.PEN00           PPGS_PEN00                    
                  IO_PPGS.bit.PEN01           PPGS_PEN01                    
                  IO_PPGS.bit.PEN10           PPGS_PEN10                    
                  IO_PPGS.bit.PEN11           PPGS_PEN11                    
                  IO_PPGS.bit.PEN20           PPGS_PEN20                    
                  IO_PPGS.bit.PEN21           PPGS_PEN21                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : REVC                        傾僪儗僗丗0xfa5
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_REVC.byte                REVC                          
  價僢僩          IO_REVC.bit.REV00           REVC_REV00                    
                  IO_REVC.bit.REV01           REVC_REV01                    
                  IO_REVC.bit.REV10           REVC_REV10                    
                  IO_REVC.bit.REV11           REVC_REV11                    
                  IO_REVC.bit.REV20           REVC_REV20                    
                  IO_REVC.bit.REV21           REVC_REV21                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : PPS21                       傾僪儗僗丗0xfa6
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PPS21                    PPS21                         
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : PPS20                       傾僪儗僗丗0xfa7
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PPS20                    PPS20                         
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : TMR1                        傾僪儗僗丗0xfa8-0xfa9
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_TMR1.word                TMR1                          
  僶僀僩/儚乕僪   IO_TMR1.byte.TMRH1          TMR1_TMRH1                    
                  IO_TMR1.byte.TMRL1          TMR1_TMRL1                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : PDS21                       傾僪儗僗丗0xfaa
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PDS21                    PDS21                         
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : PDS20                       傾僪儗僗丗0xfab
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PDS20                    PDS20                         
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : PDCR1                       傾僪儗僗丗0xfb0-0xfb1
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PDCR1.word               PDCR1                         
  僶僀僩/儚乕僪   IO_PDCR1.byte.PDCRH         PDCR1_PDCRH                   
                  IO_PDCR1.byte.PDCRL         PDCR1_PDCRL                   
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : PCSR1                       傾僪儗僗丗0xfb2-0xfb3
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PCSR1.word               PCSR1                         
  僶僀僩/儚乕僪   IO_PCSR1.byte.PCSRH         PCSR1_PCSRH                   
                  IO_PCSR1.byte.PCSRL         PCSR1_PCSRL                   
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : PDUT1                       傾僪儗僗丗0xfb4-0xfb5
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PDUT1.word               PDUT1                         
  僶僀僩/儚乕僪   IO_PDUT1.byte.PDUTH         PDUT1_PDUTH                   
                  IO_PDUT1.byte.PDUTL         PDUT1_PDUTL                   
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : BGR1                        傾僪儗僗丗0xfbc
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_BGR1                     BGR1                          
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : BGR0                        傾僪儗僗丗0xfbd
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_BGR0                     BGR0                          
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : PSSR0                       傾僪儗僗丗0xfbe
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_PSSR0.byte               PSSR0                         
  價僢僩          IO_PSSR0.bit.PSS0           PSSR0_PSS0                    
                  IO_PSSR0.bit.PSS1           PSSR0_PSS1                    
                  IO_PSSR0.bit.BRGE           PSSR0_BRGE                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : BRSR0                       傾僪儗僗丗0xfbf
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_BRSR0                    BRSR0                         
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : AIDRL                       傾僪儗僗丗0xfc3
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_AIDRL.byte               AIDRL                         
  價僢僩          IO_AIDRL.bit.P00            AIDRL_P00                     
                  IO_AIDRL.bit.P01            AIDRL_P01                     
                  IO_AIDRL.bit.P02            AIDRL_P02                     
                  IO_AIDRL.bit.P03            AIDRL_P03                     
                  IO_AIDRL.bit.P04            AIDRL_P04                     
                  IO_AIDRL.bit.P05            AIDRL_P05                     
                  IO_AIDRL.bit.P06            AIDRL_P06                     
                  IO_AIDRL.bit.P07            AIDRL_P07                     
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : OPDBRH0                     傾僪儗僗丗0xfc4
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_OPDBRH0.byte             OPDBRH0                       
  價僢僩          IO_OPDBRH0.bit.OP40         OPDBRH0_OP40                  
                  IO_OPDBRH0.bit.OP41         OPDBRH0_OP41                  
                  IO_OPDBRH0.bit.OP50         OPDBRH0_OP50                  
                  IO_OPDBRH0.bit.OP51         OPDBRH0_OP51                  
                  IO_OPDBRH0.bit.RDA0         OPDBRH0_RDA0                  
                  IO_OPDBRH0.bit.RDA1         OPDBRH0_RDA1                  
                  IO_OPDBRH0.bit.RDA2         OPDBRH0_RDA2                  
                  IO_OPDBRH0.bit.BNKF         OPDBRH0_BNKF                  
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : OPDBRL0                     傾僪儗僗丗0xfc5
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_OPDBRL0.byte             OPDBRL0                       
  價僢僩          IO_OPDBRL0.bit.OP00         OPDBRL0_OP00                  
                  IO_OPDBRL0.bit.OP01         OPDBRL0_OP01                  
                  IO_OPDBRL0.bit.OP10         OPDBRL0_OP10                  
                  IO_OPDBRL0.bit.OP11         OPDBRL0_OP11                  
                  IO_OPDBRL0.bit.OP20         OPDBRL0_OP20                  
                  IO_OPDBRL0.bit.OP21         OPDBRL0_OP21                  
                  IO_OPDBRL0.bit.OP30         OPDBRL0_OP30                  
                  IO_OPDBRL0.bit.OP31         OPDBRL0_OP31                  
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : OPDBRH1                     傾僪儗僗丗0xfc6
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_OPDBRH1.byte             OPDBRH1                       
  價僢僩          IO_OPDBRH1.bit.OP40         OPDBRH1_OP40                  
                  IO_OPDBRH1.bit.OP41         OPDBRH1_OP41                  
                  IO_OPDBRH1.bit.OP50         OPDBRH1_OP50                  
                  IO_OPDBRH1.bit.OP51         OPDBRH1_OP51                  
                  IO_OPDBRH1.bit.RDA0         OPDBRH1_RDA0                  
                  IO_OPDBRH1.bit.RDA1         OPDBRH1_RDA1                  
                  IO_OPDBRH1.bit.RDA2         OPDBRH1_RDA2                  
                  IO_OPDBRH1.bit.BNKF         OPDBRH1_BNKF                  
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : OPDBRL1                     傾僪儗僗丗0xfc7
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_OPDBRL1.byte             OPDBRL1                       
  價僢僩          IO_OPDBRL1.bit.OP00         OPDBRL1_OP00                  
                  IO_OPDBRL1.bit.OP01         OPDBRL1_OP01                  
                  IO_OPDBRL1.bit.OP10         OPDBRL1_OP10                  
                  IO_OPDBRL1.bit.OP11         OPDBRL1_OP11                  
                  IO_OPDBRL1.bit.OP20         OPDBRL1_OP20                  
                  IO_OPDBRL1.bit.OP21         OPDBRL1_OP21                  
                  IO_OPDBRL1.bit.OP30         OPDBRL1_OP30                  
                  IO_OPDBRL1.bit.OP31         OPDBRL1_OP31                  
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : OPDBRH2                     傾僪儗僗丗0xfc8
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_OPDBRH2.byte             OPDBRH2                       
  價僢僩          IO_OPDBRH2.bit.OP40         OPDBRH2_OP40                  
                  IO_OPDBRH2.bit.OP41         OPDBRH2_OP41                  
                  IO_OPDBRH2.bit.OP50         OPDBRH2_OP50                  
                  IO_OPDBRH2.bit.OP51         OPDBRH2_OP51                  
                  IO_OPDBRH2.bit.RDA0         OPDBRH2_RDA0                  
                  IO_OPDBRH2.bit.RDA1         OPDBRH2_RDA1                  
                  IO_OPDBRH2.bit.RDA2         OPDBRH2_RDA2                  
                  IO_OPDBRH2.bit.BNKF         OPDBRH2_BNKF                  
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : OPDBRL2                     傾僪儗僗丗0xfc9
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_OPDBRL2.byte             OPDBRL2                       
  價僢僩          IO_OPDBRL2.bit.OP00         OPDBRL2_OP00                  
                  IO_OPDBRL2.bit.OP01         OPDBRL2_OP01                  
                  IO_OPDBRL2.bit.OP10         OPDBRL2_OP10                  
                  IO_OPDBRL2.bit.OP11         OPDBRL2_OP11                  
                  IO_OPDBRL2.bit.OP20         OPDBRL2_OP20                  
                  IO_OPDBRL2.bit.OP21         OPDBRL2_OP21                  
                  IO_OPDBRL2.bit.OP30         OPDBRL2_OP30                  
                  IO_OPDBRL2.bit.OP31         OPDBRL2_OP31                  
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : OPDBRH3                     傾僪儗僗丗0xfca
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_OPDBRH3.byte             OPDBRH3                       
  價僢僩          IO_OPDBRH3.bit.OP40         OPDBRH3_OP40                  
                  IO_OPDBRH3.bit.OP41         OPDBRH3_OP41                  
                  IO_OPDBRH3.bit.OP50         OPDBRH3_OP50                  
                  IO_OPDBRH3.bit.OP51         OPDBRH3_OP51                  
                  IO_OPDBRH3.bit.RDA0         OPDBRH3_RDA0                  
                  IO_OPDBRH3.bit.RDA1         OPDBRH3_RDA1                  
                  IO_OPDBRH3.bit.RDA2         OPDBRH3_RDA2                  
                  IO_OPDBRH3.bit.BNKF         OPDBRH3_BNKF                  
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : OPDBRL3                     傾僪儗僗丗0xfcb
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_OPDBRL3.byte             OPDBRL3                       
  價僢僩          IO_OPDBRL3.bit.OP00         OPDBRL3_OP00                  
                  IO_OPDBRL3.bit.OP01         OPDBRL3_OP01                  
                  IO_OPDBRL3.bit.OP10         OPDBRL3_OP10                  
                  IO_OPDBRL3.bit.OP11         OPDBRL3_OP11                  
                  IO_OPDBRL3.bit.OP20         OPDBRL3_OP20                  
                  IO_OPDBRL3.bit.OP21         OPDBRL3_OP21                  
                  IO_OPDBRL3.bit.OP30         OPDBRL3_OP30                  
                  IO_OPDBRL3.bit.OP31         OPDBRL3_OP31                  
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : OPDBRH4                     傾僪儗僗丗0xfcc
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_OPDBRH4.byte             OPDBRH4                       
  價僢僩          IO_OPDBRH4.bit.OP40         OPDBRH4_OP40                  
                  IO_OPDBRH4.bit.OP41         OPDBRH4_OP41                  
                  IO_OPDBRH4.bit.OP50         OPDBRH4_OP50                  
                  IO_OPDBRH4.bit.OP51         OPDBRH4_OP51                  
                  IO_OPDBRH4.bit.RDA0         OPDBRH4_RDA0                  
                  IO_OPDBRH4.bit.RDA1         OPDBRH4_RDA1                  
                  IO_OPDBRH4.bit.RDA2         OPDBRH4_RDA2                  
                  IO_OPDBRH4.bit.BNKF         OPDBRH4_BNKF                  
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : OPDBRL4                     傾僪儗僗丗0xfcd
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_OPDBRL4.byte             OPDBRL4                       
  價僢僩          IO_OPDBRL4.bit.OP00         OPDBRL4_OP00                  
                  IO_OPDBRL4.bit.OP01         OPDBRL4_OP01                  
                  IO_OPDBRL4.bit.OP10         OPDBRL4_OP10                  
                  IO_OPDBRL4.bit.OP11         OPDBRL4_OP11                  
                  IO_OPDBRL4.bit.OP20         OPDBRL4_OP20                  
                  IO_OPDBRL4.bit.OP21         OPDBRL4_OP21                  
                  IO_OPDBRL4.bit.OP30         OPDBRL4_OP30                  
                  IO_OPDBRL4.bit.OP31         OPDBRL4_OP31                  
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : OPDBRH5                     傾僪儗僗丗0xfce
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_OPDBRH5.byte             OPDBRH5                       
  價僢僩          IO_OPDBRH5.bit.OP40         OPDBRH5_OP40                  
                  IO_OPDBRH5.bit.OP41         OPDBRH5_OP41                  
                  IO_OPDBRH5.bit.OP50         OPDBRH5_OP50                  
                  IO_OPDBRH5.bit.OP51         OPDBRH5_OP51                  
                  IO_OPDBRH5.bit.RDA0         OPDBRH5_RDA0                  
                  IO_OPDBRH5.bit.RDA1         OPDBRH5_RDA1                  
                  IO_OPDBRH5.bit.RDA2         OPDBRH5_RDA2                  
                  IO_OPDBRH5.bit.BNKF         OPDBRH5_BNKF                  
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : OPDBRL5                     傾僪儗僗丗0xfcf
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_OPDBRL5.byte             OPDBRL5                       
  價僢僩          IO_OPDBRL5.bit.OP00         OPDBRL5_OP00                  
                  IO_OPDBRL5.bit.OP01         OPDBRL5_OP01                  
                  IO_OPDBRL5.bit.OP10         OPDBRL5_OP10                  
                  IO_OPDBRL5.bit.OP11         OPDBRL5_OP11                  
                  IO_OPDBRL5.bit.OP20         OPDBRL5_OP20                  
                  IO_OPDBRL5.bit.OP21         OPDBRL5_OP21                  
                  IO_OPDBRL5.bit.OP30         OPDBRL5_OP30                  
                  IO_OPDBRL5.bit.OP31         OPDBRL5_OP31                  
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : OPDBRH6                     傾僪儗僗丗0xfd0
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_OPDBRH6.byte             OPDBRH6                       
  價僢僩          IO_OPDBRH6.bit.OP40         OPDBRH6_OP40                  
                  IO_OPDBRH6.bit.OP41         OPDBRH6_OP41                  
                  IO_OPDBRH6.bit.OP50         OPDBRH6_OP50                  
                  IO_OPDBRH6.bit.OP51         OPDBRH6_OP51                  
                  IO_OPDBRH6.bit.RDA0         OPDBRH6_RDA0                  
                  IO_OPDBRH6.bit.RDA1         OPDBRH6_RDA1                  
                  IO_OPDBRH6.bit.RDA2         OPDBRH6_RDA2                  
                  IO_OPDBRH6.bit.BNKF         OPDBRH6_BNKF                  
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : OPDBRL6                     傾僪儗僗丗0xfd1
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_OPDBRL6.byte             OPDBRL6                       
  價僢僩          IO_OPDBRL6.bit.OP00         OPDBRL6_OP00                  
                  IO_OPDBRL6.bit.OP01         OPDBRL6_OP01                  
                  IO_OPDBRL6.bit.OP10         OPDBRL6_OP10                  
                  IO_OPDBRL6.bit.OP11         OPDBRL6_OP11                  
                  IO_OPDBRL6.bit.OP20         OPDBRL6_OP20                  
                  IO_OPDBRL6.bit.OP21         OPDBRL6_OP21                  
                  IO_OPDBRL6.bit.OP30         OPDBRL6_OP30                  
                  IO_OPDBRL6.bit.OP31         OPDBRL6_OP31                  
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : OPDBRH7                     傾僪儗僗丗0xfd2
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_OPDBRH7.byte             OPDBRH7                       
  價僢僩          IO_OPDBRH7.bit.OP40         OPDBRH7_OP40                  
                  IO_OPDBRH7.bit.OP41         OPDBRH7_OP41                  
                  IO_OPDBRH7.bit.OP50         OPDBRH7_OP50                  
                  IO_OPDBRH7.bit.OP51         OPDBRH7_OP51                  
                  IO_OPDBRH7.bit.RDA0         OPDBRH7_RDA0                  
                  IO_OPDBRH7.bit.RDA1         OPDBRH7_RDA1                  
                  IO_OPDBRH7.bit.RDA2         OPDBRH7_RDA2                  
                  IO_OPDBRH7.bit.BNKF         OPDBRH7_BNKF                  
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : OPDBRL7                     傾僪儗僗丗0xfd3
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_OPDBRL7.byte             OPDBRL7                       
  價僢僩          IO_OPDBRL7.bit.OP00         OPDBRL7_OP00                  
                  IO_OPDBRL7.bit.OP01         OPDBRL7_OP01                  
                  IO_OPDBRL7.bit.OP10         OPDBRL7_OP10                  
                  IO_OPDBRL7.bit.OP11         OPDBRL7_OP11                  
                  IO_OPDBRL7.bit.OP20         OPDBRL7_OP20                  
                  IO_OPDBRL7.bit.OP21         OPDBRL7_OP21                  
                  IO_OPDBRL7.bit.OP30         OPDBRL7_OP30                  
                  IO_OPDBRL7.bit.OP31         OPDBRL7_OP31                  
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : OPDBRH8                     傾僪儗僗丗0xfd4
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_OPDBRH8.byte             OPDBRH8                       
  價僢僩          IO_OPDBRH8.bit.OP40         OPDBRH8_OP40                  
                  IO_OPDBRH8.bit.OP41         OPDBRH8_OP41                  
                  IO_OPDBRH8.bit.OP50         OPDBRH8_OP50                  
                  IO_OPDBRH8.bit.OP51         OPDBRH8_OP51                  
                  IO_OPDBRH8.bit.RDA0         OPDBRH8_RDA0                  
                  IO_OPDBRH8.bit.RDA1         OPDBRH8_RDA1                  
                  IO_OPDBRH8.bit.RDA2         OPDBRH8_RDA2                  
                  IO_OPDBRH8.bit.BNKF         OPDBRH8_BNKF                  
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : OPDBRL8                     傾僪儗僗丗0xfd5
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_OPDBRL8.byte             OPDBRL8                       
  價僢僩          IO_OPDBRL8.bit.OP00         OPDBRL8_OP00                  
                  IO_OPDBRL8.bit.OP01         OPDBRL8_OP01                  
                  IO_OPDBRL8.bit.OP10         OPDBRL8_OP10                  
                  IO_OPDBRL8.bit.OP11         OPDBRL8_OP11                  
                  IO_OPDBRL8.bit.OP20         OPDBRL8_OP20                  
                  IO_OPDBRL8.bit.OP21         OPDBRL8_OP21                  
                  IO_OPDBRL8.bit.OP30         OPDBRL8_OP30                  
                  IO_OPDBRL8.bit.OP31         OPDBRL8_OP31                  
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : OPDBRH9                     傾僪儗僗丗0xfd6
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_OPDBRH9.byte             OPDBRH9                       
  價僢僩          IO_OPDBRH9.bit.OP40         OPDBRH9_OP40                  
                  IO_OPDBRH9.bit.OP41         OPDBRH9_OP41                  
                  IO_OPDBRH9.bit.OP50         OPDBRH9_OP50                  
                  IO_OPDBRH9.bit.OP51         OPDBRH9_OP51                  
                  IO_OPDBRH9.bit.RDA0         OPDBRH9_RDA0                  
                  IO_OPDBRH9.bit.RDA1         OPDBRH9_RDA1                  
                  IO_OPDBRH9.bit.RDA2         OPDBRH9_RDA2                  
                  IO_OPDBRH9.bit.BNKF         OPDBRH9_BNKF                  
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : OPDBRL9                     傾僪儗僗丗0xfd7
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_OPDBRL9.byte             OPDBRL9                       
  價僢僩          IO_OPDBRL9.bit.OP00         OPDBRL9_OP00                  
                  IO_OPDBRL9.bit.OP01         OPDBRL9_OP01                  
                  IO_OPDBRL9.bit.OP10         OPDBRL9_OP10                  
                  IO_OPDBRL9.bit.OP11         OPDBRL9_OP11                  
                  IO_OPDBRL9.bit.OP20         OPDBRL9_OP20                  
                  IO_OPDBRL9.bit.OP21         OPDBRL9_OP21                  
                  IO_OPDBRL9.bit.OP30         OPDBRL9_OP30                  
                  IO_OPDBRL9.bit.OP31         OPDBRL9_OP31                  
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : OPDBRHA                     傾僪儗僗丗0xfd8
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_OPDBRHA.byte             OPDBRHA                       
  價僢僩          IO_OPDBRHA.bit.OP40         OPDBRHA_OP40                  
                  IO_OPDBRHA.bit.OP41         OPDBRHA_OP41                  
                  IO_OPDBRHA.bit.OP50         OPDBRHA_OP50                  
                  IO_OPDBRHA.bit.OP51         OPDBRHA_OP51                  
                  IO_OPDBRHA.bit.RDA0         OPDBRHA_RDA0                  
                  IO_OPDBRHA.bit.RDA1         OPDBRHA_RDA1                  
                  IO_OPDBRHA.bit.RDA2         OPDBRHA_RDA2                  
                  IO_OPDBRHA.bit.BNKF         OPDBRHA_BNKF                  
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : OPDBRLA                     傾僪儗僗丗0xfd9
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_OPDBRLA.byte             OPDBRLA                       
  價僢僩          IO_OPDBRLA.bit.OP00         OPDBRLA_OP00                  
                  IO_OPDBRLA.bit.OP01         OPDBRLA_OP01                  
                  IO_OPDBRLA.bit.OP10         OPDBRLA_OP10                  
                  IO_OPDBRLA.bit.OP11         OPDBRLA_OP11                  
                  IO_OPDBRLA.bit.OP20         OPDBRLA_OP20                  
                  IO_OPDBRLA.bit.OP21         OPDBRLA_OP21                  
                  IO_OPDBRLA.bit.OP30         OPDBRLA_OP30                  
                  IO_OPDBRLA.bit.OP31         OPDBRLA_OP31                  
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : OPDBRHB                     傾僪儗僗丗0xfda
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_OPDBRHB.byte             OPDBRHB                       
  價僢僩          IO_OPDBRHB.bit.OP40         OPDBRHB_OP40                  
                  IO_OPDBRHB.bit.OP41         OPDBRHB_OP41                  
                  IO_OPDBRHB.bit.OP50         OPDBRHB_OP50                  
                  IO_OPDBRHB.bit.OP51         OPDBRHB_OP51                  
                  IO_OPDBRHB.bit.RDA0         OPDBRHB_RDA0                  
                  IO_OPDBRHB.bit.RDA1         OPDBRHB_RDA1                  
                  IO_OPDBRHB.bit.RDA2         OPDBRHB_RDA2                  
                  IO_OPDBRHB.bit.BNKF         OPDBRHB_BNKF                  
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : OPDBRLB                     傾僪儗僗丗0xfdb
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_OPDBRLB.byte             OPDBRLB                       
  價僢僩          IO_OPDBRLB.bit.OP00         OPDBRLB_OP00                  
                  IO_OPDBRLB.bit.OP01         OPDBRLB_OP01                  
                  IO_OPDBRLB.bit.OP10         OPDBRLB_OP10                  
                  IO_OPDBRLB.bit.OP11         OPDBRLB_OP11                  
                  IO_OPDBRLB.bit.OP20         OPDBRLB_OP20                  
                  IO_OPDBRLB.bit.OP21         OPDBRLB_OP21                  
                  IO_OPDBRLB.bit.OP30         OPDBRLB_OP30                  
                  IO_OPDBRLB.bit.OP31         OPDBRLB_OP31                  
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : OPDUR                       傾僪儗僗丗0xfdc
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_OPDUR.byte               OPDUR                         
  價僢僩          IO_OPDUR.bit.OP40           OPDUR_OP40                    
                  IO_OPDUR.bit.OP41           OPDUR_OP41                    
                  IO_OPDUR.bit.OP50           OPDUR_OP50                    
                  IO_OPDUR.bit.OP51           OPDUR_OP51                    
                  IO_OPDUR.bit.RDA0           OPDUR_RDA0                    
                  IO_OPDUR.bit.RDA1           OPDUR_RDA1                    
                  IO_OPDUR.bit.RDA2           OPDUR_RDA2                    
                  IO_OPDUR.bit.BNKF           OPDUR_BNKF                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : OPDLR                       傾僪儗僗丗0xfdd
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_OPDLR.byte               OPDLR                         
  價僢僩          IO_OPDLR.bit.OP00           OPDLR_OP00                    
                  IO_OPDLR.bit.OP01           OPDLR_OP01                    
                  IO_OPDLR.bit.OP10           OPDLR_OP10                    
                  IO_OPDLR.bit.OP11           OPDLR_OP11                    
                  IO_OPDLR.bit.OP20           OPDLR_OP20                    
                  IO_OPDLR.bit.OP21           OPDLR_OP21                    
                  IO_OPDLR.bit.OP30           OPDLR_OP30                    
                  IO_OPDLR.bit.OP31           OPDLR_OP31                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : CPCUR                       傾僪儗僗丗0xfde
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_CPCUR                    CPCUR                         
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : CPCLR                       傾僪儗僗丗0xfdf
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_CPCLR                    CPCLR                         
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : TMBUR                       傾僪儗僗丗0xfe2
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_TMBUR                    TMBUR                         
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : TMBLR                       傾僪儗僗丗0xfe3
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_TMBLR                    TMBLR                         
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : CRTH                        傾僪儗僗丗0xfe4
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_CRTH.byte                CRTH                          
  價僢僩          IO_CRTH.bit.CRTH0           CRTH_CRTH0                    
                  IO_CRTH.bit.CRTH1           CRTH_CRTH1                    
                  IO_CRTH.bit.CRTH2           CRTH_CRTH2                    
                  IO_CRTH.bit.CRTH3           CRTH_CRTH3                    
                  IO_CRTH.bit.CRTH4           CRTH_CRTH4                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : CRTL                        傾僪儗僗丗0xfe5
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_CRTL.byte                CRTL                          
  價僢僩          IO_CRTL.bit.CRTL0           CRTL_CRTL0                    
                  IO_CRTL.bit.CRTL1           CRTL_CRTL1                    
                  IO_CRTL.bit.CRTL2           CRTL_CRTL2                    
                  IO_CRTL.bit.CRTL3           CRTL_CRTL3                    
                  IO_CRTL.bit.CRTL4           CRTL_CRTL4                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : CRTDA                       傾僪儗僗丗0xfe7
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_CRTDA.byte               CRTDA                         
  價僢僩          IO_CRTDA.bit.CRTDA0         CRTDA_CRTDA0                  
                  IO_CRTDA.bit.CRTDA1         CRTDA_CRTDA1                  
                  IO_CRTDA.bit.CRTDA2         CRTDA_CRTDA2                  
                  IO_CRTDA.bit.CRTDA3         CRTDA_CRTDA3                  
                  IO_CRTDA.bit.CRTDA4         CRTDA_CRTDA4                  
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : SYSC                        傾僪儗僗丗0xfe8
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_SYSC.byte                SYSC                          
  價僢僩          IO_SYSC.bit.RSTEN           SYSC_RSTEN                    
                  IO_SYSC.bit.RSTOE           SYSC_RSTOE                    
                  IO_SYSC.bit.PPGSEL          SYSC_PPGSEL                   
                  IO_SYSC.bit.EC0SL           SYSC_EC0SL                    
                  IO_SYSC.bit.PFSEL           SYSC_PFSEL                    
                  IO_SYSC.bit.PGSEL           SYSC_PGSEL                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : CMCR                        傾僪儗僗丗0xfe9
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_CMCR.byte                CMCR                          
  價僢僩          IO_CMCR.bit.CMCEN           CMCR_CMCEN                    
                  IO_CMCR.bit.TBTSEL0         CMCR_TBTSEL0                  
                  IO_CMCR.bit.TBTSEL1         CMCR_TBTSEL1                  
                  IO_CMCR.bit.TBTSEL2         CMCR_TBTSEL2                  
                  IO_CMCR.bit.CMCSEL          CMCR_CMCSEL                   
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)


  I/O儗僕僗僞柤 : CMDR                        傾僪儗僗丗0xfea
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_CMDR                     CMDR                          
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : WDTH                        傾僪儗僗丗0xfeb
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_WDTH                     WDTH                          
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : WDTL                        傾僪儗僗丗0xfec
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_WDTL                     WDTL                          
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

  I/O儗僕僗僞柤 : WICR                        傾僪儗僗丗0xfef
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  傾僋僙僗        僔儞儃儖柤                  儅僋儘柤
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒
  僶僀僩/儚乕僪   IO_WICR.byte                WICR                          
  價僢僩          IO_WICR.bit.TRG1            WICR_TRG1                     
                  IO_WICR.bit.UCK0            WICR_UCK0                     
                  IO_WICR.bit.UI0             WICR_UI0                      
                  IO_WICR.bit.EC1             WICR_EC1                      
                  IO_WICR.bit.INT00           WICR_INT00                    
劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒劒

拲乯杮儗僕僗僞傊偺彂崬傒傪峴偆帪偼丄岆彂姺偊傪杊巭偡傞堊丄掕悢傪
    扨弮戙擖幃偱戙擖偟偰壓偝偄丅(戞俁復亙拲堄帠崁亜嶲徠)





 亂夵斉棜楌亃
   V01L01  2011.07.07   怴婯嶌惉
   V01L02  2011.08.08   壓婰儗僕僗僞偺掕媊曄峏
                        SYCC(0x7),STBC(0x8),SYCC2(0xD),CMR0C(0x42),
                        ADC1(0x6C),FSR3(0x74),CRTH(0xFE4),CRTL(0xFE5),
                        SYSC(0xFE8)



劇劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劉
劆丒杮帒椏偺婰嵹撪梕偼, 梊崘側偟偵曄峏偡傞偙偲偑偁傝傑偡偺偱, 偛梡柦偺嵺偼  劆
劆  塩嬈晹栧偵偛妋擣偔偩偝偄丅                                              劆
劆丒杮帒椏偵婰嵹偝傟偨摦嶌奣梫傗墳梡夞楬椺偼, 敿摫懱僨僶僀僗偺昗弨揑側摦嶌  劆
劆  傗巊偄曽傪帵偟偨傕偺偱, 幚嵺偵巊梡偡傞婡婍偱偺摦嶌傪曐徹偡傞傕偺偱偼偁  劆
劆  傝傑偣傫丅偟偨偑偄傑偟偰, 偙傟傜傪巊梡偡傞偵偁偨偭偰偼偍媞條偺愑擟偵偍  劆
劆  偄偰婡婍偺愝寁傪峴偭偰偔偩偝偄丅偙傟傜偺巊梡偵婲場偡傞懝奞側偳偵偮偄偰  劆
劆  偼, 摉幮偼偦偺愑擟傪晧偄傑偣傫丅                                        劆
劆丒杮帒椏偵婰嵹偝傟偨摦嶌奣梫丒夞楬恾傪娷傓媄弍忣曬偼, 摉幮傕偟偔偼戞嶰幰  劆
劆  偺摿嫋尃, 挊嶌尃摍偺抦揑嵿嶻尃傗偦偺懠偺尃棙偺巊梡尃傑偨偼幚巤尃偺嫋戻  劆
劆  傪堄枴偡傞傕偺偱偼偁傝傑偣傫丅傑偨, 偙傟傜偺巊梡偵偮偄偰, 戞嶰幰偺抦揑  劆
劆  嵿嶻尃傗偦偺懠偺尃棙偺幚巤偑偱偒傞偙偲偺曐徹傪峴偆傕偺偱偼偁傝傑偣傫丅  劆
劆  偟偨偑偭偰, 偙傟傜偺巊梡偵婲場偡傞戞嶰幰偺抦揑嵿嶻尃傗偦偺懠偺尃棙偺怤  劆
劆  奞偵偮偄偰, 摉幮偼偦偺愑擟傪晧偄傑偣傫丅                                劆
劆丒杮帒椏偵婰嵹偝傟偨惢昳偼, 捠忢偺嶻嬈梡, 堦斒帠柋梡, 僷乕僜僫儖梡, 壠掚  劆
劆  梡側偳偺堦斒揑梡搑偵巊梡偝傟傞偙偲傪堄恾偟偰愝寁丒惢憿偝傟偰偄傑偡丅嬌  劆
劆  傔偰崅搙側埨慡惈偑梫媮偝傟, 壖偵摉奩埨慡惈偑妋曐偝傟側偄応崌, 幮夛揑偵  劆
劆  廳戝側塭嬁傪梌偊偐偮捈愙惗柦丒恎懱偵懳偡傞廳戝側婋尟惈傪敽偆梡搑乮尨巕  劆
劆  椡巤愝偵偍偗傞妀斀墳惂屼, 峲嬻婡帺摦旘峴惂屼, 峲嬻岎捠娗惂, 戝検桝憲僔  劆
劆  僗僥儉偵偍偗傞塣峴惂屼, 惗柦堐帩偺偨傔偺堛椕婡婍, 暫婍僔僗僥儉偵偍偗傞  劆
劆  儈僒僀儖敪幩惂屼傪偄偆乯, 側傜傃偵嬌傔偰崅偄怣棅惈偑梫媮偝傟傞梡搑乮奀  劆
劆  掙拞宲婍, 塅拡塹惎傪偄偆乯偵巊梡偝傟傞傛偆愝寁丒惢憿偝傟偨傕偺偱偼偁傝  劆
劆  傑偣傫丅偟偨偑偭偰, 偙傟傜偺梡搑偵偛巊梡傪偍峫偊偺偍媞條偼, 昁偢帠慜偵  劆
劆  塩嬈晹栧傑偱偛憡択偔偩偝偄丅偛憡択側偔巊梡偝傟偨偙偲偵傛傝敪惗偟偨懝奞  劆
劆  側偳偵偮偄偰偼, 愑擟傪晧偄偐偹傑偡偺偱偛椆彸偔偩偝偄丅                  劆
劆丒敿摫懱僨僶僀僗偼偁傞妋棪偱屘忈偑敪惗偟傑偡丅摉幮敿摫懱僨僶僀僗偑屘忈偟  劆
劆  偰傕, 寢壥揑偵恖恎帠屘, 壩嵭帠屘, 幮夛揑側懝奞傪惗偠偝偣側偄傛偆, 偍媞  劆
劆  條偼, 憰抲偺忕挿愝寁, 墑從懳嶔愝寁, 夁揹棳杊巭懳嶔愝寁, 岆摦嶌杊巭愝寁  劆
劆  側偳偺埨慡愝寁傪偍婅偄偟傑偡丅                                          劆
劆丒杮帒椏偵婰嵹偝傟偨惢昳傪桝弌傑偨偼採嫙偡傞応崌偼, 奜崙堊懼媦傃奜崙杅堈  劆
劆  朄偍傛傃暷崙桝弌娗棟娭楢朄婯摍偺婯惂傪偛妋擣偺忋, 昁梫側庤懕偒傪偍偲傝  劆
劆  偔偩偝偄丅                                                              劆
劋劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劅劊
  (C)2011 FUJITSU SEMICONDUCTOR LIMITED Printed in Japan
