# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic WL30K8Vx
GenWL3.menu.pnum.GENERIC_WL30K8VX=Generic WL30K8Vx
GenWL3.menu.pnum.GENERIC_WL30K8VX.upload.maximum_size=65536
GenWL3.menu.pnum.GENERIC_WL30K8VX.upload.maximum_data_size=8192
GenWL3.menu.pnum.GENERIC_WL30K8VX.build.board=GENERIC_WL30K8VX
GenWL3.menu.pnum.GENERIC_WL30K8VX.build.product_line=STM32WL3XX
GenWL3.menu.pnum.GENERIC_WL30K8VX.build.variant=STM32WL3x/WL30K(8-B)V
GenWL3.menu.pnum.GENERIC_WL30K8VX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32WL3x/STM32WL30.svd

# Generic WL30KBVx
GenWL3.menu.pnum.GENERIC_WL30KBVX=Generic WL30KBVx
GenWL3.menu.pnum.GENERIC_WL30KBVX.upload.maximum_size=131072
GenWL3.menu.pnum.GENERIC_WL30KBVX.upload.maximum_data_size=16384
GenWL3.menu.pnum.GENERIC_WL30KBVX.build.board=GENERIC_WL30KBVX
GenWL3.menu.pnum.GENERIC_WL30KBVX.build.product_line=STM32WL3XX
GenWL3.menu.pnum.GENERIC_WL30KBVX.build.variant=STM32WL3x/WL30K(8-B)V
GenWL3.menu.pnum.GENERIC_WL30KBVX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32WL3x/STM32WL30.svd

