# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic G071K8TxN
GenG0.menu.pnum.GENERIC_G071K8TXN=Generic G071K8TxN
GenG0.menu.pnum.GENERIC_G071K8TXN.upload.maximum_size=65536
GenG0.menu.pnum.GENERIC_G071K8TXN.upload.maximum_data_size=36864
GenG0.menu.pnum.GENERIC_G071K8TXN.build.board=GENERIC_G071K8TXN
GenG0.menu.pnum.GENERIC_G071K8TXN.build.product_line=STM32G071xx
GenG0.menu.pnum.GENERIC_G071K8TXN.build.variant=STM32G0xx/G071K(8-B)(T-U)xN_G081KB(T-U)xN
GenG0.menu.pnum.GENERIC_G071K8TXN.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G071.svd

# Generic G071KBTxN
GenG0.menu.pnum.GENERIC_G071KBTXN=Generic G071KBTxN
GenG0.menu.pnum.GENERIC_G071KBTXN.upload.maximum_size=131072
GenG0.menu.pnum.GENERIC_G071KBTXN.upload.maximum_data_size=36864
GenG0.menu.pnum.GENERIC_G071KBTXN.build.board=GENERIC_G071KBTXN
GenG0.menu.pnum.GENERIC_G071KBTXN.build.product_line=STM32G071xx
GenG0.menu.pnum.GENERIC_G071KBTXN.build.variant=STM32G0xx/G071K(8-B)(T-U)xN_G081KB(T-U)xN
GenG0.menu.pnum.GENERIC_G071KBTXN.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G071.svd

# Generic G071K8UxN
GenG0.menu.pnum.GENERIC_G071K8UXN=Generic G071K8UxN
GenG0.menu.pnum.GENERIC_G071K8UXN.upload.maximum_size=65536
GenG0.menu.pnum.GENERIC_G071K8UXN.upload.maximum_data_size=36864
GenG0.menu.pnum.GENERIC_G071K8UXN.build.board=GENERIC_G071K8UXN
GenG0.menu.pnum.GENERIC_G071K8UXN.build.product_line=STM32G071xx
GenG0.menu.pnum.GENERIC_G071K8UXN.build.variant=STM32G0xx/G071K(8-B)(T-U)xN_G081KB(T-U)xN
GenG0.menu.pnum.GENERIC_G071K8UXN.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G071.svd

# Generic G071KBUxN
GenG0.menu.pnum.GENERIC_G071KBUXN=Generic G071KBUxN
GenG0.menu.pnum.GENERIC_G071KBUXN.upload.maximum_size=131072
GenG0.menu.pnum.GENERIC_G071KBUXN.upload.maximum_data_size=36864
GenG0.menu.pnum.GENERIC_G071KBUXN.build.board=GENERIC_G071KBUXN
GenG0.menu.pnum.GENERIC_G071KBUXN.build.product_line=STM32G071xx
GenG0.menu.pnum.GENERIC_G071KBUXN.build.variant=STM32G0xx/G071K(8-B)(T-U)xN_G081KB(T-U)xN
GenG0.menu.pnum.GENERIC_G071KBUXN.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G071.svd

# Generic G081KBTxN
GenG0.menu.pnum.GENERIC_G081KBTXN=Generic G081KBTxN
GenG0.menu.pnum.GENERIC_G081KBTXN.upload.maximum_size=131072
GenG0.menu.pnum.GENERIC_G081KBTXN.upload.maximum_data_size=36864
GenG0.menu.pnum.GENERIC_G081KBTXN.build.board=GENERIC_G081KBTXN
GenG0.menu.pnum.GENERIC_G081KBTXN.build.product_line=STM32G081xx
GenG0.menu.pnum.GENERIC_G081KBTXN.build.variant=STM32G0xx/G071K(8-B)(T-U)xN_G081KB(T-U)xN
GenG0.menu.pnum.GENERIC_G081KBTXN.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G081.svd

# Generic G081KBUxN
GenG0.menu.pnum.GENERIC_G081KBUXN=Generic G081KBUxN
GenG0.menu.pnum.GENERIC_G081KBUXN.upload.maximum_size=131072
GenG0.menu.pnum.GENERIC_G081KBUXN.upload.maximum_data_size=36864
GenG0.menu.pnum.GENERIC_G081KBUXN.build.board=GENERIC_G081KBUXN
GenG0.menu.pnum.GENERIC_G081KBUXN.build.product_line=STM32G081xx
GenG0.menu.pnum.GENERIC_G081KBUXN.build.variant=STM32G0xx/G071K(8-B)(T-U)xN_G081KB(T-U)xN
GenG0.menu.pnum.GENERIC_G081KBUXN.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G081.svd

