# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic WL3RK8Vx
GenWL3.menu.pnum.GENERIC_WL3RK8VX=Generic WL3RK8Vx
GenWL3.menu.pnum.GENERIC_WL3RK8VX.upload.maximum_size=65536
GenWL3.menu.pnum.GENERIC_WL3RK8VX.upload.maximum_data_size=8192
GenWL3.menu.pnum.GENERIC_WL3RK8VX.build.board=GENERIC_WL3RK8VX
GenWL3.menu.pnum.GENERIC_WL3RK8VX.build.product_line=STM32WL3RX
GenWL3.menu.pnum.GENERIC_WL3RK8VX.build.variant=STM32WL3x/WL3RK(8-B)Vx(X)
GenWL3.menu.pnum.GENERIC_WL3RK8VX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32WL3x/STM32WL3R.svd

# Generic WL3RK8VxX
GenWL3.menu.pnum.GENERIC_WL3RK8VXX=Generic WL3RK8VxX
GenWL3.menu.pnum.GENERIC_WL3RK8VXX.upload.maximum_size=65536
GenWL3.menu.pnum.GENERIC_WL3RK8VXX.upload.maximum_data_size=8192
GenWL3.menu.pnum.GENERIC_WL3RK8VXX.build.board=GENERIC_WL3RK8VXX
GenWL3.menu.pnum.GENERIC_WL3RK8VXX.build.product_line=STM32WL3RX
GenWL3.menu.pnum.GENERIC_WL3RK8VXX.build.variant=STM32WL3x/WL3RK(8-B)Vx(X)
GenWL3.menu.pnum.GENERIC_WL3RK8VXX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32WL3x/STM32WL3R.svd

# Generic WL3RKBVx
GenWL3.menu.pnum.GENERIC_WL3RKBVX=Generic WL3RKBVx
GenWL3.menu.pnum.GENERIC_WL3RKBVX.upload.maximum_size=131072
GenWL3.menu.pnum.GENERIC_WL3RKBVX.upload.maximum_data_size=16384
GenWL3.menu.pnum.GENERIC_WL3RKBVX.build.board=GENERIC_WL3RKBVX
GenWL3.menu.pnum.GENERIC_WL3RKBVX.build.product_line=STM32WL3RX
GenWL3.menu.pnum.GENERIC_WL3RKBVX.build.variant=STM32WL3x/WL3RK(8-B)Vx(X)
GenWL3.menu.pnum.GENERIC_WL3RKBVX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32WL3x/STM32WL3R.svd

# Generic WL3RKBVxX
GenWL3.menu.pnum.GENERIC_WL3RKBVXX=Generic WL3RKBVxX
GenWL3.menu.pnum.GENERIC_WL3RKBVXX.upload.maximum_size=131072
GenWL3.menu.pnum.GENERIC_WL3RKBVXX.upload.maximum_data_size=16384
GenWL3.menu.pnum.GENERIC_WL3RKBVXX.build.board=GENERIC_WL3RKBVXX
GenWL3.menu.pnum.GENERIC_WL3RKBVXX.build.product_line=STM32WL3RX
GenWL3.menu.pnum.GENERIC_WL3RKBVXX.build.variant=STM32WL3x/WL3RK(8-B)Vx(X)
GenWL3.menu.pnum.GENERIC_WL3RKBVXX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32WL3x/STM32WL3R.svd

