# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F373V8Hx
GenF3.menu.pnum.GENERIC_F373V8HX=Generic F373V8Hx
GenF3.menu.pnum.GENERIC_F373V8HX.upload.maximum_size=65536
GenF3.menu.pnum.GENERIC_F373V8HX.upload.maximum_data_size=16384
GenF3.menu.pnum.GENERIC_F373V8HX.build.board=GENERIC_F373V8HX
GenF3.menu.pnum.GENERIC_F373V8HX.build.product_line=STM32F373xC
GenF3.menu.pnum.GENERIC_F373V8HX.build.variant=STM32F3xx/F373V(8-B-C)(H-T)
GenF3.menu.pnum.GENERIC_F373V8HX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F373.svd

# Generic F373VBHx
GenF3.menu.pnum.GENERIC_F373VBHX=Generic F373VBHx
GenF3.menu.pnum.GENERIC_F373VBHX.upload.maximum_size=131072
GenF3.menu.pnum.GENERIC_F373VBHX.upload.maximum_data_size=24576
GenF3.menu.pnum.GENERIC_F373VBHX.build.board=GENERIC_F373VBHX
GenF3.menu.pnum.GENERIC_F373VBHX.build.product_line=STM32F373xC
GenF3.menu.pnum.GENERIC_F373VBHX.build.variant=STM32F3xx/F373V(8-B-C)(H-T)
GenF3.menu.pnum.GENERIC_F373VBHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F373.svd

# Generic F373VCHx
GenF3.menu.pnum.GENERIC_F373VCHX=Generic F373VCHx
GenF3.menu.pnum.GENERIC_F373VCHX.upload.maximum_size=262144
GenF3.menu.pnum.GENERIC_F373VCHX.upload.maximum_data_size=32768
GenF3.menu.pnum.GENERIC_F373VCHX.build.board=GENERIC_F373VCHX
GenF3.menu.pnum.GENERIC_F373VCHX.build.product_line=STM32F373xC
GenF3.menu.pnum.GENERIC_F373VCHX.build.variant=STM32F3xx/F373V(8-B-C)(H-T)
GenF3.menu.pnum.GENERIC_F373VCHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F373.svd

# Generic F373V8Tx
GenF3.menu.pnum.GENERIC_F373V8TX=Generic F373V8Tx
GenF3.menu.pnum.GENERIC_F373V8TX.upload.maximum_size=65536
GenF3.menu.pnum.GENERIC_F373V8TX.upload.maximum_data_size=16384
GenF3.menu.pnum.GENERIC_F373V8TX.build.board=GENERIC_F373V8TX
GenF3.menu.pnum.GENERIC_F373V8TX.build.product_line=STM32F373xC
GenF3.menu.pnum.GENERIC_F373V8TX.build.variant=STM32F3xx/F373V(8-B-C)(H-T)
GenF3.menu.pnum.GENERIC_F373V8TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F373.svd

# Generic F373VBTx
GenF3.menu.pnum.GENERIC_F373VBTX=Generic F373VBTx
GenF3.menu.pnum.GENERIC_F373VBTX.upload.maximum_size=131072
GenF3.menu.pnum.GENERIC_F373VBTX.upload.maximum_data_size=24576
GenF3.menu.pnum.GENERIC_F373VBTX.build.board=GENERIC_F373VBTX
GenF3.menu.pnum.GENERIC_F373VBTX.build.product_line=STM32F373xC
GenF3.menu.pnum.GENERIC_F373VBTX.build.variant=STM32F3xx/F373V(8-B-C)(H-T)
GenF3.menu.pnum.GENERIC_F373VBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F373.svd

# Generic F373VCTx
GenF3.menu.pnum.GENERIC_F373VCTX=Generic F373VCTx
GenF3.menu.pnum.GENERIC_F373VCTX.upload.maximum_size=262144
GenF3.menu.pnum.GENERIC_F373VCTX.upload.maximum_data_size=32768
GenF3.menu.pnum.GENERIC_F373VCTX.build.board=GENERIC_F373VCTX
GenF3.menu.pnum.GENERIC_F373VCTX.build.product_line=STM32F373xC
GenF3.menu.pnum.GENERIC_F373VCTX.build.variant=STM32F3xx/F373V(8-B-C)(H-T)
GenF3.menu.pnum.GENERIC_F373VCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F373.svd

