# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F205ZCTx
GenF2.menu.pnum.GENERIC_F205ZCTX=Generic F205ZCTx
GenF2.menu.pnum.GENERIC_F205ZCTX.upload.maximum_size=262144
GenF2.menu.pnum.GENERIC_F205ZCTX.upload.maximum_data_size=98304
GenF2.menu.pnum.GENERIC_F205ZCTX.build.board=GENERIC_F205ZCTX
GenF2.menu.pnum.GENERIC_F205ZCTX.build.product_line=STM32F205xx
GenF2.menu.pnum.GENERIC_F205ZCTX.build.variant=STM32F2xx/F205Z(C-E-F-G)T_F215Z(E-G)T
GenF2.menu.pnum.GENERIC_F205ZCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F2xx/STM32F205.svd

# Generic F205ZETx
GenF2.menu.pnum.GENERIC_F205ZETX=Generic F205ZETx
GenF2.menu.pnum.GENERIC_F205ZETX.upload.maximum_size=524288
GenF2.menu.pnum.GENERIC_F205ZETX.upload.maximum_data_size=131072
GenF2.menu.pnum.GENERIC_F205ZETX.build.board=GENERIC_F205ZETX
GenF2.menu.pnum.GENERIC_F205ZETX.build.product_line=STM32F205xx
GenF2.menu.pnum.GENERIC_F205ZETX.build.variant=STM32F2xx/F205Z(C-E-F-G)T_F215Z(E-G)T
GenF2.menu.pnum.GENERIC_F205ZETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F2xx/STM32F205.svd

# Generic F205ZFTx
GenF2.menu.pnum.GENERIC_F205ZFTX=Generic F205ZFTx
GenF2.menu.pnum.GENERIC_F205ZFTX.upload.maximum_size=786432
GenF2.menu.pnum.GENERIC_F205ZFTX.upload.maximum_data_size=131072
GenF2.menu.pnum.GENERIC_F205ZFTX.build.board=GENERIC_F205ZFTX
GenF2.menu.pnum.GENERIC_F205ZFTX.build.product_line=STM32F205xx
GenF2.menu.pnum.GENERIC_F205ZFTX.build.variant=STM32F2xx/F205Z(C-E-F-G)T_F215Z(E-G)T
GenF2.menu.pnum.GENERIC_F205ZFTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F2xx/STM32F205.svd

# Generic F205ZGTx
GenF2.menu.pnum.GENERIC_F205ZGTX=Generic F205ZGTx
GenF2.menu.pnum.GENERIC_F205ZGTX.upload.maximum_size=1048576
GenF2.menu.pnum.GENERIC_F205ZGTX.upload.maximum_data_size=131072
GenF2.menu.pnum.GENERIC_F205ZGTX.build.board=GENERIC_F205ZGTX
GenF2.menu.pnum.GENERIC_F205ZGTX.build.product_line=STM32F205xx
GenF2.menu.pnum.GENERIC_F205ZGTX.build.variant=STM32F2xx/F205Z(C-E-F-G)T_F215Z(E-G)T
GenF2.menu.pnum.GENERIC_F205ZGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F2xx/STM32F205.svd

# Generic F215ZETx
GenF2.menu.pnum.GENERIC_F215ZETX=Generic F215ZETx
GenF2.menu.pnum.GENERIC_F215ZETX.upload.maximum_size=524288
GenF2.menu.pnum.GENERIC_F215ZETX.upload.maximum_data_size=131072
GenF2.menu.pnum.GENERIC_F215ZETX.build.board=GENERIC_F215ZETX
GenF2.menu.pnum.GENERIC_F215ZETX.build.product_line=STM32F215xx
GenF2.menu.pnum.GENERIC_F215ZETX.build.variant=STM32F2xx/F205Z(C-E-F-G)T_F215Z(E-G)T
GenF2.menu.pnum.GENERIC_F215ZETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F2xx/STM32F215.svd

# Generic F215ZGTx
GenF2.menu.pnum.GENERIC_F215ZGTX=Generic F215ZGTx
GenF2.menu.pnum.GENERIC_F215ZGTX.upload.maximum_size=1048576
GenF2.menu.pnum.GENERIC_F215ZGTX.upload.maximum_data_size=131072
GenF2.menu.pnum.GENERIC_F215ZGTX.build.board=GENERIC_F215ZGTX
GenF2.menu.pnum.GENERIC_F215ZGTX.build.product_line=STM32F215xx
GenF2.menu.pnum.GENERIC_F215ZGTX.build.variant=STM32F2xx/F205Z(C-E-F-G)T_F215Z(E-G)T
GenF2.menu.pnum.GENERIC_F215ZGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F2xx/STM32F215.svd

