# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L010F4Px
GenL0.menu.pnum.GENERIC_L010F4PX=Generic L010F4Px
GenL0.menu.pnum.GENERIC_L010F4PX.upload.maximum_size=16384
GenL0.menu.pnum.GENERIC_L010F4PX.upload.maximum_data_size=2048
GenL0.menu.pnum.GENERIC_L010F4PX.build.board=GENERIC_L010F4PX
GenL0.menu.pnum.GENERIC_L010F4PX.build.product_line=STM32L010x4
GenL0.menu.pnum.GENERIC_L010F4PX.build.variant=STM32L0xx/L010F4P_L011F(3-4)P_L021F4P
GenL0.menu.pnum.GENERIC_L010F4PX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x0.svd

# Generic L011F3Px
GenL0.menu.pnum.GENERIC_L011F3PX=Generic L011F3Px
GenL0.menu.pnum.GENERIC_L011F3PX.upload.maximum_size=8192
GenL0.menu.pnum.GENERIC_L011F3PX.upload.maximum_data_size=2048
GenL0.menu.pnum.GENERIC_L011F3PX.build.board=GENERIC_L011F3PX
GenL0.menu.pnum.GENERIC_L011F3PX.build.product_line=STM32L011xx
GenL0.menu.pnum.GENERIC_L011F3PX.build.variant=STM32L0xx/L010F4P_L011F(3-4)P_L021F4P
GenL0.menu.pnum.GENERIC_L011F3PX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

# Generic L011F4Px
GenL0.menu.pnum.GENERIC_L011F4PX=Generic L011F4Px
GenL0.menu.pnum.GENERIC_L011F4PX.upload.maximum_size=16384
GenL0.menu.pnum.GENERIC_L011F4PX.upload.maximum_data_size=2048
GenL0.menu.pnum.GENERIC_L011F4PX.build.board=GENERIC_L011F4PX
GenL0.menu.pnum.GENERIC_L011F4PX.build.product_line=STM32L011xx
GenL0.menu.pnum.GENERIC_L011F4PX.build.variant=STM32L0xx/L010F4P_L011F(3-4)P_L021F4P
GenL0.menu.pnum.GENERIC_L011F4PX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

# Generic L021F4Px
GenL0.menu.pnum.GENERIC_L021F4PX=Generic L021F4Px
GenL0.menu.pnum.GENERIC_L021F4PX.upload.maximum_size=16384
GenL0.menu.pnum.GENERIC_L021F4PX.upload.maximum_data_size=2048
GenL0.menu.pnum.GENERIC_L021F4PX.build.board=GENERIC_L021F4PX
GenL0.menu.pnum.GENERIC_L021F4PX.build.product_line=STM32L021xx
GenL0.menu.pnum.GENERIC_L021F4PX.build.variant=STM32L0xx/L010F4P_L011F(3-4)P_L021F4P
GenL0.menu.pnum.GENERIC_L021F4PX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

