# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L4R9ZGJx
GenL4.menu.pnum.GENERIC_L4R9ZGJX=Generic L4R9ZGJx
GenL4.menu.pnum.GENERIC_L4R9ZGJX.upload.maximum_size=1048576
GenL4.menu.pnum.GENERIC_L4R9ZGJX.upload.maximum_data_size=655360
GenL4.menu.pnum.GENERIC_L4R9ZGJX.build.board=GENERIC_L4R9ZGJX
GenL4.menu.pnum.GENERIC_L4R9ZGJX.build.product_line=STM32L4R9xx
GenL4.menu.pnum.GENERIC_L4R9ZGJX.build.variant=STM32L4xx/L4R9Z(G-I)J_L4S9ZIJ
GenL4.menu.pnum.GENERIC_L4R9ZGJX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L4R9.svd

# Generic L4R9ZIJx
GenL4.menu.pnum.GENERIC_L4R9ZIJX=Generic L4R9ZIJx
GenL4.menu.pnum.GENERIC_L4R9ZIJX.upload.maximum_size=2097152
GenL4.menu.pnum.GENERIC_L4R9ZIJX.upload.maximum_data_size=655360
GenL4.menu.pnum.GENERIC_L4R9ZIJX.build.board=GENERIC_L4R9ZIJX
GenL4.menu.pnum.GENERIC_L4R9ZIJX.build.product_line=STM32L4R9xx
GenL4.menu.pnum.GENERIC_L4R9ZIJX.build.variant=STM32L4xx/L4R9Z(G-I)J_L4S9ZIJ
GenL4.menu.pnum.GENERIC_L4R9ZIJX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L4R9.svd

# Generic L4S9ZIJx
GenL4.menu.pnum.GENERIC_L4S9ZIJX=Generic L4S9ZIJx
GenL4.menu.pnum.GENERIC_L4S9ZIJX.upload.maximum_size=2097152
GenL4.menu.pnum.GENERIC_L4S9ZIJX.upload.maximum_data_size=655360
GenL4.menu.pnum.GENERIC_L4S9ZIJX.build.board=GENERIC_L4S9ZIJX
GenL4.menu.pnum.GENERIC_L4S9ZIJX.build.product_line=STM32L4S9xx
GenL4.menu.pnum.GENERIC_L4S9ZIJX.build.variant=STM32L4xx/L4R9Z(G-I)J_L4S9ZIJ
GenL4.menu.pnum.GENERIC_L4S9ZIJX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L4S9.svd

