# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F401RBTx
GenF4.menu.pnum.GENERIC_F401RBTX=Generic F401RBTx
GenF4.menu.pnum.GENERIC_F401RBTX.upload.maximum_size=131072
GenF4.menu.pnum.GENERIC_F401RBTX.upload.maximum_data_size=65536
GenF4.menu.pnum.GENERIC_F401RBTX.build.board=GENERIC_F401RBTX
GenF4.menu.pnum.GENERIC_F401RBTX.build.product_line=STM32F401xC
GenF4.menu.pnum.GENERIC_F401RBTX.build.variant=STM32F4xx/F401R(B-C-D-E)T
GenF4.menu.pnum.GENERIC_F401RBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F401.svd

# Generic F401RCTx
GenF4.menu.pnum.GENERIC_F401RCTX=Generic F401RCTx
GenF4.menu.pnum.GENERIC_F401RCTX.upload.maximum_size=262144
GenF4.menu.pnum.GENERIC_F401RCTX.upload.maximum_data_size=65536
GenF4.menu.pnum.GENERIC_F401RCTX.build.board=GENERIC_F401RCTX
GenF4.menu.pnum.GENERIC_F401RCTX.build.product_line=STM32F401xC
GenF4.menu.pnum.GENERIC_F401RCTX.build.variant=STM32F4xx/F401R(B-C-D-E)T
GenF4.menu.pnum.GENERIC_F401RCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F401.svd

# Generic F401RDTx
GenF4.menu.pnum.GENERIC_F401RDTX=Generic F401RDTx
GenF4.menu.pnum.GENERIC_F401RDTX.upload.maximum_size=393216
GenF4.menu.pnum.GENERIC_F401RDTX.upload.maximum_data_size=98304
GenF4.menu.pnum.GENERIC_F401RDTX.build.board=GENERIC_F401RDTX
GenF4.menu.pnum.GENERIC_F401RDTX.build.product_line=STM32F401xE
GenF4.menu.pnum.GENERIC_F401RDTX.build.variant=STM32F4xx/F401R(B-C-D-E)T
GenF4.menu.pnum.GENERIC_F401RDTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F401.svd

# Generic F401RETx
GenF4.menu.pnum.GENERIC_F401RETX=Generic F401RETx
GenF4.menu.pnum.GENERIC_F401RETX.upload.maximum_size=524288
GenF4.menu.pnum.GENERIC_F401RETX.upload.maximum_data_size=98304
GenF4.menu.pnum.GENERIC_F401RETX.build.board=GENERIC_F401RETX
GenF4.menu.pnum.GENERIC_F401RETX.build.product_line=STM32F401xE
GenF4.menu.pnum.GENERIC_F401RETX.build.variant=STM32F4xx/F401R(B-C-D-E)T
GenF4.menu.pnum.GENERIC_F401RETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F401.svd

