# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F723VCTx
GenF7.menu.pnum.GENERIC_F723VCTX=Generic F723VCTx
GenF7.menu.pnum.GENERIC_F723VCTX.upload.maximum_size=262144
GenF7.menu.pnum.GENERIC_F723VCTX.upload.maximum_data_size=196608
GenF7.menu.pnum.GENERIC_F723VCTX.build.board=GENERIC_F723VCTX
GenF7.menu.pnum.GENERIC_F723VCTX.build.product_line=STM32F723xx
GenF7.menu.pnum.GENERIC_F723VCTX.build.variant=STM32F7xx/F723V(C-E)(T-Y)_F733VE(T-Y)
GenF7.menu.pnum.GENERIC_F723VCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F723.svd

# Generic F723VETx
GenF7.menu.pnum.GENERIC_F723VETX=Generic F723VETx
GenF7.menu.pnum.GENERIC_F723VETX.upload.maximum_size=524288
GenF7.menu.pnum.GENERIC_F723VETX.upload.maximum_data_size=196608
GenF7.menu.pnum.GENERIC_F723VETX.build.board=GENERIC_F723VETX
GenF7.menu.pnum.GENERIC_F723VETX.build.product_line=STM32F723xx
GenF7.menu.pnum.GENERIC_F723VETX.build.variant=STM32F7xx/F723V(C-E)(T-Y)_F733VE(T-Y)
GenF7.menu.pnum.GENERIC_F723VETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F723.svd

# Generic F723VCYx
GenF7.menu.pnum.GENERIC_F723VCYX=Generic F723VCYx
GenF7.menu.pnum.GENERIC_F723VCYX.upload.maximum_size=262144
GenF7.menu.pnum.GENERIC_F723VCYX.upload.maximum_data_size=196608
GenF7.menu.pnum.GENERIC_F723VCYX.build.board=GENERIC_F723VCYX
GenF7.menu.pnum.GENERIC_F723VCYX.build.product_line=STM32F723xx
GenF7.menu.pnum.GENERIC_F723VCYX.build.variant=STM32F7xx/F723V(C-E)(T-Y)_F733VE(T-Y)
GenF7.menu.pnum.GENERIC_F723VCYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F723.svd

# Generic F723VEYx
GenF7.menu.pnum.GENERIC_F723VEYX=Generic F723VEYx
GenF7.menu.pnum.GENERIC_F723VEYX.upload.maximum_size=524288
GenF7.menu.pnum.GENERIC_F723VEYX.upload.maximum_data_size=196608
GenF7.menu.pnum.GENERIC_F723VEYX.build.board=GENERIC_F723VEYX
GenF7.menu.pnum.GENERIC_F723VEYX.build.product_line=STM32F723xx
GenF7.menu.pnum.GENERIC_F723VEYX.build.variant=STM32F7xx/F723V(C-E)(T-Y)_F733VE(T-Y)
GenF7.menu.pnum.GENERIC_F723VEYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F723.svd

# Generic F733VETx
GenF7.menu.pnum.GENERIC_F733VETX=Generic F733VETx
GenF7.menu.pnum.GENERIC_F733VETX.upload.maximum_size=524288
GenF7.menu.pnum.GENERIC_F733VETX.upload.maximum_data_size=196608
GenF7.menu.pnum.GENERIC_F733VETX.build.board=GENERIC_F733VETX
GenF7.menu.pnum.GENERIC_F733VETX.build.product_line=STM32F733xx
GenF7.menu.pnum.GENERIC_F733VETX.build.variant=STM32F7xx/F723V(C-E)(T-Y)_F733VE(T-Y)
GenF7.menu.pnum.GENERIC_F733VETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F733.svd

# Generic F733VEYx
GenF7.menu.pnum.GENERIC_F733VEYX=Generic F733VEYx
GenF7.menu.pnum.GENERIC_F733VEYX.upload.maximum_size=524288
GenF7.menu.pnum.GENERIC_F733VEYX.upload.maximum_data_size=196608
GenF7.menu.pnum.GENERIC_F733VEYX.build.board=GENERIC_F733VEYX
GenF7.menu.pnum.GENERIC_F733VEYX.build.product_line=STM32F733xx
GenF7.menu.pnum.GENERIC_F733VEYX.build.variant=STM32F7xx/F723V(C-E)(T-Y)_F733VE(T-Y)
GenF7.menu.pnum.GENERIC_F733VEYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F733.svd

