# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F765IGKx
GenF7.menu.pnum.GENERIC_F765IGKX=Generic F765IGKx
GenF7.menu.pnum.GENERIC_F765IGKX.upload.maximum_size=1048576
GenF7.menu.pnum.GENERIC_F765IGKX.upload.maximum_data_size=393216
GenF7.menu.pnum.GENERIC_F765IGKX.build.board=GENERIC_F765IGKX
GenF7.menu.pnum.GENERIC_F765IGKX.build.product_line=STM32F765xx
GenF7.menu.pnum.GENERIC_F765IGKX.build.variant=STM32F7xx/F765I(G-I)(K-T)_F767I(G-I)(K-T)_F777II(K-T)
GenF7.menu.pnum.GENERIC_F765IGKX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F765.svd

# Generic F765IIKx
GenF7.menu.pnum.GENERIC_F765IIKX=Generic F765IIKx
GenF7.menu.pnum.GENERIC_F765IIKX.upload.maximum_size=2097152
GenF7.menu.pnum.GENERIC_F765IIKX.upload.maximum_data_size=393216
GenF7.menu.pnum.GENERIC_F765IIKX.build.board=GENERIC_F765IIKX
GenF7.menu.pnum.GENERIC_F765IIKX.build.product_line=STM32F765xx
GenF7.menu.pnum.GENERIC_F765IIKX.build.variant=STM32F7xx/F765I(G-I)(K-T)_F767I(G-I)(K-T)_F777II(K-T)
GenF7.menu.pnum.GENERIC_F765IIKX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F765.svd

# Generic F765IGTx
GenF7.menu.pnum.GENERIC_F765IGTX=Generic F765IGTx
GenF7.menu.pnum.GENERIC_F765IGTX.upload.maximum_size=1048576
GenF7.menu.pnum.GENERIC_F765IGTX.upload.maximum_data_size=393216
GenF7.menu.pnum.GENERIC_F765IGTX.build.board=GENERIC_F765IGTX
GenF7.menu.pnum.GENERIC_F765IGTX.build.product_line=STM32F765xx
GenF7.menu.pnum.GENERIC_F765IGTX.build.variant=STM32F7xx/F765I(G-I)(K-T)_F767I(G-I)(K-T)_F777II(K-T)
GenF7.menu.pnum.GENERIC_F765IGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F765.svd

# Generic F765IITx
GenF7.menu.pnum.GENERIC_F765IITX=Generic F765IITx
GenF7.menu.pnum.GENERIC_F765IITX.upload.maximum_size=2097152
GenF7.menu.pnum.GENERIC_F765IITX.upload.maximum_data_size=393216
GenF7.menu.pnum.GENERIC_F765IITX.build.board=GENERIC_F765IITX
GenF7.menu.pnum.GENERIC_F765IITX.build.product_line=STM32F765xx
GenF7.menu.pnum.GENERIC_F765IITX.build.variant=STM32F7xx/F765I(G-I)(K-T)_F767I(G-I)(K-T)_F777II(K-T)
GenF7.menu.pnum.GENERIC_F765IITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F765.svd

# Generic F767IGKx
GenF7.menu.pnum.GENERIC_F767IGKX=Generic F767IGKx
GenF7.menu.pnum.GENERIC_F767IGKX.upload.maximum_size=1048576
GenF7.menu.pnum.GENERIC_F767IGKX.upload.maximum_data_size=393216
GenF7.menu.pnum.GENERIC_F767IGKX.build.board=GENERIC_F767IGKX
GenF7.menu.pnum.GENERIC_F767IGKX.build.product_line=STM32F767xx
GenF7.menu.pnum.GENERIC_F767IGKX.build.variant=STM32F7xx/F765I(G-I)(K-T)_F767I(G-I)(K-T)_F777II(K-T)
GenF7.menu.pnum.GENERIC_F767IGKX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F767.svd

# Generic F767IIKx
GenF7.menu.pnum.GENERIC_F767IIKX=Generic F767IIKx
GenF7.menu.pnum.GENERIC_F767IIKX.upload.maximum_size=2097152
GenF7.menu.pnum.GENERIC_F767IIKX.upload.maximum_data_size=393216
GenF7.menu.pnum.GENERIC_F767IIKX.build.board=GENERIC_F767IIKX
GenF7.menu.pnum.GENERIC_F767IIKX.build.product_line=STM32F767xx
GenF7.menu.pnum.GENERIC_F767IIKX.build.variant=STM32F7xx/F765I(G-I)(K-T)_F767I(G-I)(K-T)_F777II(K-T)
GenF7.menu.pnum.GENERIC_F767IIKX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F767.svd

# Generic F767IGTx
GenF7.menu.pnum.GENERIC_F767IGTX=Generic F767IGTx
GenF7.menu.pnum.GENERIC_F767IGTX.upload.maximum_size=1048576
GenF7.menu.pnum.GENERIC_F767IGTX.upload.maximum_data_size=393216
GenF7.menu.pnum.GENERIC_F767IGTX.build.board=GENERIC_F767IGTX
GenF7.menu.pnum.GENERIC_F767IGTX.build.product_line=STM32F767xx
GenF7.menu.pnum.GENERIC_F767IGTX.build.variant=STM32F7xx/F765I(G-I)(K-T)_F767I(G-I)(K-T)_F777II(K-T)
GenF7.menu.pnum.GENERIC_F767IGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F767.svd

# Generic F767IITx
GenF7.menu.pnum.GENERIC_F767IITX=Generic F767IITx
GenF7.menu.pnum.GENERIC_F767IITX.upload.maximum_size=2097152
GenF7.menu.pnum.GENERIC_F767IITX.upload.maximum_data_size=393216
GenF7.menu.pnum.GENERIC_F767IITX.build.board=GENERIC_F767IITX
GenF7.menu.pnum.GENERIC_F767IITX.build.product_line=STM32F767xx
GenF7.menu.pnum.GENERIC_F767IITX.build.variant=STM32F7xx/F765I(G-I)(K-T)_F767I(G-I)(K-T)_F777II(K-T)
GenF7.menu.pnum.GENERIC_F767IITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F767.svd

# Generic F777IIKx
GenF7.menu.pnum.GENERIC_F777IIKX=Generic F777IIKx
GenF7.menu.pnum.GENERIC_F777IIKX.upload.maximum_size=2097152
GenF7.menu.pnum.GENERIC_F777IIKX.upload.maximum_data_size=393216
GenF7.menu.pnum.GENERIC_F777IIKX.build.board=GENERIC_F777IIKX
GenF7.menu.pnum.GENERIC_F777IIKX.build.product_line=STM32F777xx
GenF7.menu.pnum.GENERIC_F777IIKX.build.variant=STM32F7xx/F765I(G-I)(K-T)_F767I(G-I)(K-T)_F777II(K-T)
GenF7.menu.pnum.GENERIC_F777IIKX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F777.svd

# Generic F777IITx
GenF7.menu.pnum.GENERIC_F777IITX=Generic F777IITx
GenF7.menu.pnum.GENERIC_F777IITX.upload.maximum_size=2097152
GenF7.menu.pnum.GENERIC_F777IITX.upload.maximum_data_size=393216
GenF7.menu.pnum.GENERIC_F777IITX.build.board=GENERIC_F777IITX
GenF7.menu.pnum.GENERIC_F777IITX.build.product_line=STM32F777xx
GenF7.menu.pnum.GENERIC_F777IITX.build.variant=STM32F7xx/F765I(G-I)(K-T)_F767I(G-I)(K-T)_F777II(K-T)
GenF7.menu.pnum.GENERIC_F777IITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F777.svd

