# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic G0B1NEYx
GenG0.menu.pnum.GENERIC_G0B1NEYX=Generic G0B1NEYx
GenG0.menu.pnum.GENERIC_G0B1NEYX.upload.maximum_size=524288
GenG0.menu.pnum.GENERIC_G0B1NEYX.upload.maximum_data_size=147456
GenG0.menu.pnum.GENERIC_G0B1NEYX.build.board=GENERIC_G0B1NEYX
GenG0.menu.pnum.GENERIC_G0B1NEYX.build.product_line=STM32G0B1xx
GenG0.menu.pnum.GENERIC_G0B1NEYX.build.variant=STM32G0xx/G0B1NEY_G0C1NEY
GenG0.menu.pnum.GENERIC_G0B1NEYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G0B1.svd

# Generic G0C1NEYx
GenG0.menu.pnum.GENERIC_G0C1NEYX=Generic G0C1NEYx
GenG0.menu.pnum.GENERIC_G0C1NEYX.upload.maximum_size=524288
GenG0.menu.pnum.GENERIC_G0C1NEYX.upload.maximum_data_size=147456
GenG0.menu.pnum.GENERIC_G0C1NEYX.build.board=GENERIC_G0C1NEYX
GenG0.menu.pnum.GENERIC_G0C1NEYX.build.product_line=STM32G0C1xx
GenG0.menu.pnum.GENERIC_G0C1NEYX.build.variant=STM32G0xx/G0B1NEY_G0C1NEY
GenG0.menu.pnum.GENERIC_G0C1NEYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G0C1.svd

