# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic G473CBUx
GenG4.menu.pnum.GENERIC_G473CBUX=Generic G473CBUx
GenG4.menu.pnum.GENERIC_G473CBUX.upload.maximum_size=131072
GenG4.menu.pnum.GENERIC_G473CBUX.upload.maximum_data_size=131072
GenG4.menu.pnum.GENERIC_G473CBUX.build.board=GENERIC_G473CBUX
GenG4.menu.pnum.GENERIC_G473CBUX.build.product_line=STM32G473xx
GenG4.menu.pnum.GENERIC_G473CBUX.build.variant=STM32G4xx/G473C(B-C-E)U_G474C(B-C-E)U_G483CEU_G484CEU
GenG4.menu.pnum.GENERIC_G473CBUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G473.svd

# Generic G473CCUx
GenG4.menu.pnum.GENERIC_G473CCUX=Generic G473CCUx
GenG4.menu.pnum.GENERIC_G473CCUX.upload.maximum_size=262144
GenG4.menu.pnum.GENERIC_G473CCUX.upload.maximum_data_size=131072
GenG4.menu.pnum.GENERIC_G473CCUX.build.board=GENERIC_G473CCUX
GenG4.menu.pnum.GENERIC_G473CCUX.build.product_line=STM32G473xx
GenG4.menu.pnum.GENERIC_G473CCUX.build.variant=STM32G4xx/G473C(B-C-E)U_G474C(B-C-E)U_G483CEU_G484CEU
GenG4.menu.pnum.GENERIC_G473CCUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G473.svd

# Generic G473CEUx
GenG4.menu.pnum.GENERIC_G473CEUX=Generic G473CEUx
GenG4.menu.pnum.GENERIC_G473CEUX.upload.maximum_size=524288
GenG4.menu.pnum.GENERIC_G473CEUX.upload.maximum_data_size=131072
GenG4.menu.pnum.GENERIC_G473CEUX.build.board=GENERIC_G473CEUX
GenG4.menu.pnum.GENERIC_G473CEUX.build.product_line=STM32G473xx
GenG4.menu.pnum.GENERIC_G473CEUX.build.variant=STM32G4xx/G473C(B-C-E)U_G474C(B-C-E)U_G483CEU_G484CEU
GenG4.menu.pnum.GENERIC_G473CEUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G473.svd

# Generic G474CBUx
GenG4.menu.pnum.GENERIC_G474CBUX=Generic G474CBUx
GenG4.menu.pnum.GENERIC_G474CBUX.upload.maximum_size=131072
GenG4.menu.pnum.GENERIC_G474CBUX.upload.maximum_data_size=131072
GenG4.menu.pnum.GENERIC_G474CBUX.build.board=GENERIC_G474CBUX
GenG4.menu.pnum.GENERIC_G474CBUX.build.product_line=STM32G474xx
GenG4.menu.pnum.GENERIC_G474CBUX.build.variant=STM32G4xx/G473C(B-C-E)U_G474C(B-C-E)U_G483CEU_G484CEU
GenG4.menu.pnum.GENERIC_G474CBUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G474.svd

# Generic G474CCUx
GenG4.menu.pnum.GENERIC_G474CCUX=Generic G474CCUx
GenG4.menu.pnum.GENERIC_G474CCUX.upload.maximum_size=262144
GenG4.menu.pnum.GENERIC_G474CCUX.upload.maximum_data_size=131072
GenG4.menu.pnum.GENERIC_G474CCUX.build.board=GENERIC_G474CCUX
GenG4.menu.pnum.GENERIC_G474CCUX.build.product_line=STM32G474xx
GenG4.menu.pnum.GENERIC_G474CCUX.build.variant=STM32G4xx/G473C(B-C-E)U_G474C(B-C-E)U_G483CEU_G484CEU
GenG4.menu.pnum.GENERIC_G474CCUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G474.svd

# Generic G474CEUx
GenG4.menu.pnum.GENERIC_G474CEUX=Generic G474CEUx
GenG4.menu.pnum.GENERIC_G474CEUX.upload.maximum_size=524288
GenG4.menu.pnum.GENERIC_G474CEUX.upload.maximum_data_size=131072
GenG4.menu.pnum.GENERIC_G474CEUX.build.board=GENERIC_G474CEUX
GenG4.menu.pnum.GENERIC_G474CEUX.build.product_line=STM32G474xx
GenG4.menu.pnum.GENERIC_G474CEUX.build.variant=STM32G4xx/G473C(B-C-E)U_G474C(B-C-E)U_G483CEU_G484CEU
GenG4.menu.pnum.GENERIC_G474CEUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G474.svd

# Generic G483CEUx
GenG4.menu.pnum.GENERIC_G483CEUX=Generic G483CEUx
GenG4.menu.pnum.GENERIC_G483CEUX.upload.maximum_size=524288
GenG4.menu.pnum.GENERIC_G483CEUX.upload.maximum_data_size=131072
GenG4.menu.pnum.GENERIC_G483CEUX.build.board=GENERIC_G483CEUX
GenG4.menu.pnum.GENERIC_G483CEUX.build.product_line=STM32G483xx
GenG4.menu.pnum.GENERIC_G483CEUX.build.variant=STM32G4xx/G473C(B-C-E)U_G474C(B-C-E)U_G483CEU_G484CEU
GenG4.menu.pnum.GENERIC_G483CEUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G483.svd

# Generic G484CEUx
GenG4.menu.pnum.GENERIC_G484CEUX=Generic G484CEUx
GenG4.menu.pnum.GENERIC_G484CEUX.upload.maximum_size=524288
GenG4.menu.pnum.GENERIC_G484CEUX.upload.maximum_data_size=131072
GenG4.menu.pnum.GENERIC_G484CEUX.build.board=GENERIC_G484CEUX
GenG4.menu.pnum.GENERIC_G484CEUX.build.product_line=STM32G484xx
GenG4.menu.pnum.GENERIC_G484CEUX.build.variant=STM32G4xx/G473C(B-C-E)U_G474C(B-C-E)U_G483CEU_G484CEU
GenG4.menu.pnum.GENERIC_G484CEUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G484.svd

