# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L431RBIx
GenL4.menu.pnum.GENERIC_L431RBIX=Generic L431RBIx
GenL4.menu.pnum.GENERIC_L431RBIX.upload.maximum_size=131072
GenL4.menu.pnum.GENERIC_L431RBIX.upload.maximum_data_size=65536
GenL4.menu.pnum.GENERIC_L431RBIX.build.board=GENERIC_L431RBIX
GenL4.menu.pnum.GENERIC_L431RBIX.build.product_line=STM32L431xx
GenL4.menu.pnum.GENERIC_L431RBIX.build.variant=STM32L4xx/L431R(B-C)(I-T-Y)
GenL4.menu.pnum.GENERIC_L431RBIX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L431.svd

# Generic L431RCIx
GenL4.menu.pnum.GENERIC_L431RCIX=Generic L431RCIx
GenL4.menu.pnum.GENERIC_L431RCIX.upload.maximum_size=262144
GenL4.menu.pnum.GENERIC_L431RCIX.upload.maximum_data_size=65536
GenL4.menu.pnum.GENERIC_L431RCIX.build.board=GENERIC_L431RCIX
GenL4.menu.pnum.GENERIC_L431RCIX.build.product_line=STM32L431xx
GenL4.menu.pnum.GENERIC_L431RCIX.build.variant=STM32L4xx/L431R(B-C)(I-T-Y)
GenL4.menu.pnum.GENERIC_L431RCIX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L431.svd

# Generic L431RBTx
GenL4.menu.pnum.GENERIC_L431RBTX=Generic L431RBTx
GenL4.menu.pnum.GENERIC_L431RBTX.upload.maximum_size=131072
GenL4.menu.pnum.GENERIC_L431RBTX.upload.maximum_data_size=65536
GenL4.menu.pnum.GENERIC_L431RBTX.build.board=GENERIC_L431RBTX
GenL4.menu.pnum.GENERIC_L431RBTX.build.product_line=STM32L431xx
GenL4.menu.pnum.GENERIC_L431RBTX.build.variant=STM32L4xx/L431R(B-C)(I-T-Y)
GenL4.menu.pnum.GENERIC_L431RBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L431.svd

# Generic L431RCTx
GenL4.menu.pnum.GENERIC_L431RCTX=Generic L431RCTx
GenL4.menu.pnum.GENERIC_L431RCTX.upload.maximum_size=262144
GenL4.menu.pnum.GENERIC_L431RCTX.upload.maximum_data_size=65536
GenL4.menu.pnum.GENERIC_L431RCTX.build.board=GENERIC_L431RCTX
GenL4.menu.pnum.GENERIC_L431RCTX.build.product_line=STM32L431xx
GenL4.menu.pnum.GENERIC_L431RCTX.build.variant=STM32L4xx/L431R(B-C)(I-T-Y)
GenL4.menu.pnum.GENERIC_L431RCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L431.svd

# Generic L431RBYx
GenL4.menu.pnum.GENERIC_L431RBYX=Generic L431RBYx
GenL4.menu.pnum.GENERIC_L431RBYX.upload.maximum_size=131072
GenL4.menu.pnum.GENERIC_L431RBYX.upload.maximum_data_size=65536
GenL4.menu.pnum.GENERIC_L431RBYX.build.board=GENERIC_L431RBYX
GenL4.menu.pnum.GENERIC_L431RBYX.build.product_line=STM32L431xx
GenL4.menu.pnum.GENERIC_L431RBYX.build.variant=STM32L4xx/L431R(B-C)(I-T-Y)
GenL4.menu.pnum.GENERIC_L431RBYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L431.svd

# Generic L431RCYx
GenL4.menu.pnum.GENERIC_L431RCYX=Generic L431RCYx
GenL4.menu.pnum.GENERIC_L431RCYX.upload.maximum_size=262144
GenL4.menu.pnum.GENERIC_L431RCYX.upload.maximum_data_size=65536
GenL4.menu.pnum.GENERIC_L431RCYX.build.board=GENERIC_L431RCYX
GenL4.menu.pnum.GENERIC_L431RCYX.build.product_line=STM32L431xx
GenL4.menu.pnum.GENERIC_L431RCYX.build.variant=STM32L4xx/L431R(B-C)(I-T-Y)
GenL4.menu.pnum.GENERIC_L431RCYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L431.svd

