# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F469BETx
GenF4.menu.pnum.GENERIC_F469BETX=Generic F469BETx
GenF4.menu.pnum.GENERIC_F469BETX.upload.maximum_size=524288
GenF4.menu.pnum.GENERIC_F469BETX.upload.maximum_data_size=327680
GenF4.menu.pnum.GENERIC_F469BETX.build.board=GENERIC_F469BETX
GenF4.menu.pnum.GENERIC_F469BETX.build.product_line=STM32F469xx
GenF4.menu.pnum.GENERIC_F469BETX.build.variant=STM32F4xx/F469B(E-G-I)T_F469N(E-G-I)H_F479B(G-I)T_F479N(G-I)H
GenF4.menu.pnum.GENERIC_F469BETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F469.svd

# Generic F469BGTx
GenF4.menu.pnum.GENERIC_F469BGTX=Generic F469BGTx
GenF4.menu.pnum.GENERIC_F469BGTX.upload.maximum_size=1048576
GenF4.menu.pnum.GENERIC_F469BGTX.upload.maximum_data_size=327680
GenF4.menu.pnum.GENERIC_F469BGTX.build.board=GENERIC_F469BGTX
GenF4.menu.pnum.GENERIC_F469BGTX.build.product_line=STM32F469xx
GenF4.menu.pnum.GENERIC_F469BGTX.build.variant=STM32F4xx/F469B(E-G-I)T_F469N(E-G-I)H_F479B(G-I)T_F479N(G-I)H
GenF4.menu.pnum.GENERIC_F469BGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F469.svd

# Generic F469BITx
GenF4.menu.pnum.GENERIC_F469BITX=Generic F469BITx
GenF4.menu.pnum.GENERIC_F469BITX.upload.maximum_size=2097152
GenF4.menu.pnum.GENERIC_F469BITX.upload.maximum_data_size=327680
GenF4.menu.pnum.GENERIC_F469BITX.build.board=GENERIC_F469BITX
GenF4.menu.pnum.GENERIC_F469BITX.build.product_line=STM32F469xx
GenF4.menu.pnum.GENERIC_F469BITX.build.variant=STM32F4xx/F469B(E-G-I)T_F469N(E-G-I)H_F479B(G-I)T_F479N(G-I)H
GenF4.menu.pnum.GENERIC_F469BITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F469.svd

# Generic F469NEHx
GenF4.menu.pnum.GENERIC_F469NEHX=Generic F469NEHx
GenF4.menu.pnum.GENERIC_F469NEHX.upload.maximum_size=524288
GenF4.menu.pnum.GENERIC_F469NEHX.upload.maximum_data_size=327680
GenF4.menu.pnum.GENERIC_F469NEHX.build.board=GENERIC_F469NEHX
GenF4.menu.pnum.GENERIC_F469NEHX.build.product_line=STM32F469xx
GenF4.menu.pnum.GENERIC_F469NEHX.build.variant=STM32F4xx/F469B(E-G-I)T_F469N(E-G-I)H_F479B(G-I)T_F479N(G-I)H
GenF4.menu.pnum.GENERIC_F469NEHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F469.svd

# Generic F469NGHx
GenF4.menu.pnum.GENERIC_F469NGHX=Generic F469NGHx
GenF4.menu.pnum.GENERIC_F469NGHX.upload.maximum_size=1048576
GenF4.menu.pnum.GENERIC_F469NGHX.upload.maximum_data_size=327680
GenF4.menu.pnum.GENERIC_F469NGHX.build.board=GENERIC_F469NGHX
GenF4.menu.pnum.GENERIC_F469NGHX.build.product_line=STM32F469xx
GenF4.menu.pnum.GENERIC_F469NGHX.build.variant=STM32F4xx/F469B(E-G-I)T_F469N(E-G-I)H_F479B(G-I)T_F479N(G-I)H
GenF4.menu.pnum.GENERIC_F469NGHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F469.svd

# Generic F469NIHx
GenF4.menu.pnum.GENERIC_F469NIHX=Generic F469NIHx
GenF4.menu.pnum.GENERIC_F469NIHX.upload.maximum_size=2097152
GenF4.menu.pnum.GENERIC_F469NIHX.upload.maximum_data_size=327680
GenF4.menu.pnum.GENERIC_F469NIHX.build.board=GENERIC_F469NIHX
GenF4.menu.pnum.GENERIC_F469NIHX.build.product_line=STM32F469xx
GenF4.menu.pnum.GENERIC_F469NIHX.build.variant=STM32F4xx/F469B(E-G-I)T_F469N(E-G-I)H_F479B(G-I)T_F479N(G-I)H
GenF4.menu.pnum.GENERIC_F469NIHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F469.svd

# Generic F479BGTx
GenF4.menu.pnum.GENERIC_F479BGTX=Generic F479BGTx
GenF4.menu.pnum.GENERIC_F479BGTX.upload.maximum_size=1048576
GenF4.menu.pnum.GENERIC_F479BGTX.upload.maximum_data_size=327680
GenF4.menu.pnum.GENERIC_F479BGTX.build.board=GENERIC_F479BGTX
GenF4.menu.pnum.GENERIC_F479BGTX.build.product_line=STM32F479xx
GenF4.menu.pnum.GENERIC_F479BGTX.build.variant=STM32F4xx/F469B(E-G-I)T_F469N(E-G-I)H_F479B(G-I)T_F479N(G-I)H
GenF4.menu.pnum.GENERIC_F479BGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F479.svd

# Generic F479BITx
GenF4.menu.pnum.GENERIC_F479BITX=Generic F479BITx
GenF4.menu.pnum.GENERIC_F479BITX.upload.maximum_size=2097152
GenF4.menu.pnum.GENERIC_F479BITX.upload.maximum_data_size=327680
GenF4.menu.pnum.GENERIC_F479BITX.build.board=GENERIC_F479BITX
GenF4.menu.pnum.GENERIC_F479BITX.build.product_line=STM32F479xx
GenF4.menu.pnum.GENERIC_F479BITX.build.variant=STM32F4xx/F469B(E-G-I)T_F469N(E-G-I)H_F479B(G-I)T_F479N(G-I)H
GenF4.menu.pnum.GENERIC_F479BITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F479.svd

# Generic F479NGHx
GenF4.menu.pnum.GENERIC_F479NGHX=Generic F479NGHx
GenF4.menu.pnum.GENERIC_F479NGHX.upload.maximum_size=1048576
GenF4.menu.pnum.GENERIC_F479NGHX.upload.maximum_data_size=327680
GenF4.menu.pnum.GENERIC_F479NGHX.build.board=GENERIC_F479NGHX
GenF4.menu.pnum.GENERIC_F479NGHX.build.product_line=STM32F479xx
GenF4.menu.pnum.GENERIC_F479NGHX.build.variant=STM32F4xx/F469B(E-G-I)T_F469N(E-G-I)H_F479B(G-I)T_F479N(G-I)H
GenF4.menu.pnum.GENERIC_F479NGHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F479.svd

# Generic F479NIHx
GenF4.menu.pnum.GENERIC_F479NIHX=Generic F479NIHx
GenF4.menu.pnum.GENERIC_F479NIHX.upload.maximum_size=2097152
GenF4.menu.pnum.GENERIC_F479NIHX.upload.maximum_data_size=327680
GenF4.menu.pnum.GENERIC_F479NIHX.build.board=GENERIC_F479NIHX
GenF4.menu.pnum.GENERIC_F479NIHX.build.product_line=STM32F479xx
GenF4.menu.pnum.GENERIC_F479NIHX.build.variant=STM32F4xx/F469B(E-G-I)T_F469N(E-G-I)H_F479B(G-I)T_F479N(G-I)H
GenF4.menu.pnum.GENERIC_F479NIHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F479.svd

