# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F091RBTx
GenF0.menu.pnum.GENERIC_F091RBTX=Generic F091RBTx
GenF0.menu.pnum.GENERIC_F091RBTX.upload.maximum_size=131072
GenF0.menu.pnum.GENERIC_F091RBTX.upload.maximum_data_size=32768
GenF0.menu.pnum.GENERIC_F091RBTX.build.board=GENERIC_F091RBTX
GenF0.menu.pnum.GENERIC_F091RBTX.build.product_line=STM32F091xC
GenF0.menu.pnum.GENERIC_F091RBTX.build.variant=STM32F0xx/F091RBT_F091RC(H-T-Y)
GenF0.menu.pnum.GENERIC_F091RBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F0xx/STM32F0x1.svd

# Generic F091RCTx
GenF0.menu.pnum.GENERIC_F091RCTX=Generic F091RCTx
GenF0.menu.pnum.GENERIC_F091RCTX.upload.maximum_size=262144
GenF0.menu.pnum.GENERIC_F091RCTX.upload.maximum_data_size=32768
GenF0.menu.pnum.GENERIC_F091RCTX.build.board=GENERIC_F091RCTX
GenF0.menu.pnum.GENERIC_F091RCTX.build.product_line=STM32F091xC
GenF0.menu.pnum.GENERIC_F091RCTX.build.variant=STM32F0xx/F091RBT_F091RC(H-T-Y)
GenF0.menu.pnum.GENERIC_F091RCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F0xx/STM32F0x1.svd

# Generic F091RCHx
GenF0.menu.pnum.GENERIC_F091RCHX=Generic F091RCHx
GenF0.menu.pnum.GENERIC_F091RCHX.upload.maximum_size=262144
GenF0.menu.pnum.GENERIC_F091RCHX.upload.maximum_data_size=32768
GenF0.menu.pnum.GENERIC_F091RCHX.build.board=GENERIC_F091RCHX
GenF0.menu.pnum.GENERIC_F091RCHX.build.product_line=STM32F091xC
GenF0.menu.pnum.GENERIC_F091RCHX.build.variant=STM32F0xx/F091RBT_F091RC(H-T-Y)
GenF0.menu.pnum.GENERIC_F091RCHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F0xx/STM32F0x1.svd

# Generic F091RCYx
GenF0.menu.pnum.GENERIC_F091RCYX=Generic F091RCYx
GenF0.menu.pnum.GENERIC_F091RCYX.upload.maximum_size=262144
GenF0.menu.pnum.GENERIC_F091RCYX.upload.maximum_data_size=32768
GenF0.menu.pnum.GENERIC_F091RCYX.build.board=GENERIC_F091RCYX
GenF0.menu.pnum.GENERIC_F091RCYX.build.product_line=STM32F091xC
GenF0.menu.pnum.GENERIC_F091RCYX.build.variant=STM32F0xx/F091RBT_F091RC(H-T-Y)
GenF0.menu.pnum.GENERIC_F091RCYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F0xx/STM32F0x1.svd

