# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L071CBYx
GenL0.menu.pnum.GENERIC_L071CBYX=Generic L071CBYx
GenL0.menu.pnum.GENERIC_L071CBYX.upload.maximum_size=131072
GenL0.menu.pnum.GENERIC_L071CBYX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L071CBYX.build.board=GENERIC_L071CBYX
GenL0.menu.pnum.GENERIC_L071CBYX.build.product_line=STM32L071xx
GenL0.menu.pnum.GENERIC_L071CBYX.build.variant=STM32L0xx/L071C(B-Z)Y
GenL0.menu.pnum.GENERIC_L071CBYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

# Generic L071CZYx
GenL0.menu.pnum.GENERIC_L071CZYX=Generic L071CZYx
GenL0.menu.pnum.GENERIC_L071CZYX.upload.maximum_size=196608
GenL0.menu.pnum.GENERIC_L071CZYX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L071CZYX.build.board=GENERIC_L071CZYX
GenL0.menu.pnum.GENERIC_L071CZYX.build.product_line=STM32L071xx
GenL0.menu.pnum.GENERIC_L071CZYX.build.variant=STM32L0xx/L071C(B-Z)Y
GenL0.menu.pnum.GENERIC_L071CZYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

