# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F769IGTx
GenF7.menu.pnum.GENERIC_F769IGTX=Generic F769IGTx
GenF7.menu.pnum.GENERIC_F769IGTX.upload.maximum_size=1048576
GenF7.menu.pnum.GENERIC_F769IGTX.upload.maximum_data_size=393216
GenF7.menu.pnum.GENERIC_F769IGTX.build.board=GENERIC_F769IGTX
GenF7.menu.pnum.GENERIC_F769IGTX.build.product_line=STM32F769xx
GenF7.menu.pnum.GENERIC_F769IGTX.build.variant=STM32F7xx/F769I(G-I)T_F779IIT
GenF7.menu.pnum.GENERIC_F769IGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F769.svd

# Generic F769IITx
GenF7.menu.pnum.GENERIC_F769IITX=Generic F769IITx
GenF7.menu.pnum.GENERIC_F769IITX.upload.maximum_size=2097152
GenF7.menu.pnum.GENERIC_F769IITX.upload.maximum_data_size=393216
GenF7.menu.pnum.GENERIC_F769IITX.build.board=GENERIC_F769IITX
GenF7.menu.pnum.GENERIC_F769IITX.build.product_line=STM32F769xx
GenF7.menu.pnum.GENERIC_F769IITX.build.variant=STM32F7xx/F769I(G-I)T_F779IIT
GenF7.menu.pnum.GENERIC_F769IITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F769.svd

# Generic F779IITx
GenF7.menu.pnum.GENERIC_F779IITX=Generic F779IITx
GenF7.menu.pnum.GENERIC_F779IITX.upload.maximum_size=2097152
GenF7.menu.pnum.GENERIC_F779IITX.upload.maximum_data_size=393216
GenF7.menu.pnum.GENERIC_F779IITX.build.board=GENERIC_F779IITX
GenF7.menu.pnum.GENERIC_F779IITX.build.product_line=STM32F779xx
GenF7.menu.pnum.GENERIC_F779IITX.build.variant=STM32F7xx/F769I(G-I)T_F779IIT
GenF7.menu.pnum.GENERIC_F779IITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F779.svd

