# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L011G3Ux
GenL0.menu.pnum.GENERIC_L011G3UX=Generic L011G3Ux
GenL0.menu.pnum.GENERIC_L011G3UX.upload.maximum_size=8192
GenL0.menu.pnum.GENERIC_L011G3UX.upload.maximum_data_size=2048
GenL0.menu.pnum.GENERIC_L011G3UX.build.board=GENERIC_L011G3UX
GenL0.menu.pnum.GENERIC_L011G3UX.build.product_line=STM32L011xx
GenL0.menu.pnum.GENERIC_L011G3UX.build.variant=STM32L0xx/L011G(3-4)U_L021G4U
GenL0.menu.pnum.GENERIC_L011G3UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

# Generic L011G4Ux
GenL0.menu.pnum.GENERIC_L011G4UX=Generic L011G4Ux
GenL0.menu.pnum.GENERIC_L011G4UX.upload.maximum_size=16384
GenL0.menu.pnum.GENERIC_L011G4UX.upload.maximum_data_size=2048
GenL0.menu.pnum.GENERIC_L011G4UX.build.board=GENERIC_L011G4UX
GenL0.menu.pnum.GENERIC_L011G4UX.build.product_line=STM32L011xx
GenL0.menu.pnum.GENERIC_L011G4UX.build.variant=STM32L0xx/L011G(3-4)U_L021G4U
GenL0.menu.pnum.GENERIC_L011G4UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

# Generic L021G4Ux
GenL0.menu.pnum.GENERIC_L021G4UX=Generic L021G4Ux
GenL0.menu.pnum.GENERIC_L021G4UX.upload.maximum_size=16384
GenL0.menu.pnum.GENERIC_L021G4UX.upload.maximum_data_size=2048
GenL0.menu.pnum.GENERIC_L021G4UX.build.board=GENERIC_L021G4UX
GenL0.menu.pnum.GENERIC_L021G4UX.build.product_line=STM32L021xx
GenL0.menu.pnum.GENERIC_L021G4UX.build.variant=STM32L0xx/L011G(3-4)U_L021G4U
GenL0.menu.pnum.GENERIC_L021G4UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

