# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic H562ZGTx
GenH5.menu.pnum.GENERIC_H562ZGTX=Generic H562ZGTx
GenH5.menu.pnum.GENERIC_H562ZGTX.upload.maximum_size=1048576
GenH5.menu.pnum.GENERIC_H562ZGTX.upload.maximum_data_size=655360
GenH5.menu.pnum.GENERIC_H562ZGTX.build.board=GENERIC_H562ZGTX
GenH5.menu.pnum.GENERIC_H562ZGTX.build.product_line=STM32H562xx
GenH5.menu.pnum.GENERIC_H562ZGTX.build.variant=STM32H5xx/H562Z(G-I)T
GenH5.menu.pnum.GENERIC_H562ZGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32H5xx/STM32H562.svd

# Generic H562ZITx
GenH5.menu.pnum.GENERIC_H562ZITX=Generic H562ZITx
GenH5.menu.pnum.GENERIC_H562ZITX.upload.maximum_size=2097152
GenH5.menu.pnum.GENERIC_H562ZITX.upload.maximum_data_size=655360
GenH5.menu.pnum.GENERIC_H562ZITX.build.board=GENERIC_H562ZITX
GenH5.menu.pnum.GENERIC_H562ZITX.build.product_line=STM32H562xx
GenH5.menu.pnum.GENERIC_H562ZITX.build.variant=STM32H5xx/H562Z(G-I)T
GenH5.menu.pnum.GENERIC_H562ZITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32H5xx/STM32H562.svd

