# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F413MGYx
GenF4.menu.pnum.GENERIC_F413MGYX=Generic F413MGYx
GenF4.menu.pnum.GENERIC_F413MGYX.upload.maximum_size=1048576
GenF4.menu.pnum.GENERIC_F413MGYX.upload.maximum_data_size=327680
GenF4.menu.pnum.GENERIC_F413MGYX.build.board=GENERIC_F413MGYX
GenF4.menu.pnum.GENERIC_F413MGYX.build.product_line=STM32F413xx
GenF4.menu.pnum.GENERIC_F413MGYX.build.variant=STM32F4xx/F413M(G-H)Y_F423MHY
GenF4.menu.pnum.GENERIC_F413MGYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F413.svd

# Generic F413MHYx
GenF4.menu.pnum.GENERIC_F413MHYX=Generic F413MHYx
GenF4.menu.pnum.GENERIC_F413MHYX.upload.maximum_size=1572864
GenF4.menu.pnum.GENERIC_F413MHYX.upload.maximum_data_size=327680
GenF4.menu.pnum.GENERIC_F413MHYX.build.board=GENERIC_F413MHYX
GenF4.menu.pnum.GENERIC_F413MHYX.build.product_line=STM32F413xx
GenF4.menu.pnum.GENERIC_F413MHYX.build.variant=STM32F4xx/F413M(G-H)Y_F423MHY
GenF4.menu.pnum.GENERIC_F413MHYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F413.svd

# Generic F423MHYx
GenF4.menu.pnum.GENERIC_F423MHYX=Generic F423MHYx
GenF4.menu.pnum.GENERIC_F423MHYX.upload.maximum_size=1572864
GenF4.menu.pnum.GENERIC_F423MHYX.upload.maximum_data_size=327680
GenF4.menu.pnum.GENERIC_F423MHYX.build.board=GENERIC_F423MHYX
GenF4.menu.pnum.GENERIC_F423MHYX.build.product_line=STM32F423xx
GenF4.menu.pnum.GENERIC_F423MHYX.build.variant=STM32F4xx/F413M(G-H)Y_F423MHY
GenF4.menu.pnum.GENERIC_F423MHYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F423.svd

