# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic H563ZGTx
GenH5.menu.pnum.GENERIC_H563ZGTX=Generic H563ZGTx
GenH5.menu.pnum.GENERIC_H563ZGTX.upload.maximum_size=1048576
GenH5.menu.pnum.GENERIC_H563ZGTX.upload.maximum_data_size=655360
GenH5.menu.pnum.GENERIC_H563ZGTX.build.board=GENERIC_H563ZGTX
GenH5.menu.pnum.GENERIC_H563ZGTX.build.product_line=STM32H563xx
GenH5.menu.pnum.GENERIC_H563ZGTX.build.variant=STM32H5xx/H563Z(G-I)T_H573ZIT
GenH5.menu.pnum.GENERIC_H563ZGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32H5xx/STM32H563.svd

# Generic H563ZITx
GenH5.menu.pnum.GENERIC_H563ZITX=Generic H563ZITx
GenH5.menu.pnum.GENERIC_H563ZITX.upload.maximum_size=2097152
GenH5.menu.pnum.GENERIC_H563ZITX.upload.maximum_data_size=655360
GenH5.menu.pnum.GENERIC_H563ZITX.build.board=GENERIC_H563ZITX
GenH5.menu.pnum.GENERIC_H563ZITX.build.product_line=STM32H563xx
GenH5.menu.pnum.GENERIC_H563ZITX.build.variant=STM32H5xx/H563Z(G-I)T_H573ZIT
GenH5.menu.pnum.GENERIC_H563ZITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32H5xx/STM32H563.svd

# Generic H573ZITx
GenH5.menu.pnum.GENERIC_H573ZITX=Generic H573ZITx
GenH5.menu.pnum.GENERIC_H573ZITX.upload.maximum_size=2097152
GenH5.menu.pnum.GENERIC_H573ZITX.upload.maximum_data_size=655360
GenH5.menu.pnum.GENERIC_H573ZITX.build.board=GENERIC_H573ZITX
GenH5.menu.pnum.GENERIC_H573ZITX.build.product_line=STM32H573xx
GenH5.menu.pnum.GENERIC_H573ZITX.build.variant=STM32H5xx/H563Z(G-I)T_H573ZIT
GenH5.menu.pnum.GENERIC_H573ZITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32H5xx/STM32H573.svd

