# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F100R8Tx
GenF1.menu.pnum.GENERIC_F100R8TX=Generic F100R8Tx
GenF1.menu.pnum.GENERIC_F100R8TX.upload.maximum_size=65536
GenF1.menu.pnum.GENERIC_F100R8TX.upload.maximum_data_size=8192
GenF1.menu.pnum.GENERIC_F100R8TX.build.board=GENERIC_F100R8TX
GenF1.menu.pnum.GENERIC_F100R8TX.build.product_line=STM32F100xB
GenF1.menu.pnum.GENERIC_F100R8TX.build.variant=STM32F1xx/F100R(8-B)T
GenF1.menu.pnum.GENERIC_F100R8TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F1xx/STM32F100.svd

# Generic F100RBTx
GenF1.menu.pnum.GENERIC_F100RBTX=Generic F100RBTx
GenF1.menu.pnum.GENERIC_F100RBTX.upload.maximum_size=131072
GenF1.menu.pnum.GENERIC_F100RBTX.upload.maximum_data_size=8192
GenF1.menu.pnum.GENERIC_F100RBTX.build.board=GENERIC_F100RBTX
GenF1.menu.pnum.GENERIC_F100RBTX.build.product_line=STM32F100xB
GenF1.menu.pnum.GENERIC_F100RBTX.build.variant=STM32F1xx/F100R(8-B)T
GenF1.menu.pnum.GENERIC_F100RBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F1xx/STM32F100.svd

