# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L412R8Ix
GenL4.menu.pnum.GENERIC_L412R8IX=Generic L412R8Ix
GenL4.menu.pnum.GENERIC_L412R8IX.upload.maximum_size=65536
GenL4.menu.pnum.GENERIC_L412R8IX.upload.maximum_data_size=40960
GenL4.menu.pnum.GENERIC_L412R8IX.build.board=GENERIC_L412R8IX
GenL4.menu.pnum.GENERIC_L412R8IX.build.product_line=STM32L412xx
GenL4.menu.pnum.GENERIC_L412R8IX.build.variant=STM32L4xx/L412R(8-B)(I-T)_L422RB(I-T)
GenL4.menu.pnum.GENERIC_L412R8IX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L412.svd

# Generic L412R8Tx
GenL4.menu.pnum.GENERIC_L412R8TX=Generic L412R8Tx
GenL4.menu.pnum.GENERIC_L412R8TX.upload.maximum_size=65536
GenL4.menu.pnum.GENERIC_L412R8TX.upload.maximum_data_size=40960
GenL4.menu.pnum.GENERIC_L412R8TX.build.board=GENERIC_L412R8TX
GenL4.menu.pnum.GENERIC_L412R8TX.build.product_line=STM32L412xx
GenL4.menu.pnum.GENERIC_L412R8TX.build.variant=STM32L4xx/L412R(8-B)(I-T)_L422RB(I-T)
GenL4.menu.pnum.GENERIC_L412R8TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L412.svd

# Generic L412RBIx
GenL4.menu.pnum.GENERIC_L412RBIX=Generic L412RBIx
GenL4.menu.pnum.GENERIC_L412RBIX.upload.maximum_size=131072
GenL4.menu.pnum.GENERIC_L412RBIX.upload.maximum_data_size=40960
GenL4.menu.pnum.GENERIC_L412RBIX.build.board=GENERIC_L412RBIX
GenL4.menu.pnum.GENERIC_L412RBIX.build.product_line=STM32L412xx
GenL4.menu.pnum.GENERIC_L412RBIX.build.variant=STM32L4xx/L412R(8-B)(I-T)_L422RB(I-T)
GenL4.menu.pnum.GENERIC_L412RBIX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L412.svd

# Generic L412RBTx
GenL4.menu.pnum.GENERIC_L412RBTX=Generic L412RBTx
GenL4.menu.pnum.GENERIC_L412RBTX.upload.maximum_size=131072
GenL4.menu.pnum.GENERIC_L412RBTX.upload.maximum_data_size=40960
GenL4.menu.pnum.GENERIC_L412RBTX.build.board=GENERIC_L412RBTX
GenL4.menu.pnum.GENERIC_L412RBTX.build.product_line=STM32L412xx
GenL4.menu.pnum.GENERIC_L412RBTX.build.variant=STM32L4xx/L412R(8-B)(I-T)_L422RB(I-T)
GenL4.menu.pnum.GENERIC_L412RBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L412.svd

# Generic L422RBIx
GenL4.menu.pnum.GENERIC_L422RBIX=Generic L422RBIx
GenL4.menu.pnum.GENERIC_L422RBIX.upload.maximum_size=131072
GenL4.menu.pnum.GENERIC_L422RBIX.upload.maximum_data_size=40960
GenL4.menu.pnum.GENERIC_L422RBIX.build.board=GENERIC_L422RBIX
GenL4.menu.pnum.GENERIC_L422RBIX.build.product_line=STM32L422xx
GenL4.menu.pnum.GENERIC_L422RBIX.build.variant=STM32L4xx/L412R(8-B)(I-T)_L422RB(I-T)
GenL4.menu.pnum.GENERIC_L422RBIX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L422.svd

# Generic L422RBTx
GenL4.menu.pnum.GENERIC_L422RBTX=Generic L422RBTx
GenL4.menu.pnum.GENERIC_L422RBTX.upload.maximum_size=131072
GenL4.menu.pnum.GENERIC_L422RBTX.upload.maximum_data_size=40960
GenL4.menu.pnum.GENERIC_L422RBTX.build.board=GENERIC_L422RBTX
GenL4.menu.pnum.GENERIC_L422RBTX.build.product_line=STM32L422xx
GenL4.menu.pnum.GENERIC_L422RBTX.build.variant=STM32L4xx/L412R(8-B)(I-T)_L422RB(I-T)
GenL4.menu.pnum.GENERIC_L422RBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L422.svd

