# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L476ZETx
GenL4.menu.pnum.GENERIC_L476ZETX=Generic L476ZETx
GenL4.menu.pnum.GENERIC_L476ZETX.upload.maximum_size=524288
GenL4.menu.pnum.GENERIC_L476ZETX.upload.maximum_data_size=131072
GenL4.menu.pnum.GENERIC_L476ZETX.build.board=GENERIC_L476ZETX
GenL4.menu.pnum.GENERIC_L476ZETX.build.product_line=STM32L476xx
GenL4.menu.pnum.GENERIC_L476ZETX.build.variant=STM32L4xx/L476ZET_L476ZG(J-T)_L486ZGT
GenL4.menu.pnum.GENERIC_L476ZETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L476.svd

# Generic L476ZGTx
GenL4.menu.pnum.GENERIC_L476ZGTX=Generic L476ZGTx
GenL4.menu.pnum.GENERIC_L476ZGTX.upload.maximum_size=1048576
GenL4.menu.pnum.GENERIC_L476ZGTX.upload.maximum_data_size=131072
GenL4.menu.pnum.GENERIC_L476ZGTX.build.board=GENERIC_L476ZGTX
GenL4.menu.pnum.GENERIC_L476ZGTX.build.product_line=STM32L476xx
GenL4.menu.pnum.GENERIC_L476ZGTX.build.variant=STM32L4xx/L476ZET_L476ZG(J-T)_L486ZGT
GenL4.menu.pnum.GENERIC_L476ZGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L476.svd

# Generic L476ZGJx
GenL4.menu.pnum.GENERIC_L476ZGJX=Generic L476ZGJx
GenL4.menu.pnum.GENERIC_L476ZGJX.upload.maximum_size=1048576
GenL4.menu.pnum.GENERIC_L476ZGJX.upload.maximum_data_size=131072
GenL4.menu.pnum.GENERIC_L476ZGJX.build.board=GENERIC_L476ZGJX
GenL4.menu.pnum.GENERIC_L476ZGJX.build.product_line=STM32L476xx
GenL4.menu.pnum.GENERIC_L476ZGJX.build.variant=STM32L4xx/L476ZET_L476ZG(J-T)_L486ZGT
GenL4.menu.pnum.GENERIC_L476ZGJX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L476.svd

# Generic L486ZGTx
GenL4.menu.pnum.GENERIC_L486ZGTX=Generic L486ZGTx
GenL4.menu.pnum.GENERIC_L486ZGTX.upload.maximum_size=1048576
GenL4.menu.pnum.GENERIC_L486ZGTX.upload.maximum_data_size=131072
GenL4.menu.pnum.GENERIC_L486ZGTX.build.board=GENERIC_L486ZGTX
GenL4.menu.pnum.GENERIC_L486ZGTX.build.product_line=STM32L486xx
GenL4.menu.pnum.GENERIC_L486ZGTX.build.variant=STM32L4xx/L476ZET_L476ZG(J-T)_L486ZGT
GenL4.menu.pnum.GENERIC_L486ZGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L486.svd

