# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L051R6Hx
GenL0.menu.pnum.GENERIC_L051R6HX=Generic L051R6Hx
GenL0.menu.pnum.GENERIC_L051R6HX.upload.maximum_size=32768
GenL0.menu.pnum.GENERIC_L051R6HX.upload.maximum_data_size=8192
GenL0.menu.pnum.GENERIC_L051R6HX.build.board=GENERIC_L051R6HX
GenL0.menu.pnum.GENERIC_L051R6HX.build.product_line=STM32L051xx
GenL0.menu.pnum.GENERIC_L051R6HX.build.variant=STM32L0xx/L051R(6-8)H
GenL0.menu.pnum.GENERIC_L051R6HX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

# Generic L051R8Hx
GenL0.menu.pnum.GENERIC_L051R8HX=Generic L051R8Hx
GenL0.menu.pnum.GENERIC_L051R8HX.upload.maximum_size=65536
GenL0.menu.pnum.GENERIC_L051R8HX.upload.maximum_data_size=8192
GenL0.menu.pnum.GENERIC_L051R8HX.build.board=GENERIC_L051R8HX
GenL0.menu.pnum.GENERIC_L051R8HX.build.product_line=STM32L051xx
GenL0.menu.pnum.GENERIC_L051R8HX.build.variant=STM32L0xx/L051R(6-8)H
GenL0.menu.pnum.GENERIC_L051R8HX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

