# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic G431K6Tx
GenG4.menu.pnum.GENERIC_G431K6TX=Generic G431K6Tx
GenG4.menu.pnum.GENERIC_G431K6TX.upload.maximum_size=32768
GenG4.menu.pnum.GENERIC_G431K6TX.upload.maximum_data_size=32768
GenG4.menu.pnum.GENERIC_G431K6TX.build.board=GENERIC_G431K6TX
GenG4.menu.pnum.GENERIC_G431K6TX.build.product_line=STM32G431xx
GenG4.menu.pnum.GENERIC_G431K6TX.build.variant=STM32G4xx/G431K(6-8-B)(T-U)_G441KB(T-U)
GenG4.menu.pnum.GENERIC_G431K6TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G431.svd

# Generic G431K8Tx
GenG4.menu.pnum.GENERIC_G431K8TX=Generic G431K8Tx
GenG4.menu.pnum.GENERIC_G431K8TX.upload.maximum_size=65536
GenG4.menu.pnum.GENERIC_G431K8TX.upload.maximum_data_size=32768
GenG4.menu.pnum.GENERIC_G431K8TX.build.board=GENERIC_G431K8TX
GenG4.menu.pnum.GENERIC_G431K8TX.build.product_line=STM32G431xx
GenG4.menu.pnum.GENERIC_G431K8TX.build.variant=STM32G4xx/G431K(6-8-B)(T-U)_G441KB(T-U)
GenG4.menu.pnum.GENERIC_G431K8TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G431.svd

# Generic G431KBTx
GenG4.menu.pnum.GENERIC_G431KBTX=Generic G431KBTx
GenG4.menu.pnum.GENERIC_G431KBTX.upload.maximum_size=131072
GenG4.menu.pnum.GENERIC_G431KBTX.upload.maximum_data_size=32768
GenG4.menu.pnum.GENERIC_G431KBTX.build.board=GENERIC_G431KBTX
GenG4.menu.pnum.GENERIC_G431KBTX.build.product_line=STM32G431xx
GenG4.menu.pnum.GENERIC_G431KBTX.build.variant=STM32G4xx/G431K(6-8-B)(T-U)_G441KB(T-U)
GenG4.menu.pnum.GENERIC_G431KBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G431.svd

# Generic G431K6Ux
GenG4.menu.pnum.GENERIC_G431K6UX=Generic G431K6Ux
GenG4.menu.pnum.GENERIC_G431K6UX.upload.maximum_size=32768
GenG4.menu.pnum.GENERIC_G431K6UX.upload.maximum_data_size=32768
GenG4.menu.pnum.GENERIC_G431K6UX.build.board=GENERIC_G431K6UX
GenG4.menu.pnum.GENERIC_G431K6UX.build.product_line=STM32G431xx
GenG4.menu.pnum.GENERIC_G431K6UX.build.variant=STM32G4xx/G431K(6-8-B)(T-U)_G441KB(T-U)
GenG4.menu.pnum.GENERIC_G431K6UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G431.svd

# Generic G431K8Ux
GenG4.menu.pnum.GENERIC_G431K8UX=Generic G431K8Ux
GenG4.menu.pnum.GENERIC_G431K8UX.upload.maximum_size=65536
GenG4.menu.pnum.GENERIC_G431K8UX.upload.maximum_data_size=32768
GenG4.menu.pnum.GENERIC_G431K8UX.build.board=GENERIC_G431K8UX
GenG4.menu.pnum.GENERIC_G431K8UX.build.product_line=STM32G431xx
GenG4.menu.pnum.GENERIC_G431K8UX.build.variant=STM32G4xx/G431K(6-8-B)(T-U)_G441KB(T-U)
GenG4.menu.pnum.GENERIC_G431K8UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G431.svd

# Generic G431KBUx
GenG4.menu.pnum.GENERIC_G431KBUX=Generic G431KBUx
GenG4.menu.pnum.GENERIC_G431KBUX.upload.maximum_size=131072
GenG4.menu.pnum.GENERIC_G431KBUX.upload.maximum_data_size=32768
GenG4.menu.pnum.GENERIC_G431KBUX.build.board=GENERIC_G431KBUX
GenG4.menu.pnum.GENERIC_G431KBUX.build.product_line=STM32G431xx
GenG4.menu.pnum.GENERIC_G431KBUX.build.variant=STM32G4xx/G431K(6-8-B)(T-U)_G441KB(T-U)
GenG4.menu.pnum.GENERIC_G431KBUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G431.svd

# Generic G441KBTx
GenG4.menu.pnum.GENERIC_G441KBTX=Generic G441KBTx
GenG4.menu.pnum.GENERIC_G441KBTX.upload.maximum_size=131072
GenG4.menu.pnum.GENERIC_G441KBTX.upload.maximum_data_size=32768
GenG4.menu.pnum.GENERIC_G441KBTX.build.board=GENERIC_G441KBTX
GenG4.menu.pnum.GENERIC_G441KBTX.build.product_line=STM32G441xx
GenG4.menu.pnum.GENERIC_G441KBTX.build.variant=STM32G4xx/G431K(6-8-B)(T-U)_G441KB(T-U)
GenG4.menu.pnum.GENERIC_G441KBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G441.svd

# Generic G441KBUx
GenG4.menu.pnum.GENERIC_G441KBUX=Generic G441KBUx
GenG4.menu.pnum.GENERIC_G441KBUX.upload.maximum_size=131072
GenG4.menu.pnum.GENERIC_G441KBUX.upload.maximum_data_size=32768
GenG4.menu.pnum.GENERIC_G441KBUX.build.board=GENERIC_G441KBUX
GenG4.menu.pnum.GENERIC_G441KBUX.build.product_line=STM32G441xx
GenG4.menu.pnum.GENERIC_G441KBUX.build.variant=STM32G4xx/G431K(6-8-B)(T-U)_G441KB(T-U)
GenG4.menu.pnum.GENERIC_G441KBUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G441.svd

