# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic C011D6Yx
GenC0.menu.pnum.GENERIC_C011D6YX=Generic C011D6Yx
GenC0.menu.pnum.GENERIC_C011D6YX.upload.maximum_size=32768
GenC0.menu.pnum.GENERIC_C011D6YX.upload.maximum_data_size=6144
GenC0.menu.pnum.GENERIC_C011D6YX.build.board=GENERIC_C011D6YX
GenC0.menu.pnum.GENERIC_C011D6YX.build.product_line=STM32C011xx
GenC0.menu.pnum.GENERIC_C011D6YX.build.variant=STM32C0xx/C011D6Y_C011F(4-6)(P-U)
GenC0.menu.pnum.GENERIC_C011D6YX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32C0xx/STM32C011.svd

# Generic C011F4Px
GenC0.menu.pnum.GENERIC_C011F4PX=Generic C011F4Px
GenC0.menu.pnum.GENERIC_C011F4PX.upload.maximum_size=16384
GenC0.menu.pnum.GENERIC_C011F4PX.upload.maximum_data_size=6144
GenC0.menu.pnum.GENERIC_C011F4PX.build.board=GENERIC_C011F4PX
GenC0.menu.pnum.GENERIC_C011F4PX.build.product_line=STM32C011xx
GenC0.menu.pnum.GENERIC_C011F4PX.build.variant=STM32C0xx/C011D6Y_C011F(4-6)(P-U)
GenC0.menu.pnum.GENERIC_C011F4PX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32C0xx/STM32C011.svd

# Generic C011F6Px
GenC0.menu.pnum.GENERIC_C011F6PX=Generic C011F6Px
GenC0.menu.pnum.GENERIC_C011F6PX.upload.maximum_size=32768
GenC0.menu.pnum.GENERIC_C011F6PX.upload.maximum_data_size=6144
GenC0.menu.pnum.GENERIC_C011F6PX.build.board=GENERIC_C011F6PX
GenC0.menu.pnum.GENERIC_C011F6PX.build.product_line=STM32C011xx
GenC0.menu.pnum.GENERIC_C011F6PX.build.variant=STM32C0xx/C011D6Y_C011F(4-6)(P-U)
GenC0.menu.pnum.GENERIC_C011F6PX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32C0xx/STM32C011.svd

# Generic C011F4Ux
GenC0.menu.pnum.GENERIC_C011F4UX=Generic C011F4Ux
GenC0.menu.pnum.GENERIC_C011F4UX.upload.maximum_size=16384
GenC0.menu.pnum.GENERIC_C011F4UX.upload.maximum_data_size=6144
GenC0.menu.pnum.GENERIC_C011F4UX.build.board=GENERIC_C011F4UX
GenC0.menu.pnum.GENERIC_C011F4UX.build.product_line=STM32C011xx
GenC0.menu.pnum.GENERIC_C011F4UX.build.variant=STM32C0xx/C011D6Y_C011F(4-6)(P-U)
GenC0.menu.pnum.GENERIC_C011F4UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32C0xx/STM32C011.svd

# Generic C011F6Ux
GenC0.menu.pnum.GENERIC_C011F6UX=Generic C011F6Ux
GenC0.menu.pnum.GENERIC_C011F6UX.upload.maximum_size=32768
GenC0.menu.pnum.GENERIC_C011F6UX.upload.maximum_data_size=6144
GenC0.menu.pnum.GENERIC_C011F6UX.build.board=GENERIC_C011F6UX
GenC0.menu.pnum.GENERIC_C011F6UX.build.product_line=STM32C011xx
GenC0.menu.pnum.GENERIC_C011F6UX.build.variant=STM32C0xx/C011D6Y_C011F(4-6)(P-U)
GenC0.menu.pnum.GENERIC_C011F6UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32C0xx/STM32C011.svd

