# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L471ZEJx
GenL4.menu.pnum.GENERIC_L471ZEJX=Generic L471ZEJx
GenL4.menu.pnum.GENERIC_L471ZEJX.upload.maximum_size=524288
GenL4.menu.pnum.GENERIC_L471ZEJX.upload.maximum_data_size=131072
GenL4.menu.pnum.GENERIC_L471ZEJX.build.board=GENERIC_L471ZEJX
GenL4.menu.pnum.GENERIC_L471ZEJX.build.product_line=STM32L471xx
GenL4.menu.pnum.GENERIC_L471ZEJX.build.variant=STM32L4xx/L471Z(E-G)(J-T)
GenL4.menu.pnum.GENERIC_L471ZEJX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L471.svd

# Generic L471ZGJx
GenL4.menu.pnum.GENERIC_L471ZGJX=Generic L471ZGJx
GenL4.menu.pnum.GENERIC_L471ZGJX.upload.maximum_size=1048576
GenL4.menu.pnum.GENERIC_L471ZGJX.upload.maximum_data_size=131072
GenL4.menu.pnum.GENERIC_L471ZGJX.build.board=GENERIC_L471ZGJX
GenL4.menu.pnum.GENERIC_L471ZGJX.build.product_line=STM32L471xx
GenL4.menu.pnum.GENERIC_L471ZGJX.build.variant=STM32L4xx/L471Z(E-G)(J-T)
GenL4.menu.pnum.GENERIC_L471ZGJX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L471.svd

# Generic L471ZETx
GenL4.menu.pnum.GENERIC_L471ZETX=Generic L471ZETx
GenL4.menu.pnum.GENERIC_L471ZETX.upload.maximum_size=524288
GenL4.menu.pnum.GENERIC_L471ZETX.upload.maximum_data_size=131072
GenL4.menu.pnum.GENERIC_L471ZETX.build.board=GENERIC_L471ZETX
GenL4.menu.pnum.GENERIC_L471ZETX.build.product_line=STM32L471xx
GenL4.menu.pnum.GENERIC_L471ZETX.build.variant=STM32L4xx/L471Z(E-G)(J-T)
GenL4.menu.pnum.GENERIC_L471ZETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L471.svd

# Generic L471ZGTx
GenL4.menu.pnum.GENERIC_L471ZGTX=Generic L471ZGTx
GenL4.menu.pnum.GENERIC_L471ZGTX.upload.maximum_size=1048576
GenL4.menu.pnum.GENERIC_L471ZGTX.upload.maximum_data_size=131072
GenL4.menu.pnum.GENERIC_L471ZGTX.build.board=GENERIC_L471ZGTX
GenL4.menu.pnum.GENERIC_L471ZGTX.build.product_line=STM32L471xx
GenL4.menu.pnum.GENERIC_L471ZGTX.build.variant=STM32L4xx/L471Z(E-G)(J-T)
GenL4.menu.pnum.GENERIC_L471ZGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L471.svd

