# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic WBA62CGUx
GenWBA.menu.pnum.GENERIC_WBA62CGUX=Generic WBA62CGUx
GenWBA.menu.pnum.GENERIC_WBA62CGUX.upload.maximum_size=1048576
GenWBA.menu.pnum.GENERIC_WBA62CGUX.upload.maximum_data_size=262144
GenWBA.menu.pnum.GENERIC_WBA62CGUX.build.board=GENERIC_WBA62CGUX
GenWBA.menu.pnum.GENERIC_WBA62CGUX.build.product_line=STM32WBA62xx
GenWBA.menu.pnum.GENERIC_WBA62CGUX.build.variant=STM32WBAxx/WBA62C(G-I)U_WBA64C(G-I)U
GenWBA.menu.pnum.GENERIC_WBA62CGUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32WBAxx/STM32WBA62.svd

# Generic WBA62CIUx
GenWBA.menu.pnum.GENERIC_WBA62CIUX=Generic WBA62CIUx
GenWBA.menu.pnum.GENERIC_WBA62CIUX.upload.maximum_size=2097152
GenWBA.menu.pnum.GENERIC_WBA62CIUX.upload.maximum_data_size=524288
GenWBA.menu.pnum.GENERIC_WBA62CIUX.build.board=GENERIC_WBA62CIUX
GenWBA.menu.pnum.GENERIC_WBA62CIUX.build.product_line=STM32WBA62xx
GenWBA.menu.pnum.GENERIC_WBA62CIUX.build.variant=STM32WBAxx/WBA62C(G-I)U_WBA64C(G-I)U
GenWBA.menu.pnum.GENERIC_WBA62CIUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32WBAxx/STM32WBA62.svd

# Generic WBA64CGUx
GenWBA.menu.pnum.GENERIC_WBA64CGUX=Generic WBA64CGUx
GenWBA.menu.pnum.GENERIC_WBA64CGUX.upload.maximum_size=1048576
GenWBA.menu.pnum.GENERIC_WBA64CGUX.upload.maximum_data_size=262144
GenWBA.menu.pnum.GENERIC_WBA64CGUX.build.board=GENERIC_WBA64CGUX
GenWBA.menu.pnum.GENERIC_WBA64CGUX.build.product_line=STM32WBA64xx
GenWBA.menu.pnum.GENERIC_WBA64CGUX.build.variant=STM32WBAxx/WBA62C(G-I)U_WBA64C(G-I)U
GenWBA.menu.pnum.GENERIC_WBA64CGUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32WBAxx/STM32WBA64.svd

# Generic WBA64CIUx
GenWBA.menu.pnum.GENERIC_WBA64CIUX=Generic WBA64CIUx
GenWBA.menu.pnum.GENERIC_WBA64CIUX.upload.maximum_size=2097152
GenWBA.menu.pnum.GENERIC_WBA64CIUX.upload.maximum_data_size=524288
GenWBA.menu.pnum.GENERIC_WBA64CIUX.build.board=GENERIC_WBA64CIUX
GenWBA.menu.pnum.GENERIC_WBA64CIUX.build.product_line=STM32WBA64xx
GenWBA.menu.pnum.GENERIC_WBA64CIUX.build.variant=STM32WBAxx/WBA62C(G-I)U_WBA64C(G-I)U
GenWBA.menu.pnum.GENERIC_WBA64CIUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32WBAxx/STM32WBA64.svd

