# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F301K6Ux
GenF3.menu.pnum.GENERIC_F301K6UX=Generic F301K6Ux
GenF3.menu.pnum.GENERIC_F301K6UX.upload.maximum_size=32768
GenF3.menu.pnum.GENERIC_F301K6UX.upload.maximum_data_size=16384
GenF3.menu.pnum.GENERIC_F301K6UX.build.board=GENERIC_F301K6UX
GenF3.menu.pnum.GENERIC_F301K6UX.build.product_line=STM32F301x8
GenF3.menu.pnum.GENERIC_F301K6UX.build.variant=STM32F3xx/F301K(6-8)U
GenF3.menu.pnum.GENERIC_F301K6UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F301.svd

# Generic F301K8Ux
GenF3.menu.pnum.GENERIC_F301K8UX=Generic F301K8Ux
GenF3.menu.pnum.GENERIC_F301K8UX.upload.maximum_size=65536
GenF3.menu.pnum.GENERIC_F301K8UX.upload.maximum_data_size=16384
GenF3.menu.pnum.GENERIC_F301K8UX.build.board=GENERIC_F301K8UX
GenF3.menu.pnum.GENERIC_F301K8UX.build.product_line=STM32F301x8
GenF3.menu.pnum.GENERIC_F301K8UX.build.variant=STM32F3xx/F301K(6-8)U
GenF3.menu.pnum.GENERIC_F301K8UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F301.svd

