# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L151ZCTx
GenL1.menu.pnum.GENERIC_L151ZCTX=Generic L151ZCTx
GenL1.menu.pnum.GENERIC_L151ZCTX.upload.maximum_size=262144
GenL1.menu.pnum.GENERIC_L151ZCTX.upload.maximum_data_size=32768
GenL1.menu.pnum.GENERIC_L151ZCTX.build.board=GENERIC_L151ZCTX
GenL1.menu.pnum.GENERIC_L151ZCTX.build.product_line=STM32L151xC
GenL1.menu.pnum.GENERIC_L151ZCTX.build.variant=STM32L1xx/L151ZCT_L152ZCT_L162ZCT
GenL1.menu.pnum.GENERIC_L151ZCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L1xx/STM32L151.svd

# Generic L152ZCTx
GenL1.menu.pnum.GENERIC_L152ZCTX=Generic L152ZCTx
GenL1.menu.pnum.GENERIC_L152ZCTX.upload.maximum_size=262144
GenL1.menu.pnum.GENERIC_L152ZCTX.upload.maximum_data_size=32768
GenL1.menu.pnum.GENERIC_L152ZCTX.build.board=GENERIC_L152ZCTX
GenL1.menu.pnum.GENERIC_L152ZCTX.build.product_line=STM32L152xC
GenL1.menu.pnum.GENERIC_L152ZCTX.build.variant=STM32L1xx/L151ZCT_L152ZCT_L162ZCT
GenL1.menu.pnum.GENERIC_L152ZCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L1xx/STM32L152.svd

# Generic L162ZCTx
GenL1.menu.pnum.GENERIC_L162ZCTX=Generic L162ZCTx
GenL1.menu.pnum.GENERIC_L162ZCTX.upload.maximum_size=262144
GenL1.menu.pnum.GENERIC_L162ZCTX.upload.maximum_data_size=32768
GenL1.menu.pnum.GENERIC_L162ZCTX.build.board=GENERIC_L162ZCTX
GenL1.menu.pnum.GENERIC_L162ZCTX.build.product_line=STM32L162xC
GenL1.menu.pnum.GENERIC_L162ZCTX.build.variant=STM32L1xx/L151ZCT_L152ZCT_L162ZCT
GenL1.menu.pnum.GENERIC_L162ZCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L1xx/STM32L162.svd

