# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L4R5ZGYx
GenL4.menu.pnum.GENERIC_L4R5ZGYX=Generic L4R5ZGYx
GenL4.menu.pnum.GENERIC_L4R5ZGYX.upload.maximum_size=1048576
GenL4.menu.pnum.GENERIC_L4R5ZGYX.upload.maximum_data_size=655360
GenL4.menu.pnum.GENERIC_L4R5ZGYX.build.board=GENERIC_L4R5ZGYX
GenL4.menu.pnum.GENERIC_L4R5ZGYX.build.product_line=STM32L4R5xx
GenL4.menu.pnum.GENERIC_L4R5ZGYX.build.variant=STM32L4xx/L4R5Z(G-I)Y_L4R9Z(G-I)Y_L4S5ZIY_L4S9ZIY
GenL4.menu.pnum.GENERIC_L4R5ZGYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L4R5.svd

# Generic L4R5ZIYx
GenL4.menu.pnum.GENERIC_L4R5ZIYX=Generic L4R5ZIYx
GenL4.menu.pnum.GENERIC_L4R5ZIYX.upload.maximum_size=2097152
GenL4.menu.pnum.GENERIC_L4R5ZIYX.upload.maximum_data_size=655360
GenL4.menu.pnum.GENERIC_L4R5ZIYX.build.board=GENERIC_L4R5ZIYX
GenL4.menu.pnum.GENERIC_L4R5ZIYX.build.product_line=STM32L4R5xx
GenL4.menu.pnum.GENERIC_L4R5ZIYX.build.variant=STM32L4xx/L4R5Z(G-I)Y_L4R9Z(G-I)Y_L4S5ZIY_L4S9ZIY
GenL4.menu.pnum.GENERIC_L4R5ZIYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L4R5.svd

# Generic L4R9ZGYx
GenL4.menu.pnum.GENERIC_L4R9ZGYX=Generic L4R9ZGYx
GenL4.menu.pnum.GENERIC_L4R9ZGYX.upload.maximum_size=1048576
GenL4.menu.pnum.GENERIC_L4R9ZGYX.upload.maximum_data_size=655360
GenL4.menu.pnum.GENERIC_L4R9ZGYX.build.board=GENERIC_L4R9ZGYX
GenL4.menu.pnum.GENERIC_L4R9ZGYX.build.product_line=STM32L4R9xx
GenL4.menu.pnum.GENERIC_L4R9ZGYX.build.variant=STM32L4xx/L4R5Z(G-I)Y_L4R9Z(G-I)Y_L4S5ZIY_L4S9ZIY
GenL4.menu.pnum.GENERIC_L4R9ZGYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L4R9.svd

# Generic L4R9ZIYx
GenL4.menu.pnum.GENERIC_L4R9ZIYX=Generic L4R9ZIYx
GenL4.menu.pnum.GENERIC_L4R9ZIYX.upload.maximum_size=2097152
GenL4.menu.pnum.GENERIC_L4R9ZIYX.upload.maximum_data_size=655360
GenL4.menu.pnum.GENERIC_L4R9ZIYX.build.board=GENERIC_L4R9ZIYX
GenL4.menu.pnum.GENERIC_L4R9ZIYX.build.product_line=STM32L4R9xx
GenL4.menu.pnum.GENERIC_L4R9ZIYX.build.variant=STM32L4xx/L4R5Z(G-I)Y_L4R9Z(G-I)Y_L4S5ZIY_L4S9ZIY
GenL4.menu.pnum.GENERIC_L4R9ZIYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L4R9.svd

# Generic L4S5ZIYx
GenL4.menu.pnum.GENERIC_L4S5ZIYX=Generic L4S5ZIYx
GenL4.menu.pnum.GENERIC_L4S5ZIYX.upload.maximum_size=2097152
GenL4.menu.pnum.GENERIC_L4S5ZIYX.upload.maximum_data_size=655360
GenL4.menu.pnum.GENERIC_L4S5ZIYX.build.board=GENERIC_L4S5ZIYX
GenL4.menu.pnum.GENERIC_L4S5ZIYX.build.product_line=STM32L4S5xx
GenL4.menu.pnum.GENERIC_L4S5ZIYX.build.variant=STM32L4xx/L4R5Z(G-I)Y_L4R9Z(G-I)Y_L4S5ZIY_L4S9ZIY
GenL4.menu.pnum.GENERIC_L4S5ZIYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L4S5.svd

# Generic L4S9ZIYx
GenL4.menu.pnum.GENERIC_L4S9ZIYX=Generic L4S9ZIYx
GenL4.menu.pnum.GENERIC_L4S9ZIYX.upload.maximum_size=2097152
GenL4.menu.pnum.GENERIC_L4S9ZIYX.upload.maximum_data_size=655360
GenL4.menu.pnum.GENERIC_L4S9ZIYX.build.board=GENERIC_L4S9ZIYX
GenL4.menu.pnum.GENERIC_L4S9ZIYX.build.product_line=STM32L4S9xx
GenL4.menu.pnum.GENERIC_L4S9ZIYX.build.variant=STM32L4xx/L4R5Z(G-I)Y_L4R9Z(G-I)Y_L4S5ZIY_L4S9ZIY
GenL4.menu.pnum.GENERIC_L4S9ZIYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L4S9.svd

