# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic H562RGVx
GenH5.menu.pnum.GENERIC_H562RGVX=Generic H562RGVx
GenH5.menu.pnum.GENERIC_H562RGVX.upload.maximum_size=1048576
GenH5.menu.pnum.GENERIC_H562RGVX.upload.maximum_data_size=655360
GenH5.menu.pnum.GENERIC_H562RGVX.build.board=GENERIC_H562RGVX
GenH5.menu.pnum.GENERIC_H562RGVX.build.product_line=STM32H562xx
GenH5.menu.pnum.GENERIC_H562RGVX.build.variant=STM32H5xx/H562R(G-I)V
GenH5.menu.pnum.GENERIC_H562RGVX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32H5xx/STM32H562.svd

# Generic H562RIVx
GenH5.menu.pnum.GENERIC_H562RIVX=Generic H562RIVx
GenH5.menu.pnum.GENERIC_H562RIVX.upload.maximum_size=2097152
GenH5.menu.pnum.GENERIC_H562RIVX.upload.maximum_data_size=655360
GenH5.menu.pnum.GENERIC_H562RIVX.build.board=GENERIC_H562RIVX
GenH5.menu.pnum.GENERIC_H562RIVX.build.product_line=STM32H562xx
GenH5.menu.pnum.GENERIC_H562RIVX.build.variant=STM32H5xx/H562R(G-I)V
GenH5.menu.pnum.GENERIC_H562RIVX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32H5xx/STM32H562.svd

