# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic WB35CCUxA
GenWB.menu.pnum.GENERIC_WB35CCUXA=Generic WB35CCUxA
GenWB.menu.pnum.GENERIC_WB35CCUXA.upload.maximum_size=262144
GenWB.menu.pnum.GENERIC_WB35CCUXA.upload.maximum_data_size=98304
GenWB.menu.pnum.GENERIC_WB35CCUXA.build.board=GENERIC_WB35CCUXA
GenWB.menu.pnum.GENERIC_WB35CCUXA.build.product_line=STM32WB35xx
GenWB.menu.pnum.GENERIC_WB35CCUXA.build.variant=STM32WBxx/WB35C(C-E)UxA_WB55C(C-E-G)U
GenWB.menu.pnum.GENERIC_WB35CCUXA.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32WBxx/STM32WB35_CM4.svd

# Generic WB35CEUxA
GenWB.menu.pnum.GENERIC_WB35CEUXA=Generic WB35CEUxA
GenWB.menu.pnum.GENERIC_WB35CEUXA.upload.maximum_size=524288
GenWB.menu.pnum.GENERIC_WB35CEUXA.upload.maximum_data_size=98304
GenWB.menu.pnum.GENERIC_WB35CEUXA.build.board=GENERIC_WB35CEUXA
GenWB.menu.pnum.GENERIC_WB35CEUXA.build.product_line=STM32WB35xx
GenWB.menu.pnum.GENERIC_WB35CEUXA.build.variant=STM32WBxx/WB35C(C-E)UxA_WB55C(C-E-G)U
GenWB.menu.pnum.GENERIC_WB35CEUXA.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32WBxx/STM32WB35_CM4.svd

# Generic WB55CCUx
GenWB.menu.pnum.GENERIC_WB55CCUX=Generic WB55CCUx
GenWB.menu.pnum.GENERIC_WB55CCUX.upload.maximum_size=262144
GenWB.menu.pnum.GENERIC_WB55CCUX.upload.maximum_data_size=131072
GenWB.menu.pnum.GENERIC_WB55CCUX.build.board=GENERIC_WB55CCUX
GenWB.menu.pnum.GENERIC_WB55CCUX.build.product_line=STM32WB55xx
GenWB.menu.pnum.GENERIC_WB55CCUX.build.variant=STM32WBxx/WB35C(C-E)UxA_WB55C(C-E-G)U
GenWB.menu.pnum.GENERIC_WB55CCUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32WBxx/STM32WB55_CM4.svd

# Generic WB55CEUx
GenWB.menu.pnum.GENERIC_WB55CEUX=Generic WB55CEUx
GenWB.menu.pnum.GENERIC_WB55CEUX.upload.maximum_size=524288
GenWB.menu.pnum.GENERIC_WB55CEUX.upload.maximum_data_size=262144
GenWB.menu.pnum.GENERIC_WB55CEUX.build.board=GENERIC_WB55CEUX
GenWB.menu.pnum.GENERIC_WB55CEUX.build.product_line=STM32WB55xx
GenWB.menu.pnum.GENERIC_WB55CEUX.build.variant=STM32WBxx/WB35C(C-E)UxA_WB55C(C-E-G)U
GenWB.menu.pnum.GENERIC_WB55CEUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32WBxx/STM32WB55_CM4.svd

# Generic WB55CGUx
GenWB.menu.pnum.GENERIC_WB55CGUX=Generic WB55CGUx
GenWB.menu.pnum.GENERIC_WB55CGUX.upload.maximum_size=1048576
GenWB.menu.pnum.GENERIC_WB55CGUX.upload.maximum_data_size=262144
GenWB.menu.pnum.GENERIC_WB55CGUX.build.board=GENERIC_WB55CGUX
GenWB.menu.pnum.GENERIC_WB55CGUX.build.product_line=STM32WB55xx
GenWB.menu.pnum.GENERIC_WB55CGUX.build.variant=STM32WBxx/WB35C(C-E)UxA_WB55C(C-E-G)U
GenWB.menu.pnum.GENERIC_WB55CGUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32WBxx/STM32WB55_CM4.svd

