# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic H562IGKx
GenH5.menu.pnum.GENERIC_H562IGKX=Generic H562IGKx
GenH5.menu.pnum.GENERIC_H562IGKX.upload.maximum_size=1048576
GenH5.menu.pnum.GENERIC_H562IGKX.upload.maximum_data_size=655360
GenH5.menu.pnum.GENERIC_H562IGKX.build.board=GENERIC_H562IGKX
GenH5.menu.pnum.GENERIC_H562IGKX.build.product_line=STM32H562xx
GenH5.menu.pnum.GENERIC_H562IGKX.build.variant=STM32H5xx/H562I(G-I)(K-T)
GenH5.menu.pnum.GENERIC_H562IGKX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32H5xx/STM32H562.svd

# Generic H562IGTx
GenH5.menu.pnum.GENERIC_H562IGTX=Generic H562IGTx
GenH5.menu.pnum.GENERIC_H562IGTX.upload.maximum_size=1048576
GenH5.menu.pnum.GENERIC_H562IGTX.upload.maximum_data_size=655360
GenH5.menu.pnum.GENERIC_H562IGTX.build.board=GENERIC_H562IGTX
GenH5.menu.pnum.GENERIC_H562IGTX.build.product_line=STM32H562xx
GenH5.menu.pnum.GENERIC_H562IGTX.build.variant=STM32H5xx/H562I(G-I)(K-T)
GenH5.menu.pnum.GENERIC_H562IGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32H5xx/STM32H562.svd

# Generic H562IIKx
GenH5.menu.pnum.GENERIC_H562IIKX=Generic H562IIKx
GenH5.menu.pnum.GENERIC_H562IIKX.upload.maximum_size=2097152
GenH5.menu.pnum.GENERIC_H562IIKX.upload.maximum_data_size=655360
GenH5.menu.pnum.GENERIC_H562IIKX.build.board=GENERIC_H562IIKX
GenH5.menu.pnum.GENERIC_H562IIKX.build.product_line=STM32H562xx
GenH5.menu.pnum.GENERIC_H562IIKX.build.variant=STM32H5xx/H562I(G-I)(K-T)
GenH5.menu.pnum.GENERIC_H562IIKX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32H5xx/STM32H562.svd

# Generic H562IITx
GenH5.menu.pnum.GENERIC_H562IITX=Generic H562IITx
GenH5.menu.pnum.GENERIC_H562IITX.upload.maximum_size=2097152
GenH5.menu.pnum.GENERIC_H562IITX.upload.maximum_data_size=655360
GenH5.menu.pnum.GENERIC_H562IITX.build.board=GENERIC_H562IITX
GenH5.menu.pnum.GENERIC_H562IITX.build.product_line=STM32H562xx
GenH5.menu.pnum.GENERIC_H562IITX.build.variant=STM32H5xx/H562I(G-I)(K-T)
GenH5.menu.pnum.GENERIC_H562IITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32H5xx/STM32H562.svd

