# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic U575OGYxQ
GenU5.menu.pnum.GENERIC_U575OGYXQ=Generic U575OGYxQ
GenU5.menu.pnum.GENERIC_U575OGYXQ.upload.maximum_size=1048576
GenU5.menu.pnum.GENERIC_U575OGYXQ.upload.maximum_data_size=804864
GenU5.menu.pnum.GENERIC_U575OGYXQ.build.board=GENERIC_U575OGYXQ
GenU5.menu.pnum.GENERIC_U575OGYXQ.build.product_line=STM32U575xx
GenU5.menu.pnum.GENERIC_U575OGYXQ.build.variant=STM32U5xx/U575O(G-I)YxQ_U585OIYxQ
GenU5.menu.pnum.GENERIC_U575OGYXQ.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U575.svd

# Generic U575OIYxQ
GenU5.menu.pnum.GENERIC_U575OIYXQ=Generic U575OIYxQ
GenU5.menu.pnum.GENERIC_U575OIYXQ.upload.maximum_size=2097152
GenU5.menu.pnum.GENERIC_U575OIYXQ.upload.maximum_data_size=804864
GenU5.menu.pnum.GENERIC_U575OIYXQ.build.board=GENERIC_U575OIYXQ
GenU5.menu.pnum.GENERIC_U575OIYXQ.build.product_line=STM32U575xx
GenU5.menu.pnum.GENERIC_U575OIYXQ.build.variant=STM32U5xx/U575O(G-I)YxQ_U585OIYxQ
GenU5.menu.pnum.GENERIC_U575OIYXQ.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U575.svd

# Generic U585OIYxQ
GenU5.menu.pnum.GENERIC_U585OIYXQ=Generic U585OIYxQ
GenU5.menu.pnum.GENERIC_U585OIYXQ.upload.maximum_size=2097152
GenU5.menu.pnum.GENERIC_U585OIYXQ.upload.maximum_data_size=804864
GenU5.menu.pnum.GENERIC_U585OIYXQ.build.board=GENERIC_U585OIYXQ
GenU5.menu.pnum.GENERIC_U585OIYXQ.build.product_line=STM32U585xx
GenU5.menu.pnum.GENERIC_U585OIYXQ.build.variant=STM32U5xx/U575O(G-I)YxQ_U585OIYxQ
GenU5.menu.pnum.GENERIC_U585OIYXQ.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U585.svd

