# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F302RDTx
GenF3.menu.pnum.GENERIC_F302RDTX=Generic F302RDTx
GenF3.menu.pnum.GENERIC_F302RDTX.upload.maximum_size=393216
GenF3.menu.pnum.GENERIC_F302RDTX.upload.maximum_data_size=65536
GenF3.menu.pnum.GENERIC_F302RDTX.build.board=GENERIC_F302RDTX
GenF3.menu.pnum.GENERIC_F302RDTX.build.product_line=STM32F302xE
GenF3.menu.pnum.GENERIC_F302RDTX.build.variant=STM32F3xx/F302R(D-E)T
GenF3.menu.pnum.GENERIC_F302RDTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F302.svd

# Generic F302RETx
GenF3.menu.pnum.GENERIC_F302RETX=Generic F302RETx
GenF3.menu.pnum.GENERIC_F302RETX.upload.maximum_size=524288
GenF3.menu.pnum.GENERIC_F302RETX.upload.maximum_data_size=65536
GenF3.menu.pnum.GENERIC_F302RETX.build.board=GENERIC_F302RETX
GenF3.menu.pnum.GENERIC_F302RETX.build.product_line=STM32F302xE
GenF3.menu.pnum.GENERIC_F302RETX.build.variant=STM32F3xx/F302R(D-E)T
GenF3.menu.pnum.GENERIC_F302RETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F302.svd

