# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L151RCTx
GenL1.menu.pnum.GENERIC_L151RCTX=Generic L151RCTx
GenL1.menu.pnum.GENERIC_L151RCTX.upload.maximum_size=262144
GenL1.menu.pnum.GENERIC_L151RCTX.upload.maximum_data_size=32768
GenL1.menu.pnum.GENERIC_L151RCTX.build.board=GENERIC_L151RCTX
GenL1.menu.pnum.GENERIC_L151RCTX.build.product_line=STM32L151xC
GenL1.menu.pnum.GENERIC_L151RCTX.build.variant=STM32L1xx/L151RC(T-Y)x(A)_L151UCY_L152RCTx(A)_L152UCY_L162RCTx(A)
GenL1.menu.pnum.GENERIC_L151RCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L1xx/STM32L151.svd

# Generic L151RCTxA
GenL1.menu.pnum.GENERIC_L151RCTXA=Generic L151RCTxA
GenL1.menu.pnum.GENERIC_L151RCTXA.upload.maximum_size=262144
GenL1.menu.pnum.GENERIC_L151RCTXA.upload.maximum_data_size=32768
GenL1.menu.pnum.GENERIC_L151RCTXA.build.board=GENERIC_L151RCTXA
GenL1.menu.pnum.GENERIC_L151RCTXA.build.product_line=STM32L151xCA
GenL1.menu.pnum.GENERIC_L151RCTXA.build.variant=STM32L1xx/L151RC(T-Y)x(A)_L151UCY_L152RCTx(A)_L152UCY_L162RCTx(A)
GenL1.menu.pnum.GENERIC_L151RCTXA.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L1xx/STM32L151.svd

# Generic L151RCYx
GenL1.menu.pnum.GENERIC_L151RCYX=Generic L151RCYx
GenL1.menu.pnum.GENERIC_L151RCYX.upload.maximum_size=262144
GenL1.menu.pnum.GENERIC_L151RCYX.upload.maximum_data_size=32768
GenL1.menu.pnum.GENERIC_L151RCYX.build.board=GENERIC_L151RCYX
GenL1.menu.pnum.GENERIC_L151RCYX.build.product_line=STM32L151xC
GenL1.menu.pnum.GENERIC_L151RCYX.build.variant=STM32L1xx/L151RC(T-Y)x(A)_L151UCY_L152RCTx(A)_L152UCY_L162RCTx(A)
GenL1.menu.pnum.GENERIC_L151RCYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L1xx/STM32L151.svd

# Generic L151UCYx
GenL1.menu.pnum.GENERIC_L151UCYX=Generic L151UCYx
GenL1.menu.pnum.GENERIC_L151UCYX.upload.maximum_size=262144
GenL1.menu.pnum.GENERIC_L151UCYX.upload.maximum_data_size=32768
GenL1.menu.pnum.GENERIC_L151UCYX.build.board=GENERIC_L151UCYX
GenL1.menu.pnum.GENERIC_L151UCYX.build.product_line=STM32L151xC
GenL1.menu.pnum.GENERIC_L151UCYX.build.variant=STM32L1xx/L151RC(T-Y)x(A)_L151UCY_L152RCTx(A)_L152UCY_L162RCTx(A)
GenL1.menu.pnum.GENERIC_L151UCYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L1xx/STM32L151.svd

# Generic L152RCTx
GenL1.menu.pnum.GENERIC_L152RCTX=Generic L152RCTx
GenL1.menu.pnum.GENERIC_L152RCTX.upload.maximum_size=262144
GenL1.menu.pnum.GENERIC_L152RCTX.upload.maximum_data_size=32768
GenL1.menu.pnum.GENERIC_L152RCTX.build.board=GENERIC_L152RCTX
GenL1.menu.pnum.GENERIC_L152RCTX.build.product_line=STM32L152xC
GenL1.menu.pnum.GENERIC_L152RCTX.build.variant=STM32L1xx/L151RC(T-Y)x(A)_L151UCY_L152RCTx(A)_L152UCY_L162RCTx(A)
GenL1.menu.pnum.GENERIC_L152RCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L1xx/STM32L152.svd

# Generic L152RCTxA
GenL1.menu.pnum.GENERIC_L152RCTXA=Generic L152RCTxA
GenL1.menu.pnum.GENERIC_L152RCTXA.upload.maximum_size=262144
GenL1.menu.pnum.GENERIC_L152RCTXA.upload.maximum_data_size=32768
GenL1.menu.pnum.GENERIC_L152RCTXA.build.board=GENERIC_L152RCTXA
GenL1.menu.pnum.GENERIC_L152RCTXA.build.product_line=STM32L152xCA
GenL1.menu.pnum.GENERIC_L152RCTXA.build.variant=STM32L1xx/L151RC(T-Y)x(A)_L151UCY_L152RCTx(A)_L152UCY_L162RCTx(A)
GenL1.menu.pnum.GENERIC_L152RCTXA.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L1xx/STM32L152.svd

# Generic L152UCYx
GenL1.menu.pnum.GENERIC_L152UCYX=Generic L152UCYx
GenL1.menu.pnum.GENERIC_L152UCYX.upload.maximum_size=262144
GenL1.menu.pnum.GENERIC_L152UCYX.upload.maximum_data_size=32768
GenL1.menu.pnum.GENERIC_L152UCYX.build.board=GENERIC_L152UCYX
GenL1.menu.pnum.GENERIC_L152UCYX.build.product_line=STM32L152xC
GenL1.menu.pnum.GENERIC_L152UCYX.build.variant=STM32L1xx/L151RC(T-Y)x(A)_L151UCY_L152RCTx(A)_L152UCY_L162RCTx(A)
GenL1.menu.pnum.GENERIC_L152UCYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L1xx/STM32L152.svd

# Generic L162RCTx
GenL1.menu.pnum.GENERIC_L162RCTX=Generic L162RCTx
GenL1.menu.pnum.GENERIC_L162RCTX.upload.maximum_size=262144
GenL1.menu.pnum.GENERIC_L162RCTX.upload.maximum_data_size=32768
GenL1.menu.pnum.GENERIC_L162RCTX.build.board=GENERIC_L162RCTX
GenL1.menu.pnum.GENERIC_L162RCTX.build.product_line=STM32L162xC
GenL1.menu.pnum.GENERIC_L162RCTX.build.variant=STM32L1xx/L151RC(T-Y)x(A)_L151UCY_L152RCTx(A)_L152UCY_L162RCTx(A)
GenL1.menu.pnum.GENERIC_L162RCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L1xx/STM32L162.svd

# Generic L162RCTxA
GenL1.menu.pnum.GENERIC_L162RCTXA=Generic L162RCTxA
GenL1.menu.pnum.GENERIC_L162RCTXA.upload.maximum_size=262144
GenL1.menu.pnum.GENERIC_L162RCTXA.upload.maximum_data_size=32768
GenL1.menu.pnum.GENERIC_L162RCTXA.build.board=GENERIC_L162RCTXA
GenL1.menu.pnum.GENERIC_L162RCTXA.build.product_line=STM32L162xCA
GenL1.menu.pnum.GENERIC_L162RCTXA.build.variant=STM32L1xx/L151RC(T-Y)x(A)_L151UCY_L152RCTx(A)_L152UCY_L162RCTx(A)
GenL1.menu.pnum.GENERIC_L162RCTXA.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L1xx/STM32L162.svd

