# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L4R5ZGTx
GenL4.menu.pnum.GENERIC_L4R5ZGTX=Generic L4R5ZGTx
GenL4.menu.pnum.GENERIC_L4R5ZGTX.upload.maximum_size=1048576
GenL4.menu.pnum.GENERIC_L4R5ZGTX.upload.maximum_data_size=655360
GenL4.menu.pnum.GENERIC_L4R5ZGTX.build.board=GENERIC_L4R5ZGTX
GenL4.menu.pnum.GENERIC_L4R5ZGTX.build.product_line=STM32L4R5xx
GenL4.menu.pnum.GENERIC_L4R5ZGTX.build.variant=STM32L4xx/L4R5Z(G-I)T_L4R7ZIT_L4S5ZIT_L4S7ZIT
GenL4.menu.pnum.GENERIC_L4R5ZGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L4R5.svd

# Generic L4R5ZITx
GenL4.menu.pnum.GENERIC_L4R5ZITX=Generic L4R5ZITx
GenL4.menu.pnum.GENERIC_L4R5ZITX.upload.maximum_size=2097152
GenL4.menu.pnum.GENERIC_L4R5ZITX.upload.maximum_data_size=655360
GenL4.menu.pnum.GENERIC_L4R5ZITX.build.board=GENERIC_L4R5ZITX
GenL4.menu.pnum.GENERIC_L4R5ZITX.build.product_line=STM32L4R5xx
GenL4.menu.pnum.GENERIC_L4R5ZITX.build.variant=STM32L4xx/L4R5Z(G-I)T_L4R7ZIT_L4S5ZIT_L4S7ZIT
GenL4.menu.pnum.GENERIC_L4R5ZITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L4R5.svd

# Generic L4R7ZITx
GenL4.menu.pnum.GENERIC_L4R7ZITX=Generic L4R7ZITx
GenL4.menu.pnum.GENERIC_L4R7ZITX.upload.maximum_size=2097152
GenL4.menu.pnum.GENERIC_L4R7ZITX.upload.maximum_data_size=655360
GenL4.menu.pnum.GENERIC_L4R7ZITX.build.board=GENERIC_L4R7ZITX
GenL4.menu.pnum.GENERIC_L4R7ZITX.build.product_line=STM32L4R7xx
GenL4.menu.pnum.GENERIC_L4R7ZITX.build.variant=STM32L4xx/L4R5Z(G-I)T_L4R7ZIT_L4S5ZIT_L4S7ZIT
GenL4.menu.pnum.GENERIC_L4R7ZITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L4R7.svd

# Generic L4S5ZITx
GenL4.menu.pnum.GENERIC_L4S5ZITX=Generic L4S5ZITx
GenL4.menu.pnum.GENERIC_L4S5ZITX.upload.maximum_size=2097152
GenL4.menu.pnum.GENERIC_L4S5ZITX.upload.maximum_data_size=655360
GenL4.menu.pnum.GENERIC_L4S5ZITX.build.board=GENERIC_L4S5ZITX
GenL4.menu.pnum.GENERIC_L4S5ZITX.build.product_line=STM32L4S5xx
GenL4.menu.pnum.GENERIC_L4S5ZITX.build.variant=STM32L4xx/L4R5Z(G-I)T_L4R7ZIT_L4S5ZIT_L4S7ZIT
GenL4.menu.pnum.GENERIC_L4S5ZITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L4S5.svd

# Generic L4S7ZITx
GenL4.menu.pnum.GENERIC_L4S7ZITX=Generic L4S7ZITx
GenL4.menu.pnum.GENERIC_L4S7ZITX.upload.maximum_size=2097152
GenL4.menu.pnum.GENERIC_L4S7ZITX.upload.maximum_data_size=655360
GenL4.menu.pnum.GENERIC_L4S7ZITX.build.board=GENERIC_L4S7ZITX
GenL4.menu.pnum.GENERIC_L4S7ZITX.build.product_line=STM32L4S7xx
GenL4.menu.pnum.GENERIC_L4S7ZITX.build.variant=STM32L4xx/L4R5Z(G-I)T_L4R7ZIT_L4S5ZIT_L4S7ZIT
GenL4.menu.pnum.GENERIC_L4S7ZITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L4S7.svd

