# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic G071C6Tx
GenG0.menu.pnum.GENERIC_G071C6TX=Generic G071C6Tx
GenG0.menu.pnum.GENERIC_G071C6TX.upload.maximum_size=32768
GenG0.menu.pnum.GENERIC_G071C6TX.upload.maximum_data_size=36864
GenG0.menu.pnum.GENERIC_G071C6TX.build.board=GENERIC_G071C6TX
GenG0.menu.pnum.GENERIC_G071C6TX.build.product_line=STM32G071xx
GenG0.menu.pnum.GENERIC_G071C6TX.build.variant=STM32G0xx/G071C(6-8-B)(T-U)_G081CB(T-U)
GenG0.menu.pnum.GENERIC_G071C6TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G071.svd

# Generic G071C8Tx
GenG0.menu.pnum.GENERIC_G071C8TX=Generic G071C8Tx
GenG0.menu.pnum.GENERIC_G071C8TX.upload.maximum_size=65536
GenG0.menu.pnum.GENERIC_G071C8TX.upload.maximum_data_size=36864
GenG0.menu.pnum.GENERIC_G071C8TX.build.board=GENERIC_G071C8TX
GenG0.menu.pnum.GENERIC_G071C8TX.build.product_line=STM32G071xx
GenG0.menu.pnum.GENERIC_G071C8TX.build.variant=STM32G0xx/G071C(6-8-B)(T-U)_G081CB(T-U)
GenG0.menu.pnum.GENERIC_G071C8TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G071.svd

# Generic G071CBTx
GenG0.menu.pnum.GENERIC_G071CBTX=Generic G071CBTx
GenG0.menu.pnum.GENERIC_G071CBTX.upload.maximum_size=131072
GenG0.menu.pnum.GENERIC_G071CBTX.upload.maximum_data_size=36864
GenG0.menu.pnum.GENERIC_G071CBTX.build.board=GENERIC_G071CBTX
GenG0.menu.pnum.GENERIC_G071CBTX.build.product_line=STM32G071xx
GenG0.menu.pnum.GENERIC_G071CBTX.build.variant=STM32G0xx/G071C(6-8-B)(T-U)_G081CB(T-U)
GenG0.menu.pnum.GENERIC_G071CBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G071.svd

# Generic G071C6Ux
GenG0.menu.pnum.GENERIC_G071C6UX=Generic G071C6Ux
GenG0.menu.pnum.GENERIC_G071C6UX.upload.maximum_size=32768
GenG0.menu.pnum.GENERIC_G071C6UX.upload.maximum_data_size=36864
GenG0.menu.pnum.GENERIC_G071C6UX.build.board=GENERIC_G071C6UX
GenG0.menu.pnum.GENERIC_G071C6UX.build.product_line=STM32G071xx
GenG0.menu.pnum.GENERIC_G071C6UX.build.variant=STM32G0xx/G071C(6-8-B)(T-U)_G081CB(T-U)
GenG0.menu.pnum.GENERIC_G071C6UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G071.svd

# Generic G071C8Ux
GenG0.menu.pnum.GENERIC_G071C8UX=Generic G071C8Ux
GenG0.menu.pnum.GENERIC_G071C8UX.upload.maximum_size=65536
GenG0.menu.pnum.GENERIC_G071C8UX.upload.maximum_data_size=36864
GenG0.menu.pnum.GENERIC_G071C8UX.build.board=GENERIC_G071C8UX
GenG0.menu.pnum.GENERIC_G071C8UX.build.product_line=STM32G071xx
GenG0.menu.pnum.GENERIC_G071C8UX.build.variant=STM32G0xx/G071C(6-8-B)(T-U)_G081CB(T-U)
GenG0.menu.pnum.GENERIC_G071C8UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G071.svd

# Generic G071CBUx
GenG0.menu.pnum.GENERIC_G071CBUX=Generic G071CBUx
GenG0.menu.pnum.GENERIC_G071CBUX.upload.maximum_size=131072
GenG0.menu.pnum.GENERIC_G071CBUX.upload.maximum_data_size=36864
GenG0.menu.pnum.GENERIC_G071CBUX.build.board=GENERIC_G071CBUX
GenG0.menu.pnum.GENERIC_G071CBUX.build.product_line=STM32G071xx
GenG0.menu.pnum.GENERIC_G071CBUX.build.variant=STM32G0xx/G071C(6-8-B)(T-U)_G081CB(T-U)
GenG0.menu.pnum.GENERIC_G071CBUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G071.svd

# Generic G081CBTx
GenG0.menu.pnum.GENERIC_G081CBTX=Generic G081CBTx
GenG0.menu.pnum.GENERIC_G081CBTX.upload.maximum_size=131072
GenG0.menu.pnum.GENERIC_G081CBTX.upload.maximum_data_size=36864
GenG0.menu.pnum.GENERIC_G081CBTX.build.board=GENERIC_G081CBTX
GenG0.menu.pnum.GENERIC_G081CBTX.build.product_line=STM32G081xx
GenG0.menu.pnum.GENERIC_G081CBTX.build.variant=STM32G0xx/G071C(6-8-B)(T-U)_G081CB(T-U)
GenG0.menu.pnum.GENERIC_G081CBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G081.svd

# Generic G081CBUx
GenG0.menu.pnum.GENERIC_G081CBUX=Generic G081CBUx
GenG0.menu.pnum.GENERIC_G081CBUX.upload.maximum_size=131072
GenG0.menu.pnum.GENERIC_G081CBUX.upload.maximum_data_size=36864
GenG0.menu.pnum.GENERIC_G081CBUX.build.board=GENERIC_G081CBUX
GenG0.menu.pnum.GENERIC_G081CBUX.build.product_line=STM32G081xx
GenG0.menu.pnum.GENERIC_G081CBUX.build.variant=STM32G0xx/G071C(6-8-B)(T-U)_G081CB(T-U)
GenG0.menu.pnum.GENERIC_G081CBUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G081.svd

