# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L031E4Yx
GenL0.menu.pnum.GENERIC_L031E4YX=Generic L031E4Yx
GenL0.menu.pnum.GENERIC_L031E4YX.upload.maximum_size=16384
GenL0.menu.pnum.GENERIC_L031E4YX.upload.maximum_data_size=8192
GenL0.menu.pnum.GENERIC_L031E4YX.build.board=GENERIC_L031E4YX
GenL0.menu.pnum.GENERIC_L031E4YX.build.product_line=STM32L031xx
GenL0.menu.pnum.GENERIC_L031E4YX.build.variant=STM32L0xx/L031E(4-6)Y_L041E6Y
GenL0.menu.pnum.GENERIC_L031E4YX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

# Generic L031E6Yx
GenL0.menu.pnum.GENERIC_L031E6YX=Generic L031E6Yx
GenL0.menu.pnum.GENERIC_L031E6YX.upload.maximum_size=32768
GenL0.menu.pnum.GENERIC_L031E6YX.upload.maximum_data_size=8192
GenL0.menu.pnum.GENERIC_L031E6YX.build.board=GENERIC_L031E6YX
GenL0.menu.pnum.GENERIC_L031E6YX.build.product_line=STM32L031xx
GenL0.menu.pnum.GENERIC_L031E6YX.build.variant=STM32L0xx/L031E(4-6)Y_L041E6Y
GenL0.menu.pnum.GENERIC_L031E6YX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

# Generic L041E6Yx
GenL0.menu.pnum.GENERIC_L041E6YX=Generic L041E6Yx
GenL0.menu.pnum.GENERIC_L041E6YX.upload.maximum_size=32768
GenL0.menu.pnum.GENERIC_L041E6YX.upload.maximum_data_size=8192
GenL0.menu.pnum.GENERIC_L041E6YX.build.board=GENERIC_L041E6YX
GenL0.menu.pnum.GENERIC_L041E6YX.build.product_line=STM32L041xx
GenL0.menu.pnum.GENERIC_L041E6YX.build.variant=STM32L0xx/L031E(4-6)Y_L041E6Y
GenL0.menu.pnum.GENERIC_L041E6YX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

