# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F723ZCIx
GenF7.menu.pnum.GENERIC_F723ZCIX=Generic F723ZCIx
GenF7.menu.pnum.GENERIC_F723ZCIX.upload.maximum_size=262144
GenF7.menu.pnum.GENERIC_F723ZCIX.upload.maximum_data_size=196608
GenF7.menu.pnum.GENERIC_F723ZCIX.build.board=GENERIC_F723ZCIX
GenF7.menu.pnum.GENERIC_F723ZCIX.build.product_line=STM32F723xx
GenF7.menu.pnum.GENERIC_F723ZCIX.build.variant=STM32F7xx/F723Z(C-E)(I-T)_F730Z8T_F733ZE(I-T)
GenF7.menu.pnum.GENERIC_F723ZCIX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F723.svd

# Generic F723ZEIx
GenF7.menu.pnum.GENERIC_F723ZEIX=Generic F723ZEIx
GenF7.menu.pnum.GENERIC_F723ZEIX.upload.maximum_size=524288
GenF7.menu.pnum.GENERIC_F723ZEIX.upload.maximum_data_size=196608
GenF7.menu.pnum.GENERIC_F723ZEIX.build.board=GENERIC_F723ZEIX
GenF7.menu.pnum.GENERIC_F723ZEIX.build.product_line=STM32F723xx
GenF7.menu.pnum.GENERIC_F723ZEIX.build.variant=STM32F7xx/F723Z(C-E)(I-T)_F730Z8T_F733ZE(I-T)
GenF7.menu.pnum.GENERIC_F723ZEIX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F723.svd

# Generic F723ZCTx
GenF7.menu.pnum.GENERIC_F723ZCTX=Generic F723ZCTx
GenF7.menu.pnum.GENERIC_F723ZCTX.upload.maximum_size=262144
GenF7.menu.pnum.GENERIC_F723ZCTX.upload.maximum_data_size=196608
GenF7.menu.pnum.GENERIC_F723ZCTX.build.board=GENERIC_F723ZCTX
GenF7.menu.pnum.GENERIC_F723ZCTX.build.product_line=STM32F723xx
GenF7.menu.pnum.GENERIC_F723ZCTX.build.variant=STM32F7xx/F723Z(C-E)(I-T)_F730Z8T_F733ZE(I-T)
GenF7.menu.pnum.GENERIC_F723ZCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F723.svd

# Generic F723ZETx
GenF7.menu.pnum.GENERIC_F723ZETX=Generic F723ZETx
GenF7.menu.pnum.GENERIC_F723ZETX.upload.maximum_size=524288
GenF7.menu.pnum.GENERIC_F723ZETX.upload.maximum_data_size=196608
GenF7.menu.pnum.GENERIC_F723ZETX.build.board=GENERIC_F723ZETX
GenF7.menu.pnum.GENERIC_F723ZETX.build.product_line=STM32F723xx
GenF7.menu.pnum.GENERIC_F723ZETX.build.variant=STM32F7xx/F723Z(C-E)(I-T)_F730Z8T_F733ZE(I-T)
GenF7.menu.pnum.GENERIC_F723ZETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F723.svd

# Generic F730Z8Tx
GenF7.menu.pnum.GENERIC_F730Z8TX=Generic F730Z8Tx
GenF7.menu.pnum.GENERIC_F730Z8TX.upload.maximum_size=65536
GenF7.menu.pnum.GENERIC_F730Z8TX.upload.maximum_data_size=196608
GenF7.menu.pnum.GENERIC_F730Z8TX.build.board=GENERIC_F730Z8TX
GenF7.menu.pnum.GENERIC_F730Z8TX.build.product_line=STM32F730xx
GenF7.menu.pnum.GENERIC_F730Z8TX.build.variant=STM32F7xx/F723Z(C-E)(I-T)_F730Z8T_F733ZE(I-T)
GenF7.menu.pnum.GENERIC_F730Z8TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F730.svd

# Generic F733ZEIx
GenF7.menu.pnum.GENERIC_F733ZEIX=Generic F733ZEIx
GenF7.menu.pnum.GENERIC_F733ZEIX.upload.maximum_size=524288
GenF7.menu.pnum.GENERIC_F733ZEIX.upload.maximum_data_size=196608
GenF7.menu.pnum.GENERIC_F733ZEIX.build.board=GENERIC_F733ZEIX
GenF7.menu.pnum.GENERIC_F733ZEIX.build.product_line=STM32F733xx
GenF7.menu.pnum.GENERIC_F733ZEIX.build.variant=STM32F7xx/F723Z(C-E)(I-T)_F730Z8T_F733ZE(I-T)
GenF7.menu.pnum.GENERIC_F733ZEIX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F733.svd

# Generic F733ZETx
GenF7.menu.pnum.GENERIC_F733ZETX=Generic F733ZETx
GenF7.menu.pnum.GENERIC_F733ZETX.upload.maximum_size=524288
GenF7.menu.pnum.GENERIC_F733ZETX.upload.maximum_data_size=196608
GenF7.menu.pnum.GENERIC_F733ZETX.build.board=GENERIC_F733ZETX
GenF7.menu.pnum.GENERIC_F733ZETX.build.product_line=STM32F733xx
GenF7.menu.pnum.GENERIC_F733ZETX.build.variant=STM32F7xx/F723Z(C-E)(I-T)_F730Z8T_F733ZE(I-T)
GenF7.menu.pnum.GENERIC_F733ZETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F733.svd

